Router 1
Router>enable
Router#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#hostname R1
R1(config)#no ip domain-lookup
R1(config)#line console 0
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#logging synchronous
R1(config-line)#line aux 0
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#
R1#
R1#enable secret class
          ^
% Invalid input detected at '^' marker.
	
R1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#enable secret class
R1(config)#banner motd <Authorized Access Only>
Enter TEXT message.  End with the character '<'.

<Authorized access only>

R1(config)#interface gigabitethernet 0/0
R1(config-if)#ip address 200.100.1.1 255.255.255.0
R1(config-if)#no shutdown       
R1#
R1#configure terminal
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#interface Serial0/3/0
R1(config-if)#ip address 200.100.12.10 255.255.255.252
R1(config-if)#clock rate 128000
R1(config-if)#no shutdown

%LINK-5-CHANGED: Interface Serial0/3/0, changed state to down
R1(config-if)#
R1(config)#interface Serial 0/3/1
R1(config-if)#ip address 200.100.13.1 255.255.255.252
R1(config-if)#no shutdown

%LINK-5-CHANGED: Interface Serial0/3/1, changed state to down
R1(config-if)#end
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#
R1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#interface g0/0
R1(config-if)#ip address 200.100.1.1 255.255.255.0
R1(config-if)#description "Connected to R2_Primary Link"
R1(config-if)#no shutdown
R1(config-if)#exit
R1(config)#
R1(config)#router  ospf 1
R1(config-router)#network 200.100.1.1 0.0.0.255 area 0
R1(config-router)#network 200.100.12.1 0.0.0.3 area 0
R1(config-router)#network 200.100.13.1 0.0.0.3 area 0
R1(config-router)#end
R1#show ip ospf interface

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.1.1/24, Area 0
  Process ID 1, Router ID 200.100.13.1, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State DR, Priority 1
  Designated Router (ID) 200.100.13.1, Interface address 200.100.1.1
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:00
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
R1#
R1#show ip ospf neighbor

R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     200.100.1.0/24 is variably subnetted, 2 subnets, 2 masks
C       200.100.1.0/24 is directly connected, GigabitEthernet0/0
L       200.100.1.1/32 is directly connected, GigabitEthernet0/0

R1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#interface lo 0

R1(config-if)#
%LINK-5-CHANGED: Interface Loopback0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface Loopback0, changed state to up
R1(config-if)#ip add 1.1.1.1 255.255.255.255
R1(config-if)#no shutdown
R1(config-if)#end
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1(config)#router ospf 1
R1(config-router)#passive-interface g0/0
R1(config-router)#end
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#show ip ospf interface g0/0

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.1.1/24, Area 0
  Process ID 1, Router ID 200.100.13.1, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State WAITING, Priority 1
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    No Hellos (Passive interface)
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
R1#
R1#config
Configuring from terminal, memory, or network [terminal]? 
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#interface serial0/3/0
R1(config-if)#bandwidth 128
R1(config-if)#end
R1#
%SYS-5-CONFIG_I: Configured from console by console
R1#show ip route ospf
R1#show ip ospf interface brief
                          ^
% Invalid input detected at '^' marker.
	
R1#show ip ospf interface

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.1.1/24, Area 0
  Process ID 1, Router ID 200.100.13.1, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State WAITING, Priority 1
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    No Hellos (Passive interface)
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
R1#
R1>enable
Password: 
R1#config
Configuring from terminal, memory, or network [terminal]? 
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#interface serial 0/3/0
R1(config-if)#bandwidth 1000
R1(config-if)#end
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#
R1>show ip ospf database
            OSPF Router with ID (200.100.13.1) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
200.100.13.1    200.100.13.1    569         0x80000004 0x00262f 3
200.100.23.1    200.100.23.1    546         0x80000005 0x002f51 4
200.100.23.2    200.100.23.2    379         0x80000006 0x005041 5
R1>
R1>show ip ospf database
            OSPF Router with ID (200.100.13.1) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
200.100.13.1    200.100.13.1    569         0x80000004 0x00262f 3
200.100.23.1    200.100.23.1    546         0x80000005 0x002f51 4
200.100.23.2    200.100.23.2    379         0x80000006 0x005041 5
R1>show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     1.0.0.0/32 is subnetted, 1 subnets
C       1.1.1.1/32 is directly connected, Loopback0
     200.100.1.0/24 is variably subnetted, 2 subnets, 2 masks
C       200.100.1.0/24 is directly connected, GigabitEthernet0/0
L       200.100.1.1/32 is directly connected, GigabitEthernet0/0
O    200.100.2.0/24 [110/129] via 200.100.13.2, 00:09:49, Serial0/3/1
O    200.100.3.0/24 [110/65] via 200.100.13.2, 00:10:23, Serial0/3/1
     200.100.12.0/24 is variably subnetted, 3 subnets, 2 masks
O       200.100.12.0/30 [110/228] via 200.100.13.2, 00:09:49, Serial0/3/1
C       200.100.12.8/30 is directly connected, Serial0/3/0
L       200.100.12.10/32 is directly connected, Serial0/3/0
     200.100.13.0/24 is variably subnetted, 2 subnets, 2 masks
C       200.100.13.0/30 is directly connected, Serial0/3/1
L       200.100.13.1/32 is directly connected, Serial0/3/1
     200.100.23.0/30 is subnetted, 1 subnets
[bookmark: _GoBack]O       200.100.23.0/30 [110/128] via 200.100.13.2, 00:09:59, Serial0/3/1

Router2
Router>enable
Router#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#hostname R2
R2(config)#no ip domain-lookup
R2(config)#line console 0
R2(config-line)#password cisco
R2(config-line)#login
R2(config-line)#logging synchornous
                             ^
% Invalid input detected at '^' marker.
	
R2(config-line)#logging synchronous
R2(config-line)#line aux 0
R2(config-line)#
R2(config-line)#password cisco
R2(config-line)#login
R2(config-line)#line vty 0 4
R2(config-line)#login 
% Login disabled on line 388, until 'password' is set
% Login disabled on line 389, until 'password' is set
% Login disabled on line 390, until 'password' is set
% Login disabled on line 391, until 'password' is set
% Login disabled on line 392, until 'password' is set
R2(config-line)#exit
R2(config)#enable secret class
R2(config)#banner motd
% Incomplete command.
R2(config)#banner motd <Authorized Access Only>
Enter TEXT message.  End with the character '<'.
Authorized accesss only

exit
<Authorized access only>

R2(config)#interface gigabitethernet 0/0
R2(config-if)#ip address 200.100.2.1 255.255.255.0
R2(config-if)#no shutdown

R2(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0, changed state to up

R2(config-if)#interface serial 0/3/0
R2(config-if)#ip address 200.100.12.2 255.255.255.252
R2(config-if)#no shutdon
                       ^
% Invalid input detected at '^' marker.
	
R2(config-if)#no shutdown

R2(config-if)#
%LINK-5-CHANGED: Interface Serial0/3/0, changed state to up

R2(config-if)#
%LINEPROTO-5-UPDOWN: Line protocol on Interface Serial0/3/0, changed state to up

R2(config-if)#interface serial 0/3/1
R2(config-if)#ip address 200.100.23.1 255.255.255.252
R2(config-if)#clock rate 128000
R2(config-if)#no shutdown

%LINK-5-CHANGED: Interface Serial0/3/1, changed state to down
R2(config-if)#end
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#R2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R2(config)#router ospf 1
R2(config-router)#network 200.100.2.1 0.0.0.255 area 0
R2(config-router)#network 200.100.12.2 0.0.0.3 area 0
R2(config-router)#network 200.100.23.1 0.0.0.3 area 0
R2(config-router)#end
R2#
%SYS-5-CONFIG_I: Configured from console by console
R2#show ip ospf neighbor

R2#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     200.100.2.0/24 is variably subnetted, 2 subnets, 2 masks
C       200.100.2.0/24 is directly connected, GigabitEthernet0/0
L       200.100.2.1/32 is directly connected, GigabitEthernet0/0
     200.100.12.0/24 is variably subnetted, 2 subnets, 2 masks
C       200.100.12.0/30 is directly connected, Serial0/3/0
L       200.100.12.2/32 is directly connected, Serial0/3/0

R2#show ip ospf interface

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.2.1/24, Area 0
  Process ID 1, Router ID 200.100.23.1, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State DR, Priority 1
  Designated Router (ID) 200.100.23.1, Interface address 200.100.2.1
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:00
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
Serial0/3/0 is up, line protocol is up
  Internet address is 200.100.12.2/30, Area 0
  Process ID 1, Router ID 200.100.23.1, Network Type POINT-TO-POINT, Cost: 64
  Transmit Delay is 1 sec, State POINT-TO-POINT, Priority 0
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
 
    Hello due in 00:00:09
  Index 2/2, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Suppress hello for 0 neighbor(s)
R2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R2(config)#interface lo 0

R2(config-if)#
%LINK-5-CHANGED: Interface Loopback0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface Loopback0, changed state to up

R2(config-if)#ip add 2.2.2.2 255.255.255.255
R2(config-if)#no shutdown
R2(config-if)#end
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#R2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R2(config)#router ospf 1
R2(config-router)#passive-interface 0/0
                                    ^
% Invalid input detected at '^' marker.
	
R2(config-router)#end
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#show ip ospf passive-interface
                ^
% Invalid input detected at '^' marker.
	
R2#show ip ospf interface

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.2.1/24, Area 0
  Process ID 1, Router ID 200.100.23.1, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State DR, Priority 1
  Designated Router (ID) 200.100.23.1, Interface address 200.100.2.1
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:08
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
Serial0/3/0 is up, line protocol is up
  Internet address is 200.100.12.2/30, Area 0
  Process ID 1, Router ID 200.100.23.1, Network Type POINT-TO-POINT, Cost: 64
  Transmit Delay is 1 sec, State POINT-TO-POINT, Priority 0
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:07
  Index 2/2, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Suppress hello for 0 neighbor(s)
R2#
R2#
R2#show ip osfp database
             ^
% Invalid input detected at '^' marker.
	
R2#show ospf database
        ^
% Invalid input detected at '^' marker.
	
R2#show ip ospf database
            OSPF Router with ID (200.100.23.1) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
200.100.23.1    200.100.23.1    371         0x80000002 0x0047cb 2
R2#
R2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R2(config)#interface serial 0/3/0
R2(config-if)#bandwidth 1000
R2(config-if)#end
R2#
%SYS-5-CONFIG_I: Configured from console by console

Router3
Router#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#hostname R3
R3(config)#non ip domain-lookup
             ^
% Invalid input detected at '^' marker.
	
R3(config)#no ip domain-lookup
R3(config)#line console 0
R3(config-line)#passoword 
                    ^
% Invalid input detected at '^' marker.
	
R3(config-line)#password cisco
R3(config-line)#login
R3(config-line)#logging synchronous
R3(config-line)#line aux 0
R3(config-line)#login
% Login disabled on line 0, until 'password' is set
R3(config-line)#password cisco
R3(config-line)#login
R3(config-line)#line vty 0 4
R3(config-line)#paswword cisco
                   ^
% Invalid input detected at '^' marker.
	
R3(config-line)#password cisco
R3(config-line)#login
R3(config-line)#exit
R3(config)#enable secret class
R3(config)#banner motd <Authorized Access Only>
Enter TEXT message.  End with the character '<'.
<Authorized access only>

R3(config)#interface gigabitethernet 0/0
R3(config-if)#ip address 200.100.3.1 255.255.255.0
R3(config-if)#no shutdown

R3(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0, changed state to up

R3(config-if)#interface serial 0/3/0
R3(config-if)#up address 200.100.13.2 255.255.255.252
              ^
% Invalid input detected at '^' marker.
	
R3(config-if)#ip address 200.100.13.2 255.255.255.252
R3(config-if)#clock rate 128000
R3(config-if)#no shutdown

R3(config-if)#
%LINK-5-CHANGED: Interface Serial0/3/0, changed state to up

R3(config-if)#interface serial 
%LINEPROTO-5-UPDOWN: Line protocol on Interface Serial0/3/0, changed state to up

R3(config-if)#interface serial 0/3/1
R3(config-if)#ip address 200.100.23.2 255.255.255.252
R3(config-if)#no shutdown

R3(config-if)#
%LINK-5-CHANGED: Interface Serial0/3/1, changed state to up

R3(config-if)#end
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#
%LINEPROTO-5-UPDOWN: Line protocol on Interface Serial0/3/1, changed state to up

R3#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R3(config)#router ospf 1
R3(config-router)#network 200.100.3.1 0.0.0.255 area 0
R3(config-router)#network 200.100.13.2 0.0.0.3 area 0
R3(config-router)#ne
01:30:35: %OSPF-5-ADJCHG: Process 1, Nbr 200.100.13.1 on Serial0/3/0 from LOADING to FULL, Loading Done

R3(config-router)#network 200.100.23.2 0.0.0.3 area 0
R3(config-router)#
01:30:58: %OSPF-5-ADJCHG: Process 1, Nbr 200.100.23.1 on Serial0/3/1 from LOADING to FULL, Loading Done

R3(config-router)#end
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R3(config)#interface lo 0

R3(config-if)#
%LINK-5-CHANGED: Interface Loopback0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface Loopback0, changed state to up

R3(config-if)#ip add 3.3.3.3 255.255.255.255
R3(config-if)#no shutdown
R3(config-if)#end
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#router ospf 1
          ^
% Invalid input detected at '^' marker.
	
R3#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R3(config)#router ospf 1
R3(config-router)#passive-interface 0/0
                                    ^
% Invalid input detected at '^' marker.
	
R3(config-router)#bandwidth 1000
                  ^
% Invalid input detected at '^' marker.
	
R3(config-router)#end
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#config t
Enter configuration commands, one per line.  End with CNTL/Z.
R3(config)#interface serial 0/3/0
R3(config-if)#bandwidth 1000
R3(config-if)#end
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#show ip ospf neigbor
                    ^
% Invalid input detected at '^' marker.
	
R3#shoe ip ospf neighbor
        ^
% Invalid input detected at '^' marker.
	
R3#show ip ospf neighbor


Neighbor ID     Pri   State           Dead Time   Address         Interface
200.100.23.1      0   FULL/  -        00:00:39    200.100.23.1    Serial0/3/1
200.100.13.1      0   FULL/  -        00:00:36    200.100.13.1    Serial0/3/0
R3#shoe ip route
        ^
% Invalid input detected at '^' marker.
	
R3#show ospf interface
        ^
% Invalid input detected at '^' marker.
	
R3#show ip ospf interface

GigabitEthernet0/0 is up, line protocol is up
  Internet address is 200.100.3.1/24, Area 0
  Process ID 1, Router ID 200.100.23.2, Network Type BROADCAST, Cost: 1
  Transmit Delay is 1 sec, State DR, Priority 1
  Designated Router (ID) 200.100.23.2, Interface address 200.100.3.1
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:04
  Index 1/1, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 0, Adjacent neighbor count is 0
  Suppress hello for 0 neighbor(s)
Serial0/3/0 is up, line protocol is up
  Internet address is 200.100.13.2/30, Area 0
  Process ID 1, Router ID 200.100.23.2, Network Type POINT-TO-POINT, Cost: 100
  Transmit Delay is 1 sec, State POINT-TO-POINT, Priority 0
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:06
  Index 2/2, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 1 , Adjacent neighbor count is 1
    Adjacent with neighbor 200.100.13.1
  Suppress hello for 0 neighbor(s)
Serial0/3/1 is up, line protocol is up
  Internet address is 200.100.23.2/30, Area 0
  Process ID 1, Router ID 200.100.23.2, Network Type POINT-TO-POINT, Cost: 64
  Transmit Delay is 1 sec, State POINT-TO-POINT, Priority 0
  No designated router on this network
  No backup designated router on this network
  Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
    Hello due in 00:00:00
  Index 3/3, flood queue length 0
  Next 0x0(0)/0x0(0)
  Last flood scan length is 1, maximum is 1
  Last flood scan time is 0 msec, maximum is 0 msec
  Neighbor Count is 1 , Adjacent neighbor count is 1
    Adjacent with neighbor 200.100.23.1
  Suppress hello for 0 neighbor(s)
R3#
R3#show ip ospf database
            OSPF Router with ID (200.100.23.2) (Process ID 1)

                Router Link States (Area 0)

Link ID         ADV Router      Age         Seq#       Checksum Link count
200.100.13.1    200.100.13.1    277         0x80000004 0x00262f 3
200.100.23.1    200.100.23.1    254         0x80000005 0x002f51 4
200.100.23.2    200.100.23.2    87          0x80000006 0x005041 5
R3#
C:\>ping 200.100.2.3

Pinging 200.100.2.3 with 32 bytes of data:

Reply from 200.100.2.3: bytes=32 time=3ms TTL=125
Reply from 200.100.2.3: bytes=32 time=4ms TTL=125
Reply from 200.100.2.3: bytes=32 time=6ms TTL=125
Reply from 200.100.2.3: bytes=32 time=10ms TTL=125

Ping statistics for 200.100.2.3:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 3ms, Maximum = 10ms, Average = 5ms

C:\>

