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1.1. Routing in Swansea network
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2.2. Create all appropriate A records for all servers on Swansea and London Network
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[bookmark: _Toc216347288]3.1 Configuring Site-to-site VPN to London Network.
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Setting up a successful persistent connection between the two networks and using strong encryption.
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[bookmark: _Toc216347290]4.1 Creating user accounts for yourname.acca domain with all the parameters defined in the users_list_updated.xlsx document.
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[bookmark: _Toc216347292]5.1. join L-CD, clientS1, ClientL 1 to the yourname.acca domain
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[bookmark: _Toc216347294]6.1 Configuring S-DC as DHCP Server. The range is X.X.X. 10- X.X.X.20 for each network.
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Determine other DHCP options as per the infrastructure.
6.2. Configuring L-CD as DHCP Relay Server.
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6.3 Automatic IP Address updates for clients via DHCP Server.
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[bookmark: _Toc216347296]7.1 Test the network for connectivity.
The Swansea and London networks are connected and operational.
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[bookmark: _Toc216347298]8.1 Mount second disk drive to E:/Swanseafiles. Share and design required permissions. Only the domain users need to have full control permissions and other network users have read only access.
8.1 Mounting second disk drive
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8.2 Sharing and designing required permissions
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In sharing and assigning permissions, only the domain users can have full access to control permissions, while other users can have (read only access).
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[bookmark: _Toc216347300]9.1. Creating webs.yourname.acca  website and enable windows internal authentication.
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[bookmark: _Toc216347301]10. Remote Desktop Services
[bookmark: _Toc216347302]10.1. Configuring remote access for S-DC from any other machines in the network.
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