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Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switch
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
2 within 120 means 2 login attempts within the last 120 seconds.
What does the block-for 30 mean in the above command?
Block-for 30 means to block any login attempts from the user for the next 30 seconds.
b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass
Note: A privilege level of 15 gives the user administrator rights.
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
R1 did not accept the Telnet connection. The reason for this is because SSH is enabled instead, which takes priority over Telnet.
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? When typing the username as admin, and the password adminpass, login failed, However, when using the username admin with the password Admin1p@55 the login succeeded.
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
After failing the login the second time, the connection is forcibly closed, and logins cannot be made for the next 30 seconds
From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? The banner that was set previously was displayed.
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
You are disconnected, as 2 failed attempts within that time period will result in the user being blocked from the system for the next 30 seconds due to failing twice in the last 120 seconds.
Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass
Enable Telnet and SSH on the VTY lines.
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
SSH connection was successful.
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
Protocol version 1 and protocol version 2
How would you provide multiple users, each with their own username, access to a network device?
By making more users using the username command however with a lower privilege level than 15 so that the users cannot cause any malicious damage to the network by having any elevated rights that they shouldn’t.
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Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  

Here is my report on Encryption standards
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Abstract
This report goes over in detail about various different standards that are available for the encryption of data and how they work. This report includes information on methods of encryption including AES, DES, RSA, SHA and OTP.


1.Introduction: What is encryption?
Encryption is a method of hiding a set of data or disguising a set of data as something else, or in such a way that it is unreadable. The point of encryption is to make a message that would usually be easy for someone other than the sender and receiver to read to become extremely difficult if not impossible for any unwanted reader from being able to read it due to it being essentially illegible without having access to a decryption key [1].
One of the more well known and old examples of a method of encryption would be the encryption method used by Roman emperor Julius Caesar some time between 100 B.C and 44 B.C, wherein each letter of a message would be shifted up or down a few positions in the alphabet to hide the message (effectively encrypting it), although because of this, there is only 25 combinations making it effectively one of the easiest encryption methods to crack today [2].
1.1 What are some examples of encryption?
Examples of encryption methods can include AES Encryption, DES Encryption, RSA Encryption, One Time Pad Encryption and SHA Encryption [3],[4],[5].
2. AES Encryption
AES Encryption is a method of encryption that was enforced by the National Institute of standards and technology in 2001. It is an encryption method that was made to surpass the much more popular DES encryption method at the time. AES stands for Advanced Encryption Standard. AES can be described as an encryption method that has a block length of precisely 128, while allowing for keys to have lengths of 128, 192 and 256 bits respectively. [6]
3.DES Encryption
DES Encryption was the encryption method used before AES. DES was at one point considered to be one of the most popular encryption algorithms to be used at one point. It was originally enforced in 1977. DES encryption involved a plaintext message that would be up to 64 bits in length, combined with a 56 bit long key (of which was packed with 8 bits of parity) which results in a 64 bit long cryptogram being produced. [7]
4. RSA Encryption
RSA Encryption is essentially a method of encryption that takes advantage of elementary number theory. The idea behind RSA encryption is that the product of two large primary numbers multiplied together is used as a public key, while keeping the factors that made up the number for the public key completely secret which are therefore used as the secret key [8].
5. One Time Pad Encryption
One time pad is an encryption method wherein the idea behind how it works is that the plaintext is encrypted by using a key that is both the length of the plaintext, while also making the value of the key to be true random. The key is only to be used once and then never again, so any new messages must use a new key. Basically, how One Time Pad encrypts the plaintext is by combining each character of the plaintext with the character of the same position in the key to make an entirely new character. Once this has been made, the message is given to the receiver who will use the key. Once the key is used, all copies of the One Time Pad must be destroyed [9].
6. SHA Encryption
SHA Encryption is typically used with password for accounts. SHA encryption is done by turning the desired plaintext in to a checksum, and only storing the checksum. When the user enters their username and password, the password is turned in to a checksum first, then the checksum is sent to the server to be compared with the servers copy of the checksum. If the checksums match then the user is allowed to log in. There are several versions of SHA, including SHA-0, SHA-1, SHA-2 and more. SHA-0 was made in 1993 but didn’t really take off because of security issues, while SHA-1 replaced it in 1995, only to be then replaced between 2006-2010 with SHA-2. The reason that SHA-1 encryption  was replaced was once again because of a security issue that was discovered surrounding it, of which google has verified a checksum collision for.[5].
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