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	Risk and environmental impact assessment form 




	Contract name 
	Baglan Bridge Link Road
	Contract No
	D&BKD31095

	Assessed by
	Kamran Davies
	Assessment date
	12.03.2021
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	Activity / process
	Safety Hazards and Environmental Aspects and Impacts
	People at risk (tick)
	Risk rating (see table)
	Control measures - (including documentation required and compliance with procedures)
	Residual risk rating (see table)

	
	
	E
	C
	V
	S
	L
	R
	
	S
	L
	R

	Access/Egress
	Public interference and moving vehicles 
	(
	(
	
	3
	3
	9
	All site personnel to wear the approved hi-vis clothing in accordance with the current regulations. Briefings to be given to workforce so everyone has an understanding where the approved access and egress is. Tool box talks given to warn of any further hazards. Exclusion zones and designated walking routes to be installed if necessary. Members of the public to be reported if need be.
	2
	2
	4

	Working at height
	Erecting and working from mobile tower platforms. Falling from height.
	(
	(
	
	4
	3
	12
	Mobile towers to be erected by a competent person (PASMA trained minimum competency). Tower is fully checked, tagged and in safe working order to carry out the work. Toe boards required at all times to save objects falling and possibility of being struck and causing damage. Stabilisers are fitted. Exclusion zones much be implemented at least 2m either end of the tower. 
	2
	1
	2

	Noise/Dust
	Use of power tools could cause damage to hearing. Dust being exposed could cause lung cancer, asthma and silicosis. 
	(
	(
	(
	3
	3
	9
	The correct PPE is worn to carry out the tasks. The operative or people near the area must be wearing suitable ear defenders, impact goggles and FFP3 dust masks. All operatives must be face fitted. 
	1
	2
	2

	Working near a watercourse
	Weil’s disease
	(
	(
	(
	4
	3
	12
	All operatives to be made aware by including in the daily briefing Wash hands before eating food and appropriate gloves are to be worn at all times.
	4
	1
	4

	General use of plant
	Injury due to poor plant condition/lack of training. Not competent of the use of equipment
	(
	(
	
	4
	3
	12
	All tools and equipment is P.A.T tested and is suitable and fit for purpose. 
	2
	2
	4

	Manuel handling
	Possible chance of strain, falling and causing long term injury
	(
	(
	
	3
	3
	9
	All staff will be trained in the safe manual handling techniques. Where possible heavy materials/plant will be moved via mechanical means and manual handling kept to a minimum. Lift to what is comfortable and don’t over strain or stretch. Distribute to wait and ask someone to help. 
	2
	2
	4

	Working on an operational railway


	Struck by train, causing injury or death
	(
	(
	(
	5
	4
	20
	All team members are to hold a minimum of PTS competency. COSS to validate all sentinel cards. A full COSS brief is to be undertaken and all persons are to sign the declaration form to confirm they have understood the briefing. 
	5
	1
	5

	Re-fuelling site plant
	Pollution, dermatitis
	(
	(
	
	3
	2
	6
	Ensure that refuelling is carried out in a designated area, gloves to be worn at all times, plant is switched off before re-fuelling and tool box talk to be given on COSHH assessment. Spill kits to be available at all times.

PLANT NAPPIES TO BE USED FOR REFULLING.

	2
	1
	2

	Working at night
	Poor visibility
	(
	(
	(
	2
	3
	6
	Headtorches to be worn. Extra lighting in the form of handhelds or tripod lights to be on site. Make sure that generator running the lights is on a plant nappy. Extension leads if needed to be out of authorised walking routed avoid falling over and all plant is P.A.T tested.
	1
	1
	1

	Slips, trips and falls

	Wet sleepers, poor visibility, poor house keeping
	(
	(
	(
	2
	3
	6
	Use safe and authorised walking routes. Adequate footwear to be worn at all times, authorised access routes where possible and site kept clean and walk routes of mess and debris.
	2
	1
	2

	Site Specific Assessment - (to be completed by the person in charge if there are any changes to the work activity or site specific conditions)

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	Signature of the Person in Charge of the Works
	Kamran Davies
	Date
	12.03.2021

	E – Employees, C – Contractors or Suppliers, V – Visitors or Members of the Public
	Date of next review
	12.09.2021

	S – Severity multiplied by  L – Likelihood = R – Risk Rating - (high, medium or low – see guidance note SE-GN-61 for details)


This guidance must be used when completing the risk and environmental impact assessment form.
People at risk – 
(E) = Employees, (C) = Contractors or suppliers, (V) = Visitors, members of the public or damage to the wider environment – 

Place a tick in the column to indicate that this group of people may become affected by the hazards described.

Hazard –

A hazard is any situation with the potential to cause harm, injury, loss, environmental damage or pollution
Likelihood – 
(L) –
Likelihood is termed as the potential for the hazard to be realised (i.e. how likely is it to occur)
Severity – 
(S) –
The degree of injury, loss or environmental damage caused by the hazard



Risk rating –  (R) –
Use the table shown below to assess the risk rating for each of the hazards that have been identified. The risk rating is determined by identifying the level of severity and likelihood and finding the corresponding rating on the table shown below. This must be carried out both before and after the stated control measures have been implemented.

	
	
	Severity (S)
	
	1
	No injury, damage or environmental impact

	
	Ratings
	1
	2
	3
	4
	5
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	2
	Minor injury, damage or environmental impact

	Likelihood (L)
	1
	1
	2
	3
	4
	5
	
	3
	Moderate injury, damage or environmental impact

	
	2
	2
	4
	6
	8
	10
	
	4
	Major injury, damage or environmental impact

	
	3
	3
	6
	9
	12
	15
	
	5
	Catastrophic injury, loss, damage or environmental impact

	
	4
	4
	8
	12
	16
	20
	

	
	5
	5
	10
	15
	20
	25
	

	

	1
	It is very unlikely that the hazard will occur

	2
	It is unlikely that the hazard will occur

	3
	It is possible that the hazard will occur

	4
	It is likely that the hazard will occur

	5
	It is almost certain that the hazard will occur





Use the table to cross reference the severity rating (S) against the likelihood rating (L) to establish the overall risk rating (R) for the specified hazard.





Example – A severity rating of 3 with a likelihood rating of 3 corresponds within the table to identify the hazard as being rated 9 or of “Medium” risk.
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