RISK ASSESSMENT                                                                                                                                                                      Novus Construction

	Activity:
	Working around live services
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development 
	
	Assessment No.
	NC 001


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality
Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Striking/Damaging services pipes/cables resulting in injury, potentially fatal situations, loss of services.
	Employees

Contractors

Visitors

Pubic


	2
	3


	6
	Y
	A permit to excavate system will be enforced which requires Cable detection to be carried out, checks against SU drawings, visual checks for service covers and trial holes where necessary.  No excavation is to commence without a permit.  Careful digging techniques will be implemented and all known services will be exposed by hand digging.
	1
	3
	3

	Injury to personnel following service strikes
	Employees

Contractors

Visitors

Public
	2
	3
	6
	Y
	If, in the unfortunate event, a service cable or pipe is damaged all works are to cease immediately.  The incident is to be reported to the works manager, the area made safe  with all works operations ceased.  
	1
	3
	3

	Explosion due to gas main or service damage
	Employees 

Contractors

Visitors

Public
	1
	3
	3
	Y
	Following any damage to any service, regardless of whether or not there is a leak, works will cease and the damage will be reported to the works manager.
If there is a smell of gas, or if a ges main/service has knowingly been damaged all works will cease, any forms of ignition will be kept away from the area. No cutting operations, no smoking, pedestrians will be ushered away from the damaged service and asked not to smoke.
	1
	2
	2

	Damage to unearthed services
	Employees

Contractors 

Visitors

Public
	1
	3


	3
	Y
	Upon discovering a service or mains pipe, duct or cable, unearth the service using careful hand digging techniques.  Upon unearthing the service the site engineer will log the location, type of service, depth etc. before works progress.  To highlight an unearthed service it will be sprayed with a bright colour (red or white). The overseeing organisation will be consulted to determine if the service requires diverting. When backfilling over a service, sand will be used to surround it, warning tape where applicable and then care taken whilst backfilling.

	1
	3


	3

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest

	
	
	

	Foot Protection


	Y
	Hearing Protection


	Y
	Gloves

	Y
	Respiratory Protection

	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees
1) Information contained in this assessment. 2) Information contained in HSE Information sheet No. 8 Safety in Excavations.



	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………
	Activity:
	Site Security
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development 
	
	Assessment No.
	NC 002


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Working areas: 

Persons entering into works areas

Persons entering into site compound, site offices, lock-ups etc. vandalism, burglary.

Vandalism, removal of barriers, use of barriers, signs and/or materials as missiles.


	Public

Public, Employees

Public, Employees, Visitors
	2

2

2
	2

2

3
	4

4

6
	Y

Y

Y
	Works areas to be entirely sectioned off using suitable pedestrian interlocking barriers. Diversions implemented where necessary. Barriers to be maintained throughout the day by the workforce.  An appointed person will carry out checks on all barriers and signage at the start and end of every shift.  Out of hours emergency contact number to be displayed within works areas and a call out regime set up with a designated employee.  Out of hours contact to be supplied to local police and highway authority.  A closed gate policy will be implemented with plant access controlled by a designated banksman whilst a separate pedestrian access will be installed.  Site to be continuously monitored, control measures to be reviewed when necessary.

Site compound to be fenced off using anti-climb Heras fence panels double clipped top and bottom.  Site access to be securely locked out of hours.  Site offices, stores, cabins and welfare facilities secured out of hours Signs erected on fencing identifying the compound as a construction site with no unauthorised access permitted.  Heavy plant to be situated in front of stores overnight to deter theft.  Emergency contact displayed. 

Barriers to be securely erected and interlocking with each other.  All loose construction materials, debris, small tools etc. will be removed from the working area at the end of each shift.  No loose setting out pins to remain in place over the weekend. Checks of barriers to be completed as stated above.  


	1

1

1
	2

2

3
	2

2

3

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	
	Gloves


	Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 6 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………
	Activity:
	Use of lorry loader, Delivery of Plant & Equipment
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 003


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Contact with overhead cables

Electrocution

Collision with other plant/vehicles/personnel

Overturning of lorry-loader.

Crush injuries

Failure of lifting equipment.

Struck by falling objects

Falls from height.


	Employees

Employees

Employees

Employees

Employees
	2

2

2

3

2
	3

3

3

3

3
	6

6

6

9

6
	Y

Y

Y

Y

Y
	A suitable site inspection will be undertaken to determine the location of all overhead electric cables. No lifting operations will take place unless there is a minimum of 6 metres clearance between the lorry loader lifting arm and the cables.

Lifting area will be fenced off from other traffic using road cones. All workers will wear high visibility clothing.

Personnel not involved will be excluded from the working area.

Lifting will be supervised by a slinger / signaller.

The lorry will be places on firm level and even ground, avoiding manholes excavations and culverts.

The vehicle stabilisers will be fully extended and lowered on to wooden pads irrespective of ground conditions.

The weight of the load being lifted will be determined before the lift and will be within the SWL of the lorry-loader: cabins will be empty before being lifted. 

The vehicle will be located as close as possible to the load and unloading point.

The lorry-loader will only be operated by a competent driver.

All lifting items must be identifiable and be accompanied with up to date test certificates.

Safe working loads of lifting accessories will be established before use.

The legs of multi legged chains will be equally loaded.

The safety catches on all hooks will be closed.

If required hand/tag lines will be attached to the load.

Safe access will be provided for access for attaching / un-attaching lifting accessories. Ladders may be used for access of short duration as long as the equipment is in sound condition and the ladder is “footed” and is secure before use. 


	1

1

1

1

2
	3

3

3

3

3
	3

3

3

3

6

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	 Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	 Y
	Hearing Protection


	Y
	Gloves


	 Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment.



	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Site Clearance
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 004


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Infection with Leptospirosis (Weil’s disease) caused by contact with water or material contaminated with urine from infected rats
	Employees
	2
	3


	6
	Y
	Rats are not to be touched with unprotected hands.

Any cuts or grazes will be washed immediately with soap and running water. 

All cuts and broken skin will be covered with waterproof plasters before and during work.

Hands will be washed before eating drinking and smoking.

Protective clothing must be worn including gloves.

Rubbish will be disposed of regularly to avoid the possible infestation with vermin.
	1
	3


	3

	Needlestick Injuries resulting in blood loss and infection with blood-borne viruses.

NB. The term sharps usually refer to hypodermic needles but may include broken glass and knives.
	Employees
	2
	3
	6
	Y
	Bare hands are not to be used to pick up rubbish, clear out gullies,  or to unblock sewer pipes and toilets.

The handling of sharps is to be avoided; grabbing devices such as tongs will be kept in the site office and must be used

Sharps will be disposed of in appropriate containers not in plastic bags.

Steel mid-sole boots and puncture resistant gloves will be worn.

Personnel will only be permitted to eat and drink outside of the working areas during breaks.

Any wound received will receive urgent medical attention

All broken skin will be covered with a waterproof dressing prior to entering the working area.
	1
	3
	3

	
	
	
	
	
	
	
	
	
	

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	Y
	Gloves


	Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment.2) HSE Information card INDG84. Leptospirosis 3) HSE Leaflet INDG Blood-borne viruses




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Transport on Site
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 005


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	People being struck, crushed or run over by site plant and transport.
	Employees

Contractors

Pedestrians
	3
	3
	9
	Y
	All drivers will hold a relevant qualification or be subject to a competency check prior to operating any plant.

Vehicle routes will be planned to segregate pedestrians and vehicles, with routes being clearly marked.

All pedestrians will wear hi-visibility clothing.

Reversing will be kept to a minimum.

Vehicles will have all-round visibility and provide a warning to others using reversing alarms flashing beacons and lights.

Banksmen will be employed for all access to and from works areas.

Tipper vehicles will not be driven with a raised body.

The use of mobile telephones is prohibited when operating transport on site.
	1
	3


	3

	Operatives being thrown from their vehicle.
	Employees

Contractors
	3
	3


	9
	Y
	Seat belts will be worn at all times.

Speed restrictions will be imposed and rigidly enforced.

Passengers will not be carried unless additional seating is provided complete with seat belts.

Edge protection will be provided around all excavations.

When tipping into excavations stop-blocks will be put in place.

Vehicle routes will be maintained in good condition.


	1
	3


	3

	Material falling from plant.
	
	2
	3
	6
	Y
	Loads will not be slewed over personnel or vehicle cabs.

Operatives will not remain on vehicles whilst being loaded unless it is equipped with a FOPS cab.

Drivers must ensure vehicles are not overloaded and are loaded evenly
	1
	3
	3

	Electrocution caused by contact with overhead cables.
	Employees.

Contractors
	2
	3


	6
	Y
	Physical barriers and prominent notices will be used to restrict access under power lines.


	1
	3
	3

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	Seat belts
	Y

	Foot Protection


	Y
	Hearing Protection


	
	Gloves


	Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 2) HSE construction information sheet No 52 Safe use of compact dumpers.

3) HSE guidance note GS6 Avoidance of danger from overhead electric power lines.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Disc Cutting
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 006


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Eye injury from flying particles
	Employees

Contractors

Public
	3
	3
	9
	Y
	All operatives will be issued with and wear suitable eye protection.

Cutting will take place in dedicated cutting stations that will be screened from members of the public/workforce
	1
	3
	3

	Contact with the wheel causing lacerations or

amputation.
	Employees

Contractors
	3
	3
	3
	Y
	All guards will be in place and secure.

The equipment will only be used on firm level ground with the floor

area free from loose material or slippery material.

Operators will not wear baggy clothing.
	1
	3
	3

	Wheel bursting resulting in multiple injuries.
	Employees

Contractors
	2
	3
	6
	Y
	Only trained and authorised operatives will mount or operate a

disc cutter or abrasive wheel.

Chipped or damaged wheels will not be used.

The maximum speed of the wheel will be greater than that of the 

machine.

Only straight wheels will be used for cutting.

Only depressed centre wheels will be used for grinding
	1
	3
	3

	Fire caused by the creation of heat from friction

or sparks.
	Employees 

Contractors
	2
	2
	4
	Y
	A check will be made to ensure that sparks can not ignite any 

combustible material in the work area.

Petrol-engined machines will be refuelled away from the 

workplace.
	1
	2
	2

	Dust inhalation when cutting concrete and stone
	Employess

Contractors
	3
	3
	9
	Y
	Disc cutters will be used in conjunction with suppressed water bottle attachments.

P3 Dust masks will be issued to be worn during all cutting operations.
	1
	3
	3

	Hearing damage
	Emplyees

Contractors

Public
	3
	2
	6
	Y
	All operators will be equipped with hearing protection and will be

instructed in its use. 

Cutting operations within designated stations with solid barriers
	1
	3
	3

	Hand–arm vibration 
	Employees
	2
	3
	6
	Y
	Machines will only be used intermittently for short periods of time. HAV charts will be posted on site stating trigger times, this information will also be conveyed to the operatives
	1
	3
	3

	Fumes from fuel and exhausts
	Employees

Contractors

Public


	2
	2
	4
	Y
	Machines will only be used in well ventilated areas and never indoors.
	1
	2
	2

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	Y
	Gloves


	Y
	Respiratory Protection


	Y
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Manual Handling
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC007


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Lifting of Paving Slabs, Setts, Street Furniture, Other Construction Materials, Equipment

Lifting Heavy Loads, Lifting awkward loads, twisting while lifting, poor ground stabilisation, previous back problems, falling/dropping load

Repetitive Lifting, RSI, 


	Employees

Contractors

Employers

Contractors
	3

3
	2

2
	6

6
	
	Plan to eliminate the need for manual lifting, ensure personnel have been trained in lifting techniques, assess each individual for back/heart problems, if mechanical plant cannot be used lifting aides such as trolleys, pipe handlers, sack barrows etc should be used, operatives to complete manual handling operations checksheet

Lifting procedures to be adopted for repetitive lifting. Lifting and carrying of setts and paving slabs to be shared between the paving gang.  Carry distances to be minimised by positioning pallets close to works.  Stacks of setts to be positioned close to paver and handed to them.

Lifting charts will be posted on site for reference to materials and equipment weights along with guidelines for lifting procedures.

Manual Handling Assessments will be produced for the various lifting operations and conveyed to the workforce.


	1

1
	2
2
	2
2

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y 
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	
	Gloves


	Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Use of Vibrating Hand-Tools
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 008


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Hand-Arm Vibration syndrome (HAVs) and Vibration White Finger (VWF) caused by exposure to excessive levels of vibration. 
	Employees.

Contractors
	2
	2
	4
	Y
	An assessment will be made whether the job can be performed without the need for using hand-held tools.

The vibration level for the equipment will be identified from measurement or from suppliers’ information.

The exposure ready-reckoner table (displayed on site) will be used to calculate exposure limit times based on actual vibration levels.

Limit of repetitive cutting operations, eg. cutting setts/slabs, will also be displayed as a maximum no. of cuts per shift.

The use of high vibration tools will be limited to the lowest possible amount of time.

Where tools are in continual or frequent use, the users will be rotated to limit exposure times.

Several short exposure times will be employed where possible in preference to one continuous period of exposure.

All equipment will be maintained in accordance with manufacturers’ recommendations.

Gloves will always be worn for hand protection and to keep hands warm to encourage good blood circulation.

All operatives will be discouraged from smoking since this is known to reduce blood circulation.


	1
	2
	2

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.


	Head Protection


	Y
	Eye Protection


	Y


	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection
	Y


	Hearing Protection


	Y


	Gloves


	Y
	Respiratory Protection


	Y
	
	


	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 2) HSE Exposure points system and ready-reckoner.

3) HSE leaflet No.INDG 296 Hand-arm vibration




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Working with Plant And Machinery
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 009


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Entanglement with moving parts or materials in motion.

Crushing under plant or loose loads, Being thrown from plant.

Slipping, Tripping or falling whilst mounting/dismounting plant

Workplace Transport, collision with pedestrians, other workers, road vehicles, other plant

Noise, hearing damage due to working in a noisy environment.

Spillage /Contamination of watercourse


	Operatives

Employees

Operatives,

Employees

Pedestrians

Operatives

Employees

Operatives

Employees

Pedestrians

Employees.

Contractors

Pedestrians

Employees

Contractors

Environment
	2

2

2

2

3

2
	3

3

2

3

2

2
	6

6

4

6

6

4
	Y

Y

Y

Y
Y
	All dangerous parts to be guarded as per manufacturers standards.

Guards inspected as part of weekly plant checks

All operatives and fitters to be trained and competent to operate/work on plant/equipment.

No overloading of dumpers/telehandlers etc.

All plant to stick to designated haul routes.

Plant operatives to wear seat belts were fitted

Good housekeeping sitewide with rubbish, pallets, rubble cleared and disposed of daily.  Operatives to ensure clean and clear footing when mounting and dismounting.  Operatives to mount and dismount on level ground

Good pedestrian/vehicular segregation measures on site. 

High visibility clothing to be worn on site

Transport movements to be under the control of a banksman when entering/exiting works areas, compounds, pedestrianised areas,

Noise assessments to be carried out on all activities involving plant and equipment.

Sufficient measures implemented following assessment eg. hearing protection, change of working procedures

Fuel will be stored within the site compound in a double bunded bowser.

All refuelling of plant will be carried out directly from the bowser.

A soak-up drip tray will be in place at all times directly beneath the pump end of the bowser and replaced periodically.

Used soak-up trays will be disposed of in the COSHH skip on site.

Spill kits will be positioned adjacent to the bowser and in all site vans.

All plant and machinery checked at the start of each shift for leaks.

All drains in compound to be covered with plastic sheeting and barriered with sandbags.


	1

1

1

1

1

1
	3

2

2

3

2

2
	3

2

2

3

2

2

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.


	Head Protection


	Y
	Eye Protection


	Y


	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y


	Hearing Protection


	Y


	Gloves


	Y
	Respiratory Protection


	Y
	
	


	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 2) HSE Exposure points system and ready-reckoner.

3) HSE leaflet No.INDG 296 Hand-arm vibration




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Young Persons Risk Assessment :
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 010


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Falls from height
	Young Person
	3
	3
	9
	Y
	No young persons are allowed to work above ground level or 
	1
	3
	3

	
	
	
	
	
	
	enter into excavations
	
	
	

	
	
	
	
	
	
	
	
	
	

	Eye injuries
	Young Person
	3
	2
	6
	Y
	Young persons are not permitted to operate hand or power tools,
	1
	2
	2

	
	
	
	
	
	
	eye protection must be worn when observing operatives using 
	
	
	

	
	
	
	
	
	
	hand and power tools.
	
	
	

	
	
	
	
	
	
	
	
	
	

	Hearing Damage
	Young Person
	2
	3
	6
	Y
	Young persons are not permitted to operate or work in the vicinity
	1
	2
	2

	
	
	
	
	
	
	of noisy work equipment. Where doubt exists hearing protection 
	
	
	

	
	
	
	
	
	
	will be issued and worn.
	
	
	

	
	
	
	
	
	
	
	
	
	

	Sprains and Strains
	Young Person
	3
	2
	6
	Y
	Manual handling will be avoided by Young persons.
	2
	2
	4

	
	
	
	
	
	
	Training in correct lifting techniques will be given and no weight 
	
	
	

	
	
	
	
	
	
	lifted will exceed 15kg.
	
	
	

	
	
	
	
	
	
	
	
	
	

	Harmful Substances
	Young Person
	2
	3
	6
	Y
	No young person will be exposed to substances that are toxic
	1
	2
	2

	
	
	
	
	
	
	carcinogenic or involve the harmful exposure to radiation.
	
	
	

	
	
	
	
	
	
	                                     
	
	
	

	
	
	
	
	
	
	No Young person will be exposed to risks to health from extreme
	
	
	

	
	
	
	
	
	
	cold or heat.
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	Site induction will be provided and repeated monthly.
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	No duties will be given to the Young person that is beyond his
	
	
	

	
	
	
	
	
	
	physical or psychological capacity.
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	Other site personnel will be instructed of the “risks” and
	
	
	

	
	
	
	
	
	
	precautions associated with young persons.
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	The site supervisor will undertake regular checks on young 
	
	
	

	
	
	
	
	
	
	persons during work.
	
	
	

	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	No young person will operate powered work equipment.
	
	
	

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	√
	Eye Protection


	√
	Hi-visibility clothing


	√
	Fall Arrest


	
	
	

	Foot Protection


	√
	Hearing Protection


	√
	Gloves


	√
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 2) Site induction. 3) Employee Health and Safety Handbook.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………
	Activity:
	Noise At Work
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 011


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Hearing Damage, caused by :-

· Prolonged exposure to noise above 80dB(A)

· Any exposure to noise above 85dB(A) (200 pascals)
	Employees

Contractors
	3
	2
	6
	Y


	Noise levels will be reduced to their lowest practicable levels other than using PPE, ie by engineering controls.

At noise levels between 80 and 85dB(A). Employees will be advised to wear hearing protection and they will be provided with it upon request.

At noise levels above 85Db(A) hearing protection zones will be established where the wearing of hearing protection is mandatory. Access to hearing protection zones will be restricted and signs erected accordingly.

Hearing protection will be compatible with other PPE and be capable of reducing exposure at the ear to below 80dB(A)

Dirty and damaged hearing protection will be replaced; dirty ear plugs will not be used. 
	1
	2
	2

	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	Y
	Gloves


	Y
	Respiratory Protection


	
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

2) Information contained in this assessment. 2) HSE Publication indg 363(rev1) Protect your hearing or lose it.




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………
	Activity:
	Fuel Storage
	
	Assessed by
	Nathan Hunt

	Location
	Plot E9 Development
	
	Assessment No.
	NC 012


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable).  4-6 =Medium (acceptable, consider further control measures).  9 =Unacceptable/Critical risk (Do not proceed)

	Hazard  Identification
	People at Risk
	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Intoxicating fumes through poor ventilation

Splashing into eyes

Spillages

Contact with skin/ Damage to skin

Risk of Fire


	Operatives

Employees

Visitors

Operatives,

Employees

Pedestrians

Operatives

Employees

Operatives

Employees

Pedestrians

Employees.

Contractors

Pedestrians


	2

2

2

2

3


	3

3

2

3

2


	6

6

4

6

6


	Y

Y

Y

Y

Y
	Storage containers to be sealed and closed when inside.

Containers only opened outside.

Storage Sheds to be ventilated.

No overloading of dumpers/telehandlers etc.

All plant to stick to designated haul routes.

Plant operatives to wear seat belts were fitted

Containers kept closed and sealed when not in use.

Refuelling to be carried out in the open and on level surface.

Drains within the vicinity of fuel storage and refuelling operations to be protected with sandbags and plastic sheeting.

soak-up drip tray will be in place at all times directly beneath the pump end of the bowser and replaced periodically.

Used soak-up trays will be disposed of in the COSHH skip on site.

Spill kits will be positioned adjacent to the bowser and in all site vans.

All plant and machinery checked at the start of each shift for leaks

Gloves and protective clothing will be worn when handling fuel/refuelling etc.

COSHH assessments for fuel to be supplied to the anyone likely to come into contact with fuel.

Petrol to be stored in a sealed 25L containers with no more than 2 stored on site at any one time.

All fuel to be stored away from sources of ignition eg. Electrical switching, disc cutting, generators etc.

Fuel to be within a lockable container with authorised access only.

No hot works to be performed on or near the storage vessel of any fuel unless previously purged.

Keep drums/containers away from direct heat and located in areas where there is no risk of vehicular collision
	1

1

1

1

1


	3

2

2

3

2


	3

2

2

3

2



	PERSONAL PROTECTIVE EQUIPMENT

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.


	Head Protection


	Y
	Eye Protection


	Y


	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y


	Hearing Protection


	Y


	Gloves


	Y
	Respiratory Protection


	Y
	
	


	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 2) HSE Exposure points system and ready-reckoner.

3) HSE leaflet No.INDG 296 Hand-arm vibration




	The Following Persons Have Received And Understand The Information Contained In This Assessment.

	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor………………………………………………..                       Date………………………………

	Activity:
	Dust
	
	Assessed by
	Mark Jones

	Location
	Plot E9 Development
	
	Assessment No.
	NC 013


	Legend:       Likelihood 1 = Unlikely. 2 = Possible. 3 = Likely.   Severity 1 = Minor Injury. 2 = Major Injury. 3 = Fatality

                    Risk rating (Likelihood x Severity) :- 1-3 = Low (acceptable). 4- 6 = Medium (consider further control measures).  9 = Unacceptable/Critical risk (Do not proceed)

	Hazard Identification
	People at Risk


	Initial potential for harm
	Action Req’d

(Y/N)
	Control Measures
	Residual potential for harm

	
	
	L
	S
	R
	
	
	L   
	S 
	R

	Dust resulting in inhalation, possible silicosis, general nuisance, 


	Employees

Contractors

Public
	3
	2
	6
	Y
	All cutting operations will be carried out in designated cutting bays.  Operatives cutting within these bays shall wear dusk masks minimum grade FFP3.  All cutting of stone, concrete, tarmac will require dust suppressant in the form of an attached water bottle that is prevented from running out and pumped at regular intervals to maintain pressure.  The water bottle will be attached and in operation from the moment the cutting commences.  No dry cutting is permitted, not even to score the slab.

At the end of each working day the cutting stations will be dampened down and cleared out to prevent the build up of settled dust.  During dry conditions this may be required more frequently and will be as directed on site.  

A suction sweeper is utilised on a weekly bases to removed dust and dirt from the site.  During dry conditions this again may require increasing.  

During gusty/windy conditions dust may be a nuisance and this is why we must minimise its build up.  General good housekeeping, keeping your working areas clear, regular sweeping up is required.

Other operations where dust may cause harm is:

· Mixing slurry primer

· Mixing flowpoint (flowable grout)

· Mixing Cement/Concrete

Please use appropriate PPE for these operations.  Appropriate PPE is listed within the COSHH data sheets available in the site office.


	2
	1


	2

	Personal Protective Equipment

The following PPE will be required for the work activities stated. Ensure that the correct type of PPE is selected.

	Head Protection


	Y
	Eye Protection


	Y
	Hi-visibility clothing


	Y
	Fall Arrest


	
	
	

	Foot Protection


	Y
	Hearing Protection


	
	Gloves


	Y
	Respiratory Protection


	Y
	
	

	Review And Monitoring

This assessment will be reviewed in the light of further information becoming available or a change in conditions and/or circumstances to render it no longer relevant.

In any event this assessment will be reviewed after 12 months to ensure that it remains valid.



	Information To Be Provided To Employees

1) Information contained in this assessment. 




	The Following Persons Have Received And Understand The Information Contained In This Assessment.


	Name
	Signature
	Date
	Name
	Signature
	Date

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	


Signed by Assessor……………………………………………….                         Date………………………………

