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Lab - Accessing Network Devices with SSH

Lab - Accessing Network Devices with SSH 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.1.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.11
	255.255.255.0
	192.168.1.1

	PC-A
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.1


Objectives
Part 1: Configure Basic Device Settings
Part 2: Configure Basic Security Measures on the Router and Switch
Part 3: Configure the Router for SSH Access
Part 4: Configure the Switch for SSH Access
Part 5: SSH from the CLI on the Switch
Background / Scenario
In the past, Telnet was the most common network protocol used to remotely configure network devices. Telnet does not encrypt the information between the client and server. This allows a network sniffer to intercept passwords and configuration information.
Secure Shell (SSH) is a network protocol that establishes a secure terminal emulation connection to a router or other networking device. SSH encrypts all information that passes over the network link and provides authentication of the remote computer. SSH is rapidly replacing Telnet as the remote login tool of choice for network professionals. SSH is most often used to log in to a remote device and execute commands; however, it can also transfer files using the associated Secure FTP (SFTP) or Secure Copy (SCP) protocols.
The network devices that are communicating must be configured to support SSH in order for SSH to function. In this lab, you will enable the SSH server on a router and then connect to that router using a PC with an SSH client installed. On a local network, the connection is normally made using Ethernet and IP.
Note: The routers used with CCNA hands-on labs are Cisco 1941 Integrated Services Routers (ISRs) with Cisco IOS Release 15.2(4)M3 (universalk9 image). The switches used are Cisco Catalyst 2960s with Cisco IOS Release 15.0(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of this lab for the correct interface identifiers.
Note: Make sure that the routers and switches have been erased and have no startup configurations. If you are unsure, contact your instructor.
Required Resources
1 Router (Cisco 1941 with Cisco IOS Release 15.2(4)M3 universal image or comparable)
1 Switch (Cisco 2960 with Cisco IOS Release 15.0(2) lanbasek9 image or comparable)
1 PC (Windows 7 or 8 with terminal emulation program, such as Tera Term, and Wireshark installed)
Console cables to configure the Cisco IOS devices via the console ports
Ethernet cables as shown in the topology
Configure Basic Device Settings
In Part 1, you will set up the network topology and configure basic settings, such as the interface IP addresses, device access, and passwords on the router.
Cable the network as shown in the topology.
Step 1: Initialize and reload the router and switch.
Step 2: Configure the router.
a. Console into the router and enable privileged EXEC mode.
b. Enter configuration mode.
c. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
d. Assign class as the privileged EXEC encrypted password.
e. Assign cisco as the console password and enable login.
f. Assign cisco as the VTY password and enable login.
g. Encrypt the plaintext passwords.
h. Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
i. Configure and activate the G0/1 interface on the router using the information contained in the Addressing Table.
j. Save the running configuration to the startup configuration file.
Configure PC-A.
Configure PC-A with an IP address and subnet mask.
Configure a default gateway for PC-A.
Verify network connectivity.
Ping R1 from PC-A. If the ping fails, troubleshoot the connection.



1. Configure Basic Security Measures on the Router
b. Encrypt the clear text passwords.
R1(config)# service password-encryption
b. Strengthen passwords.
An administrator should ensure that passwords meet the standard guidelines for strong passwords. These guidelines could include combining letters, numbers and special characters in the password and setting a minimum length.
Note: Best practice guidelines require the use of strong passwords, such as those shown here, in a production environment. However, the other labs in this course use the cisco and class passwords for ease in performing the labs.
2. Change the privileged EXEC encrypted password to meet guidelines.
R1(config)# enable secret Enablep@55
2. Require that a minimum of 10 characters be used for all passwords.
R1(config)# security passwords min-length 10
b. Secure the console and VTY lines.
3. You can set the router to log out of a connection that has been idle for a specified time. If a network administrator was logged into a networking device and was suddenly called away, this command automatically logs the user out after the specified time. The following commands cause the line to log out after five minutes of inactivity.
R1(config)# line console 0
R1(config-line)# exec-timeout 5 0
R1(config-line)# line vty 0 4
R1(config-line)# exec-timeout 5 0
R1(config-line)# exit
R1(config)#
3. The following command impedes brute force login attempts. The router blocks login attempts for 30 seconds if someone fails two attempts within 120 seconds. This timer is set especially low for the purpose of this lab.
R1(config)# login block-for 30 attempts 2 within 120
What does the 2 within 120 mean in the above command?
This means that a user has tried to enter a password twice and failed within the 120 seconds of trying

What does the block-for 30 mean in the above command?
If the user is blocked, then they are blocked for 30 seconds within the 120 second.

b. Verify that all unused ports are disabled.
Router ports are disabled by default, but it is always prudent to verify that all unused ports are in an administratively down state. This can be quickly checked by issuing the show ip interface brief command. Any unused ports that are not in an administratively down state should be disabled using the shutdown command in interface configuration mode.


R1# show ip interface brief
Interface                  IP-Address      OK? Method Status                Protocol
Embedded-Service-Engine0/0 unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/0         unassigned      YES NVRAM  administratively down down    
GigabitEthernet0/1         192.168.1.1     YES manual up                    up      
Serial0/0/0                unassigned      YES NVRAM  administratively down down    
Serial0/0/1                unassigned      YES NVRAM  administratively down down    

Configure the Router for SSH Access
Using Telnet to connect to a network device is a security risk because all information is transmitted in a clear text format. SSH encrypts the session data and provides device authentication, which is why SSH is recommended for remote connections. In Part 2, you will configure the router to accept SSH connections over the VTY lines.
Configure device authentication.
The device name and domain are used as part of the crypto key when it is generated. Therefore, these names must be entered prior to issuing the crypto key command.
Configure the domain for the device.
R1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
R1(config)# crypto key generate rsa modulus 1024
The name for the keys will be: R1.ccna-lab.com

% The key modulus size is 1024 bits
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds) 

R1(config)#
*Jan 28 21:09:29.867: %SSH-5-ENABLED: SSH 1.99 has been enabled
Configure a local database username.
R1(config)# username admin privilege 15 secret adminpass
Note: A privilege level of 15 gives the user administrator rights.
Enable SSH on the VTY lines.
Enable Telnet and SSH on the inbound VTY lines using the transport input command.
R1(config)# line vty 0 4
R1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
R1(config-line)# login local
R1(config-line)# end
R1#
Save the running configuration to the startup configuration file.
R1# copy running-config startup-config
Destination filename [startup-config]?
Building configuration...
[OK]
R1#
Establish an SSH connection to the router.
Start Tera Term from PC-A.
Use Tera Term to telnet to R1.
Does R1 accept the Telnet connection? Explain.
           NO as Telnet was classed as no longer safe and Sucre as it was disabled at the transport command line.
Use Tera Term, establish an SSH session to R1. Use the username admin and password adminpass. You should be able to establish an SSH session with R1.
Does R1 accept the SSH connection? Yes.
Intentionally mistype the user and password information to see if login access is blocked after two attempts.
What happened after you failed to login the second time?
I have tried to enter a password twice and failed within the 120 seconds of trying so I must wait for 30 seconds until I can log in again.
From your console session on the router, issue the show login command to view the login status. In the example below, the show login command was issued within the 30 second login blocking period and shows that the router is in Quiet-Mode. The router will not accept any login attempts for 14 more seconds.
R1# show login
     A default login delay of 1 second is applied.
     No Quiet-Mode access list has been configured.

     Router enabled to watch for login Attacks.
     If more than 2 login failures occur in 120 seconds or less,
     logins will be disabled for 30 seconds.

     Router presently in Quiet-Mode.
     Will remain in Quiet-Mode for 14 seconds.
     Denying logins from all sources.
R1#
After the 30 seconds has expired, SSH to R1 again and login using the SSHadmin username and Admin1p@55 for the password.
After you successfully logged in, what was displayed? The MOTD Banner was displayed on the screen.
Enter privileged EXEC mode and use Enablep@55 for the password.
If you mistype this password, are you disconnected from your SSH session after two failed attempts within 120 seconds? Explain.
No! as you are only blocked for 30 seconds, if you wait for 120 seconds you can try again. As you have not logged into the ssh.

Issue the show running-config command at the privileged EXEC prompt to view the security settings you have applied.
Configure the Switch for SSH Access
In Part 3, you will configure the switch in the topology to accept SSH connections. After the switch has been configured, establish an SSH session using Tera Term.
Configure the basic settings on the switch.
Console into the switch and enable privileged EXEC mode.
Enter configuration mode.
Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
Assign class as the privileged EXEC encrypted password.
Assign cisco as the console password and enable login.
Assign cisco as the VTY password and enable login.
Encrypt the plain text passwords.
Create a banner that will warn anyone accessing the device that unauthorized access is prohibited.
Configure and activate the VLAN 1 interface on the switch according to the Addressing Table.
Save the running configuration to the startup configuration file.
Configure the switch for SSH connectivity.
Use the same commands that you used to configure SSH on the router in Part 2 to configure SSH for the switch.
Configure the device name as listed in the Addressing Table.
Configure the domain for the device.
S1(config)# ip domain-name ccna-lab.com
Configure the encryption key method.
S1(config)# crypto key generate rsa modulus 1024
Configure a local database username.
S1(config)# username admin privilege 15 secret adminpass
Enable Telnet and SSH on the VTY lines.
S1(config)# line vty 0 15
S1(config-line)# transport input telnet ssh
Change the login method to use the local database for user verification.
S1(config-line)# login local
S1(config-line)# end
Establish an SSH connection to the switch.
Start Tera Term from PC-A, and then SSH to the SVI interface on S1.
Are you able to establish an SSH session with the switch?
Yes
SSH From the CLI on the Switch
The SSH client is built into the Cisco IOS and can be run from the CLI. In Part 4, you will SSH to the router from the CLI on the switch.
View the parameters available for the Cisco IOS SSH client.
Use the question mark (?) to display the parameter options available with the ssh command.
[bookmark: _GoBack]S1# ssh ?
  -c    Select encryption algorithm
  -l    Log in using this user name
  -m    Select HMAC algorithm
  -o    Specify options
  -p    Connect to this port
  -v    Specify SSH Protocol Version
  -vrf  Specify vrf name
  WORD  IP address or hostname of a remote system
SSH to R1 from S1.
You must use the –l admin option when you SSH to R1. This allows you to log in as user admin. When prompted, enter adminpass for the password.
S1# ssh -l admin 192.168.1.1
Password: 
***********************************************
  Warning: Unauthorized Access is Prohibited!
***********************************************

R1#
You can return to S1 without closing the SSH session to R1 by pressing Ctrl+Shift+6. Release the Ctrl+Shift+6 keys and press x. The switch privileged EXEC prompt displays.
R1#
S1#
To return to the SSH session on R1, press Enter on a blank CLI line. You may need to press Enter a second time to see the router CLI prompt.
S1#
[Resuming connection 1 to 192.168.1.1 ... ]

R1#
To end the SSH session on R1, type exit at the router prompt.
R1# exit

[Connection to 192.168.1.1 closed by foreign host]
S1#

What versions of SSH are supported from the CLI?
S1# ssh – v ?
1 Protocol Version 1
2 Protocol Version 2


How would you provide multiple users, each with their own username, access to a network device?

By adding each person username and password to the local database, by using the username command. 

Reflection (max 800 words): 
Write a research report comparing various Encryption standards, e.g AES, SHA, DES, RSA.  

Introduction 
Encryption is the process of encoding(hiding) information and data to prevent some one from unauthorized access to the information and data and either misusing or corrupting it.  There are a few different types of cryptographic methods, encryption and de-cryption systems must be applied in physical and security layer of the computer. The two standards used are: - [1]

Secret Key (Symmetric Key) in a symmetric cryptosystem the same key is used for both encryption and de-cryption. [2]
Public Key (Asymmetric Key) the encryption and de-cryption keys are different but related, the encryption key is known as a public key and the de-cryption key is known as the private key. The public and private keys are known as a key pair. [3]
ASE (Advanced Encryption Standard)

In 1998 Joan Daemen and Vincent Rijmen developed AES as a symmetric key block cipher, ASE can support a large combination of data 128 bits key and up to 256 bits. The encryption and de-cryption goes though 10 rounds for 128 and 14 rounds for 256-bit keys to deliver the final cipher or to retrieve the data. [4] 
SHA (Secure Hash Algorithm)
SHA is a family of cryptographic functions designed to keep information and data safe. It transforms the information and data using a hash function which consists of bitwise operations, compression functions and modular additions. The hash function produces a fixed size string that looks nothing like the original. The system is designed to be one-way functions so once they have been transformed into hash values, they are virtually impossible to transform them back again, which make it very hard to be hacked.
SHA encrypts passwords as the server side only needs to keep track of a specific person hash value, rather than the actual password, this is helpful in case a hacker tries to hack the database as they will only find the hashed functions and not the real passwords. [5]


DES (Data Encryption Standard) 
DES is widely accepted and publicly used and available cryptographic systems, IBM developed it in the 1970’s, but NIST (National Institute of Standards and Technology) it was sent to NBS (National Bureau of Standards) as a way to protect sensitive and unclassified government data. DES is no longer safe due to its small size if a poor key is used a strong force attack will crack the encryption, although DES can work in different modes such as CBC, ECB, CFB and OFB which makes if very flexible, but was cracked in January 1999 within 22 hours and 15 minutes by EFF(Electronic Frontier Foundation) [6] 

RSA (Rivest Shamir Adleman)
1977 was when RSA was founded, used as a public cryptosystem key, RSA is a cryptographic algorithm witch was named after Rivest Shamir Adleman or RSA for short the founder and creator, it is known as one of the most well known public cryptosystem for digital signatures and blocks of data. [7]

RSA is based on number theory which can block cipher systems, its use’s two prime numbers to create the public and private keys, which can be 1024 to 4096 bits. The two different keys are used to encrypt and de-crypt, the sender encrypts a message and a user who receives then decrypts the information or data with their own key.
RSA has a few problems in the design and are not good for commercial use, if the small values of p and q are used for the designing of a key, the encryption becomes too weak and can be decrypted by using random probability theory and side channel attacks. 
Whereas if you were to use large p and q lengths then it takes more time and the speed and performance degrades and slows down. [8]  
Conclusion 

Each of the cryptographic systems had points of strengths and weakness, and SHA is the best out of all the other systems as it makes it very hard for hackers to hack it with the information and data changing into random code. SHA-1 is hackable but SHA-3 is the most secure of all the SHA series. 
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