Networks and Cyber security Essentials



Student name
Student ID
Module Code
Lecturer 

Contents

1- Build a Simple Network (include Wired and Wireless device)
2- Addressing Scheme to the Network
3- Configure the IP address
4- Use necessary command to check if the connection is successful and document the results.
5- Use appropriate capture 
6- Draw both Physical and Logical Topology and document the successful.


I Built My Simple Network My House Physical
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I Built My Simple Network My House Logical
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	DEVICE
	INTERFACE
	IP ADDRESS
	SUBNET
	DEFAULT GETAWAY

	PC 1
	NIC
	192.168.1.1
	255.255.255.0
	255.255.255.0

	PC 2
	NIC
	192.168.2.100
	
	

	PRINTER
	NIC
	192.168.1.2
	255.255.255.0
	192.168.1.1

	TABLET
	NIC
	192.168.2.102
	255.255.255.0
	192.168.2.2

	WIRLESS ROUTER
	NIC
	192.168.2.2
	255.255.255.0
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(Command Prompt

Pinging 192.168.2.2 with 32 bytes of dat

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping statistics for 192.168.2.
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

>
C:\>ping 192.168.3.2

Pinging 192.168.3.2 with 32 bytes of dat

Reply from 192.168.3.2: bytes=3z
Reply from 192.168.3.2: bytes=3z
Reply from 192.168.3.2: bytes=3z
Reply from 192.168.3.2: bytes=3z

Ping statistics for 192.168.3.
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = lms, Maximm = Sms, Average = 3ms
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[Command Prompt

Packet Tracer BC Command Line 1.0

FastEthernet0 Connection: (default port)

Link-local IPVE Address.........: FES0::209:7CEFF:FEE:
IP AdAress......................: 192.168.1.10
SUBRET MaSK.....................: 255.255.255.0
Default Gateway.................: 192.168.1.1

Bluetooth Connection:
Link-local IPvG Address
IP Address..

Subnet Mask....
Default Gateway.

>





