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Practical work
Utilising ARP and routing tables:
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Deploy core services (FTP Server): [image: ]
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Installing and configuring the routing and remote access service:[image: ]
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IP packet filtering:
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