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[bookmark: _GoBack]As the P.d. or and current increase, the gradient of the graph increases meaning that the resistance is greater. This is because as more current flows or as a greater P.d. is present the filament becomes warmer and the resistance increases.
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