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OveralFeedback _ Assessment fems.

[ExpandiColapse Al |Show Incorrect fems|

Connectiiy Tests.

Assessment tems 7 [status Ponts. Component(s) _ | Feedback
5 Network
Epe
o Defaut Gateway Correct 1 ®
o Defaut Gateway Pie Correct 1 ®
£ Ports
£ Fastethemeto
v Padiress Correct 1 ®
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
& Subnet Mask Correct 1 ®
= pe2
o Defaut Gateway Correct 1 ®
o Defaut Gateway Pie Correct 1 ®
£ Ports
£ Fastethemeto
v Padiress Correct 1 ®
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
& Subnet Mask Correct 1 ®
et
o Bamerliom™ Correct 1 Other
£ Console Line:
o Logging Synch Correct 1 Physical
o Logn Correct 1 Physical
o Password Correct 1 Other
=ons
o 1P Domain Name. Correct 1 Other
& P Domain-Lookup Correct 1 Other
o Enable Secret Correct 1 Other
o HostName Correct 1 Other
£ Ports
> Loopbackt
v Padiress Correct 1 ®
o SubnetMask Correct 1 ®
£ Loopbackz
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
"o LikLocal Correct 1 ®
£ Serao2i0
o Bandwidhinfo  Correct 1 Other
o Padiress Correct 1 ®
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
o LinkLocal Correct 1 ®
o PortStatus Correct 1 Physical
o SubnetMask Correct 1 ®

Time Elapsed: 02:01:27

Score

1820
1413
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OveralFeedback _Assessmentfems _ Connectiviy Tests.

[Expand/Colapse Al |Show Incorrect tems| Seore, senoo
tem Count 841100
Assessment fems /| statws Points. Component(s) | Feedback =
o PortStatus Correct 1 Physical Component  items/Total  Score
o Subnet Mask Correct 1 ® o 3606 3636
- Serial0r2/ Other 2505 2526
o Bandwidth info Correct 1 Other Physical 1920 1920
& ClockRate Correct 1 Physical Routing e 141e
o/ Paddress Correct 1 o
= PG Addresses 0 Other
- PvB Address 1 o 1)
‘o PAddress  Correct 1 o
e LinkLocal Correct 1 o
o PortStatus Correct 1 Physical
"o SubnetMask Correct 1 L)
= Routes
- Static Routes.
o Routed Correct 1 Routing
o Routet Correct 1 Routing
- Routesve
o 6 UnicastRouting  Correct 1 Routing
- Static Routes.
o Routed Correct 1 Routing
o Routet Correct 1 Routing
& Service Password Encryption Correct 1 Other
- User Names o Other
X Usemame Incorrect 1 Other
- VTY Lines.
B VTY Line 0
o Login Correct 1 Physical
o Password Correct 1 Other
"o Transport Input Correct 1 Physical
=R
& Banner HOTD Correct 1 Other
- Console Line.
& Logging Synch Correct 1 Physical
o Login Correct 1 Physical
o Password Correct 1 Other
=DNS o Other
"o/ P Domain-Lookup Correct 1 Other
& Enable Secret Correct 1 Other
o Host Name Correct 1 Other
- Ports.
- GigabitEthernet0/0/0
o/ Paddress Correct 1 o
= PG Addresses 0 Other
- PvB Address 1 o 1)
‘o PAddress  Correct 1 o
e LinkLocal Correct 1 o
o PortStatus Correct 1 Physical
- Seril0/in
o Bandwidth info Correct 1 Other
X ClockRate Incorrect 1 Physical
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Assessment tems 7 [status Ponts. Component(s) _ | Feedback
T Enabke Secret Correct 1 Other
o HostName Correct 1 Other
& Ports
£/ Gigabithemet0/0/0
o Padiress Correct 1 ®
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
o LinkLocal Correct 1 ®
o portStatus Correct 1 Pnysical
£ Sera0i0
o Bandwidhnfo  Correct 1 Other
X ClockRate Incorrect 1 Physical
o Padiress Correct 1 ®
£ Prs Addresses o Other
5 Pyg Address 1 [ P
o Paddress Correct 1 ®
o LinkLocal Correct 1 ®
o PortStatus Correct 1 Physical
o SubnetMask Correct 1 ®
5 Routes
=5 Statc Routes.
X Routed Incorrect 1 Routing
v Routel Correct 1 Routing
v Route2 Correct 1 Routing
£ Routesve
- PvUnicastRoutng  Correct 1 Routing
=) Statc Routes.
X Routed Incorrect 1 Routing
v Routel Correct 1 Routing
v Route2 Correct 1 Routing
o Service Password Encryption Correct 1 Other
VTV Lines
VTV Line 0
o Logn Correct 1 Physical
o Password Correct 1 Other
o Transportnput  Correct 1 Physical
£
o Bamerliom Correct 1 Other
£ Console Line:
o Logging Synch Correct 1 Physical
o Logn Correct 1 Physical
o Password Correct 1 Other
o Enable Secret Correct 1 Other
o HostName Correct 1 Other
& Ports
£/ Gigabithemet0/0/0
o Padiress Correct 1 ®
£ Prs Addresses o Other
5 Prg Address 1 [ ®

Time Elapsed: 02:0205

HemsTotal  Score

T
2505 2508
1920 1920
s 1ans
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Time Elapsed: 02:0217

Score 4100
tem Count 4100

- VTY Line 0
o Logn Correct
o Password Correct
o Transportiput  Comect
& Banner HOTD Correct
Console Line
o Logging Synch Correct
o Logn Correct
o Password Correct
& Enable Secret Correct
o Hostlame Correct
Ports
£/ Gigabithemet0/0/0
o Padiress Correct
£ Prs Addresses
5 Pyg Address 1
o Paddress  Correct
o LinkLocal Correct
o PortStatus Correct
£ Seraio2it
o Bandwidhinfo  Correct
o Padiress Correct
£ Prs Addresses
5 Pyg Address 1
o Paddress Correct
o LinkLocal Correct
o PortStatus Correct
o SubnetMask Correct
Routes.
=5 Statc Routes.
X Routed Incorrect
v Routel Correct
v Route2 Correct
Routesvs.
=) Statc Routes.
X Routed Incorrect
v Routel Correct
v Route2 Correct

& Service Password Encryption Correct
VTV Lines

VTV Line 0
v Logn Correct
o Password Correct

o Transportnput  Correct
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Assessment tems 7 [status Ponts. Component(s) _ | Feedback
T Rautel Correct Routing
o Route2 Correct Routing
Other

® 08
Other 2508

1820
Routing 1418

Score

1820
1413





