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 1905836
s1#sho run
Building configuration...

Current configuration : 1456 bytes
!
! Last configuration change at 22:46:21 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname s1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 153.99.11.10 255.255.255.0
!
ip default-gateway 153.99.11.1
ip http server
ip http secure-server
!
no vstack
banner motd ^Cunathorised access^C
!
line con 0
line vty 0 4
 password cisco
 login
line vty 5 15
 password cisco
 login
!
end

s1#
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% Invalid input detected at '^' marker.

R1>en
Password:
Password:
R1#show run
Building configuration...


Current configuration : 3562 bytes
!
! Last configuration change at 12:48:09 UTC Tue Jan 14 2020
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
[bookmark: _GoBack]platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$Wzsz$/k8GCZo9V0HKWihbACmYV1
!
no aaa new-model
!
no ip domain lookup
 --More—
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Microsoft Windows [Version 16.6.18362.418] ~
(c) 2019 Microsoft Corporation. All rights reserved.

:\Users\Admin>ipconfig/all
windows TP Configuration

Host Name .
Primary Dns Suffix’
Node Type . . .

Ip Routing Enabled.
WINS Proxy Enabled.

Ethernet adapter VirtualBox Host-Only Network:

Connection-specific DNS Suffix
Description . . . . . .. ... .: VirtualBox Host-Only Ethernet Adapter
Physical Address. ©A-00-27-00-00-11

DHCP Enabled. .
Autoconfiguration Enabled .
Link-local IPv6 Address . 9e5:2167:8FFd: bfc6%17 (Preferred)
1Pv4 Address. © . ... ... :192.168.56.1(Preferred)

Subnet Mask . . . . . .. ....: 255.255.255.6

Default Gateway .
DHCPYV6 TATD . © ... ... .: 420085799

DHCPV6 Client DUID. . . . . . . . : ©0-1-60-61-25-60-28-D8-0C-9D-92-BF-BA-80

DNS Servers . 1%
2%
Fece:0:0: FFFF::3%1
NetBIOS over Tcpip. . . . . . . . : Enabled
Ethernet adapter Npcap Loopback Adapter:
Connection-specific DNS Suffix
Description . . . . . . ... ..: Npcap Loopback Adapter
Physical Address. 02-00-4C-4F-4F-50

DHCP Enabled. St Yes
Autoconfiguration Enabled . . . . : Yes

Link-local IPv6 Address . £6d6:€b76:d171:61ca%9 (Preferred)
Autoconfiguration Ipv4 Address. 169.254.97.262(Preferred)

Subnet Mask . . . . . . . ....: 255.255.0.0

Default Gateway .
DHCPYV6 TATD .
DHCPV6 Client DUID.

671219788
: 00-01-00-01-25-60-28-D8-0C-9D-92-BF -BA-80 v
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Ethernet adapter Npcap Loopback Adapter:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. S
Autoconfiguration Enabled .
Link-local IPv6 Address .

Autoconfiguration IPv4 Address.

Subnet Mask .
Default Gateway .
DHCPYV6 TATD . .
DHCPYV6 Client DUID.
DNS Servers .

NetBIOS over Tcpip.
Ethernet adapter Ethernet:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. S
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

C:\Users\Admins,

: Npcap Loopback Adapter
02-00-4C-4F-4F-50

Yes
Yes
Fego: :f0d6:eb76:d171:61ca%9 (Preferred)
169.254.97.262(Preferred)
: 255.255.0.6
671210788
: 60-61-00-01-25-66-28-D8-6C-9D-92-BF-BA-80
1%
2%
Fece:0:0: FFFF::3%1

: Enabled

: Intel(R) Ethernet Connection (2) 1219-LM
8C-9D-92-BF-BA-80

4125:42a8:57F3:9d82%8 (Preferred)
.99.11.254(Preferred)
: 255.255.255.8

153.99.11.1
101490666
: 60-61-00-01-25-66-28-D8-6C-0D-92-BF-BA-80
1%

fecB:0:0:FFFF::3%1
: Enabled
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