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6. Encrypt all the passwords in all the routers

7. Set motd banner: & unauthorized access prohibited & for all the Routers. Note, use special character & to begin and end the banner as

stated in the red, underlined text.

Part - B Route Configuration

8. Configure all devices with 1P address as shown in the Addressing table and network topology. Configure both 1Pv4 and IPv6 address. For
1Pv6 address, configure appropriate Link Local address manually

9..0n R1, configure IPv4 and IPV6 static route to R2 and R3 networks
10. On R2, configure IPv4 and IPV6 static route to R3 networks

11. On R3, configure IPv4 and IPV6 static router to R2 networks.

12. Configure IPv4 and IPV6 default static route on R2 and R3 to reach Lol and Lo2 network using next-hop ip address.
13. Set the bandwidth on serial links to 512kbps.

14. Set the clock rate on DCE to be 9600

15. In R1, create a domain with name acca.com, username: user1 and encrypted password: password. Set privelge as 10.

Part - C Network Connectivity

Using ping command, verify end-to-end connectivity for both IPv4 and TPV6 networks:

16. From PC1,

g PC2
17. From PC1, ping Lot and Lo2.

22. From PC2, ping Lot and Lo2.

Verify Telnet Connectivity

23. From PC1, establish telnet connection to R1. (Should be successful)
24. From PC2, establish SSH connection to R1. (Should Fail)
Submission Requirement

The packet tracer file should be saved as “studentname_id” and uploaded onto Moodle.

In addition to packet tracer file, you must also submit the following
screenshot in a word document clearly displaying your completed percentage and Assessment Items
the output of show running-configuration command in a text file for all devices configured

All documentation for your solution should be submitted electronically on Moodle. It is your responsi
and files correctly.

y that you submit all the outputs

End of Task!!!
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You did not complete the activity. Please close this window and try again.

OveralFeedback _Assessmentfems _ Connectiviy Tests.

[ExpandiColapse Al |Show Incorrect fems|

Assessment tems 7 [status Ponts. Component(s) _ | Feedback
5 Network
Epe
o Defaut Gateway Correct 1 ®
o Defaut Gateway Pie Correct 1 ®
£ Ports
- FastEthernetd

§§§'§ i

Time Elapsed: 02:13:15.

51100
51100

1413

Score

1820
1413




