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Router>enable
Router#configure terminal
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#host name R1
                         ^
% Invalid input detected at '^' marker.

Router(config)#^Z
Router#
*Sep  2 20:34:08.424: %SYS-5-CONFIG_I: Configured from console by consoleho













% Bad IP address or host name% Unknown command or computer name, or unable to find computer address
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#
Router#g
 iox feature is not enabled
Router#
Router#
Router#
Router#host name R1
        ^
% Invalid input detected at '^' marker.

Router#host name R1
        ^
% Invalid input detected at '^' marker.

Router#configure terminal
Enter configuration commands, one per line.  End with CNTL/Z.
Router(config)#host name R1
                         ^
% Invalid input detected at '^' marker.

Router(config)#hostname R1
R1(config)#no ip domain-look up
                             ^
% Invalid input detected at '^' marker.

R1(config)#no ip domain-loo up
                            ^
% Invalid input detected at '^' marker.

R1(config)#no ip domain-look up
                             ^
% Invalid input detected at '^' marker.

R1(config)#no ip domain-lookup
R1(config)#line vty 0 15
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#exit
R1(config)#line con 0
R1(config-line)#password cisco
R1(config-line)#login
R1(config-line)#exit
R1(config)#service password-encryption
R1(config)#banner motd # no unauthorized access #
R1(config)#configure te
                   ^
% Invalid input detected at '^' marker.

R1(config)#enterface gi
R1(config)#enterface gi
R1(config)#enterface gig
R1(config)#interface gi
R1(config)#interface gigabitEthernet 0/0/0
R1(config-if)#ip 153.99.10.1 255.255.255.0
                 ^
% Invalid input detected at '^' marker.

R1(config-if)#i paddress 153.99.10.1 255.255.255.0
                 ^
% Invalid input detected at '^' marker.

R1(config)#ip address 153.99.10.1 255.255.255.0
                     ^
% Invalid input detected at '^' marker.

R1(config)#ip address 153.99.10.1 255.255.255.0
                     ^
% Invalid input detected at '^' marker.

R1(config)#configure gig
R1(config)#configure gig
R1(config)#configure gigexit
                   ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#
*Sep  2 20:42:32.288: %SYS-5-CONFIG_I: Configured from console by consoleconf
Configuring from terminal, memory, or network [terminal]? #
?Must be "terminal", "memory" or "network"
R1#conf t
Enter configuration commands, one per line.  End with CNTL/Z.
R1(config)#inter
R1(config)#interface gig
R1(config)#interface gigabitEthernet 0/0/0
R1(config-if)#ip address 153.99.10.1 255.255.2550
                                                ^
% Invalid input detected at '^' marker.

R1(config-if)#ip address 153.99.10.1 255.255.255.0
R1(config-if)#exit
R1(config)#interface gig
R1(config)#interface gigabitEthernet 0/0/1
R1(config-if)#ip address 153.99.11.1 255.255.255.0
R1(config-if)#exit
R1(config)#show running-configuration
             ^
% Invalid input detected at '^' marker.

R1(config)#show running-configuration
             ^
% Invalid input detected at '^' marker.

R1(config)#exit
R1#sh
*Sep  2 20:44:46.991: %SYS-5-CONFIG_I: Configured from console by consoleow run
Building configuration...


Current configuration : 3508 bytes
!
! Last configuration change at 20:44:46 UTC Mon Sep 2 2013
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1783363698
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1783363698
 revocation-check none
 rsakeypair TP-self-signed-1783363698
!
!
crypto pki certificate chain TP-self-signed-1783363698
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31373833 33363336 3938301E 170D3133 30393032 31393433
  35365A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 37383333
  36333639 38308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100B274 9195AEAB 6339F727 F093A3EF 872B9D6D 0680E073 11C8C1CB
  EB6E5B0B FC22CCA3 1464ECCD 32B2367A 00B36A88 A0E8AF2E 3855F492 4381F742
  0813B36C 67AB1F42 3ED56890 91B04D97 D4B9770F B49CE360 67E2915E 05FC695C
  B61A1A6F E2B7CE65 2F9D39F7 6AB72455 EB71B163 A1E137F3 6C84C0E3 93D72427
  88E51CC7 9AC00D7F 1DB58716 B308A6D5 04301411 48929A00 04973B40 FE137AFD
  142A1382 4CCD2A66 8E567828 176D7D10 840D3839 01170C19 93C27B6D 3782EC05
  68085CFB 89BE1B33 AFACA67E 3C8BFEE4 8BD58603 21BACC45 A5E2D1CC 012EEF19
  A3BF48D4 0AAC2A54 21D5F57A 2043D357 661988AE 93F18FE0 305AF640 E60D0502
  CC348842 2A990203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 146CE604 815A0D49 43E4AE49 698468CC 09BACF38
  4D301D06 03551D0E 04160414 6CE60481 5A0D4943 E4AE4969 8468CC09 BACF384D
  300D0609 2A864886 F70D0101 05050003 82010100 2240FD50 78C639B1 39604C9D
  D40D5C3C 6B62EF5B 01124B31 D43EECC5 5E515649 059605D8 7C0B897B 156C24DF
  7C567AB3 6A049641 A6418194 925E185C E54E2AE6 F8C3BD05 F9E16B2E 1E9753B4
  A0B4B3D6 3430E82E 859BD3DD C0DFBFFF F1BD167F 1E8C66F0 CBE54942 BD09EBFC
  523D6599
E1917 BF41C648 BD9542F4 3B9B4A33 96B7A781 18DD4434 792430FC A0C770E7
  ACE4EDCB 7E64DFF0 A2AB57E5 E60A35BF EC6F8085
        quit
!
license udi pid ISR4221/K9 sn FGL2235928E
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 ip address 153.99.10.1 255.255.255.0
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 ip address 153.99.11.1 255.255.255.0
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^C no unauthorized access ^C
!
line con 0
 password 7 094F471A1A0A
 login
 transport input none
 stopbits 1
line vty 0 4
 password 7 094F471A1A0A
 login
line vty 5 15
 password 7 094F471A1A0A
 login
!
!
!
!
!
!
end
