R1:

R1>
R1>enable
R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#password letmein#
^
% Invalid input detected at '^' marker.
R1(config)#password letmein
^
% Invalid input detected at '^' marker.
R1(config)#line console 0
R1(config-line)#password letmein
R1(config-line)#login
R1(config-line)#exit
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#exit









R1 con0 is now available






Press RETURN to get started.













User Access Verification

Password: 

R1>enable
R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#babenable password cisco
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#enable secret itsasecret
^
% Invalid input detected at '^' marker.
R1#
R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#enable itsasecret
^
% Invalid input detected at '^' marker.
R1(config)#enable secret itsasecret
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#service password-encryption
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#banner motd "This is a secure system. Authoruzed Access Only!"
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#config t 
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#ip address 185.95.1.1 255.255.255.0
^
% Invalid input detected at '^' marker.
R1(config)#ipiinterface FastEthernet 0/0
R1(config-if)#ip address 185.95.1.1 255.255.255.0
R1(config-if)#no shutdown

R1(config-if)#
%LINK-5-CHANGED: Interface FastEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/0, changed state to up

R1(config-if)#exit
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#copy running-config startup-config
Destination filename [startup-config]? 
Building configuration...
[OK]
R1#
R1#
R1#configure terminal
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#router rip
R1(config-router)#




R2:
Router#config t
Enter configuration commands, one per line. End with CNTL/Z.
Router(config)#hostname R2
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#config t
Enter configuration commands, one per line. End with CNTL/Z.
R2(config)#router rip
R2(config-router)#no auto-summary
R2(config-router)#network 185.95.2.1
R2(config-router)#network 185.95.2.1
R2(config-router)#interface FastEthernet 0/0
R2(config-if)#exit
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#copy running-config startup-config
Destination filename [startup-config]? 
Building configuration...
[OK]
R2#
R2#








R2 con0 is now available






Press RETURN to get started.













R2>enable
R2#config t 
Enter configuration commands, one per line. End with CNTL/Z.
R2(config)#line console
% Incomplete command.
R2(config)#line console 0
R2(config-line)#password letmein
R2(config-line)#login
R2(config-line)#exit
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#config t
Enter configuration commands, one per line. End with CNTL/Z.
R2(config)#enable password cisco
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console
exit









R2 con0 is now available






Press RETURN to get started.













User Access Verification

Password: 

R2>enable
Password: 
R2#config t
Enter configuration commands, one per line. End with CNTL/Z.
R2(config)#banner motd "This is a secure system. Authorized Access Only!"
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#config t
Enter configuration commands, one per line. End with CNTL/Z.
R2(config)#interface FastEthernet 0/0
R2(config-if)#ip address 185.95.2.1 255.255.255.0
R2(config-if)#no shutdown

R2(config-if)#
%LINK-5-CHANGED: Interface FastEthernet0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/0, changed state to up

R2(config-if)#exit
R2(config)#exit
R2#
%SYS-5-CONFIG_I: Configured from console by console

R2#copy running-config startup-config
Destination filename [startup-config]? 
Building configuration...
[OK]
R2#
R2#



R3:
Router>
Router>enable
Router#config t
Enter configuration commands, one per line. End with CNTL/Z.
Router(config)#hostname R3
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console
exit









R3 con0 is now available






Press RETURN to get started.













R3>enable
R3#rconfig t
Enter configuration commands, one per line. End with CNTL/Z.
R3(config)#router rip
R3(config-router)#verdion 2
^
% Invalid input detected at '^' marker.
R3(config-router)#version 2
R3(config-router)#no auto-summary
R3(config-router)#network 185.95.3.1
R3(config-router)#network 185.95.3.1
R3(config-router)#interface FastEthernet 0/0
R3(config-if)#exit
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#copy running-config startup-config
Destination filename [startup-config]? 
Building configuration...
[OK]
R3#
R3#








R3 con0 is now available






Press RETURN to get started.













R3>enable
R3#config nt
^
% Invalid input detected at '^' marker.
R3#config t
Enter configuration commands, one per line. End with CNTL/Z.
R3(config)#line console 0
R3(config-line)#password letmein
R3(config-line)#login
R3(config-line)#exit
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#config t
Enter configuration commands, one per line. End with CNTL/Z.
R3(config)#enable password cisco
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#config t
Enter configuration commands, one per line. End with CNTL/Z.
R3(config)#banner motd "This is a secure system. Authorized Access Only!"
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#config t 
Enter configuration commands, one per line. End with CNTL/Z.
R3(config)#interface FastEthernet 0/0
R3(config-if)#ip address 185.95.3.1 255.255.255.0
R3(config-if)#no shutdown

R3(config-if)#
%LINK-5-CHANGED: Interface FastEthernet0/0, changed state to up

R3(config-if)#exit
R3(config)#exit
R3#
%SYS-5-CONFIG_I: Configured from console by console

R3#copy running-config startup-config
Destination filename [startup-config]? 
Building configuration...
[OK]
R3#
R3#
%LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/0, changed state to up









R3 con0 is now available






Press RETURN to get started.
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Packet Tracer BC Command Line 1.0
e\

C:\>ping all

Ping request could not find host all. Please check the name and try again.
C:\>ping 185.55.1.1

Pinging 185.55.1.1 with 32 byres of data:

Reply from 185.55.1.1: bytes=32 time<lms TTL=255
Reply from 185.55.1.1: bytes=32 time<lms ITL=255
Reply from 185.55.1.1: bytes=32 time<lms ITL=255
Reply from 185.55.1.1: bytes=32 time<lms TTL=255

Ping stavistics for 185.95.1.
Packets: Senc = 4, Received = 4, Lost = 0 (08 loss),
Approximate round trip vimes in milli-seconds:
Minimm = Ons, Maximm = Oms, Average = Oms
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Packet Tracer BC Command Line 1.0
Co\sping 185,55 2.1

Pinging 185.55.2.1 with 32 byves of daca:

Reply from 185.55.2.1: byses=32 vime<lms TTL=255
Reply from 185.55.2.1: byses=32 vime<lms TTL=255
Reply from 185.55.2.1: byses=32 vime<lms TTL=255
Reply from 185.95.2.1: byves=32 vime<lms TTL=255

Bing stavisvics for 185.95.2.1
Packecs: Senc = 4, Received Tost = 0 (08 loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = Ons, Maximm = Oms, Average = Oms
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Packet Tracer PC Command Line 1.0
Co\sping 185,55 3.1

Pinging 185.55.3.1 with 32 byres of data:

2 vime<lms TTL=255
2 vime<lms TTL-255
2 vime<lms TTL-255
2 vime<lms TTL=255

Reply from 185.55.3.1: byce:
Reply from 185.95.3.1: byces:
Reply from 185.55.3.1: byce:
Reply from 185.55.3.1: byves=:

Ping scavistics for 185.95.3.1:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),





