Name of the IOS image that the router is running? 
Non-volatile random-access memory (NVRAM) does the router have? 
How much Flash memory does the router have? What is the boot process for the router on the next reload?
 How are passwords presented in the output? 
What code is used in the routing table to indicate a directly connected network? 
C or L
How many route entries are coded with a C code in the routing table? 
0/0 0/1
What command changed the status of the Gigabit Ethernet ports from administratively down to up?
No shutdown
