Router 1: 
#show run

Building configuration...

Current configuration : 1263 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524BS86-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.1 255.255.255.252
clock rate 2000000
!
interface Serial0/0/1
ip address 185.95.13.1 255.255.255.252
clock rate 2000000
!
interface Serial0/1/0
no ip address
clock rate 2000000
shutdown
!
interface Serial0/1/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 1.1.1.1
log-adjacency-changes
passive-interface default
auto-cost reference-bandwidth 1000
neighbor 185.95.1.1
!
ip default-gateway 185.95.1.1
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a private network! Unauthorized access will be prohibited!!!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
End

#show ip int brief
show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.1.1 YES NVRAM up up 
GigabitEthernet0/1 unassigned YES NVRAM administratively down down 
GigabitEthernet0/2 unassigned YES NVRAM administratively down down 
Serial0/0/0 185.95.12.1 YES NVRAM up up 
Serial0/0/1 185.95.13.1 YES NVRAM up up 
Serial0/1/0 unassigned YES NVRAM administratively down down 
Serial0/1/1 unassigned YES NVRAM administratively down down 
Vlan1 unassigned YES NVRAM administratively down down
#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.1.0/24 is directly connected, GigabitEthernet0/0
L 185.95.1.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.1/32 is directly connected, Serial0/0/0
C 185.95.13.0/30 is directly connected, Serial0/0/1
L 185.95.13.1/32 is directly connected, Serial0/0/1
#show ip ospf neighbour 

#show ip ospf database 
Routing Process "ospf 1" with ID 1.1.1.1
Supports only single TOS(TOS0) routes
Supports opaque LSA
SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
Number of external LSA 0. Checksum Sum 0x000000
Number of opaque AS LSA 0. Checksum Sum 0x000000
Number of DCbitless external and opaque AS LSA 0
Number of DoNotAge external and opaque AS LSA 0
Number of areas in this router is 0. 0 normal 0 stub 0 nssa
External flood list length 0

Router 2: 
#show run
Building configuration...

Current configuration : 1172 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524B158-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.2.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.1 255.255.255.252
!
interface Serial0/1/0
no ip address
clock rate 2000000
shutdown
!
interface Serial0/1/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 2.2.2.2
log-adjacency-changes
passive-interface default
auto-cost reference-bandwidth 1000
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a private network! Unauthorized access will be prohibited!!!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
End

#show ip int brief

Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.2.1 YES NVRAM up up 
GigabitEthernet0/1 unassigned YES NVRAM administratively down down 
GigabitEthernet0/2 unassigned YES NVRAM administratively down down 
Serial0/0/0 185.95.12.2 YES NVRAM up up 
Serial0/0/1 185.95.23.1 YES NVRAM up up 
Serial0/1/0 unassigned YES NVRAM administratively down down 
Serial0/1/1 unassigned YES NVRAM administratively down down 
Vlan1 unassigned YES NVRAM administratively down down
#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.2.0/24 is directly connected, GigabitEthernet0/0
L 185.95.2.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.1/32 is directly connected, Serial0/0/1
#show ip ospf neighbor
#show ip ospf database
Routing Process "ospf 1" with ID 2.2.2.2
Supports only single TOS(TOS0) routes
Supports opaque LSA
SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
Number of external LSA 0. Checksum Sum 0x000000
Number of opaque AS LSA 0. Checksum Sum 0x000000
Number of DCbitless external and opaque AS LSA 0
Number of DoNotAge external and opaque AS LSA 0
Number of areas in this router is 0. 0 normal 0 stub 0 nssa
External flood list length 0
Router 3: 
#show run
R3#show run
Building configuration...

Current configuration : 1192 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15245LNV-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.3.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.13.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.2 255.255.255.252
clock rate 2000000
!
interface Serial0/1/0
no ip address
clock rate 2000000
shutdown
!
interface Serial0/1/1
no ip address
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 3.3.3.3
log-adjacency-changes
passive-interface default
auto-cost reference-bandwidth 1000
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a private network! Unauthorized access will be prohibited!!!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end
#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.3.1 YES NVRAM up up 
GigabitEthernet0/1 unassigned YES NVRAM administratively down down 
GigabitEthernet0/2 unassigned YES NVRAM administratively down down 
Serial0/0/0 185.95.13.2 YES NVRAM up up 
Serial0/0/1 185.95.23.2 YES NVRAM up up 
Serial0/1/0 unassigned YES NVRAM administratively down down 
Serial0/1/1 unassigned YES NVRAM administratively down down 
Vlan1 unassigned YES NVRAM administratively down down
#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.3.0/24 is directly connected, GigabitEthernet0/0
L 185.95.3.1/32 is directly connected, GigabitEthernet0/0
C 185.95.13.0/30 is directly connected, Serial0/0/0
L 185.95.13.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.2/32 is directly connected, Serial0/0/1

#show ip ospf neighbor
#show ip ospf database
Routing Process "ospf 1" with ID 3.3.3.3
Supports only single TOS(TOS0) routes
Supports opaque LSA
SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
Number of external LSA 0. Checksum Sum 0x000000
Number of opaque AS LSA 0. Checksum Sum 0x000000
Number of DCbitless external and opaque AS LSA 0
Number of DoNotAge external and opaque AS LSA 0
Number of areas in this router is 0. 0 normal 0 stub 0 nssa
External flood list length 0
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