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©) Enable LLDP globally on R2.

d) OnR2, configure the link to 2 to only receive LLDP messages.

©) Disable CDP on S2

§) Enable LLDP globally on S2.

) On'S2 switch, configure the link to R2 router to only send, not receive, LLDP
‘messages

1) Disable LLDP completely on access port fa 0/18 that is in use.

Submission Requirement
The packet tracer file should be saved as “studentname_id” and uploaded onto Moodle.

In addition to packet tracer file, you must also submit the following
i) screenshot in a word document clearly displaying your completed percentage and
Assessment Items. Sample is shown below. The screenshot must include Full screen
including the File name at Top and system time in Bottom.
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