


Swansea Network

1. Create a forest named yourname.acca (For example: nitheesh.acca)
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2. Join the ClientS1 to yourname.acca domain.
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Preferred DNS Server is set up for Windows 2022 Server.















3. Configure DHCP Services. The range is 172.16.1.10 – 172.16.1.20. Determine other DHCP options as per the infrastructure.
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4. Assign ClientS1 with DHCP IP Address. 















5. Install Routing and Remote access Service and modify firewall rules to allow ICMP Traffic.
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6. Create a reverse lookup zone creating PTR records for all servers.
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7. Create user accounts for yourname.acca domain with all the parameters defined in the users_list_updated.xlsx document. This document will be shared by your lecturer. You must use first letter from first name with a dot and last name as SAM Account Name. Eg: First Name: Nitheesh Last Name: Kaliyamurthy.  n.kaliyamurthy.
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8. Mount second disk drive to D:\SwanseaFiles. 
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9. Configure Site-to-Site VPN to London Network. Set the connection type to “persistent connection”.
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10. Create all appropriate A records for all servers on 10.1.1.0/24 and 172.16.1.0/24. – 
















1. In Cardiff Network, 
1.1. Install Routing and Remote access Service (equivalent) and modify firewall rules to allow ICMP Traffic.
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1.2. Configure Site-to-Site VPN to Swansea Network. Set the connection type to “persistent connection”.
[image: ]
1.3. Create a child domain named car.yourname.acca in yourname.acca tree (Eg: car.nitheesh.acca) or Join devices in this network to the yourname.acca domain. Justify your action.
1.4. Configure DHCP Services. The range is 10.1.1.10 – 10.1.1.20. Determine other DHCP options as per the infrastructure.
1.5. Depending on step no. 2.3, join the ClientC1 to appropriate domain and assign DHCP IP address.

2. Test the network for Connectivity. Note that at this stage, the Swansea and Cardiff networks are connected and fully operational. If not, Troubleshoot.

(From No. 4, you need to complete on your own. This is designed to reflect on your knowledge, understanding and cognitive skills)

3. Sharing Disk Drive: To the earlier created D:\SwanseaFiles, set access permissions to allow users in the users_list_updated.xlsx has full control permissions and other network users have only read access. Share the drive to both Cardiff and Swansea network.
4. Configure IIS Server
4.1. Create https://webs. yourname.acca website and enable windows internal authentication. 
4.2. All the users can be authenticated.
4.3. All authenticated users should be presented a text “Welcome to Swansea Website”.
5. Remote Desktop Services: Configure remote access for S-DC from any other machines in the network. Make sure that the Remote Desktop Services login page should be accessed via https://rds.yourname.acca and necessary certificates are signed.
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