Labs4Second Attempt
Convert the following from binary to IP Addresses 
PC0 NIC 11000000.10101000.01001000.00011110 /24
PC1 NIC 11000000.10101000.01001000.00101000 /24
PC3 NIC 11000000.10101000.01001000.00110010 /24
PC4 NIC 11000000.10101000.01001000.01000110 /24
Conversions 

PC0 NIC 192.168.72.30 /24
PC1 NIC 192.168.72.40 /24
PC3 NIC 192.168.72.50 /24
PC4 NIC 192.168.72.60 /24

Changing the hostname of the switch:
[image: ]
Configuring the console password: 
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Configuring the vty password: 
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Enabling the Privileged password:
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!
Running Configuration
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The privileged password is shown in the running configuration and it is displayed as 0822455D0A16.

Show the IP Address:
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PDU information for the Switch.3, you can see the Source and Target IP has been changed and 
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switch(config) #interface vlan 1
Switch(config-if) #ip address 192.168.72.254 255.255.255.0
switch(config-if) #no shut

switch(config-if) #exit
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PDU Information at Device: Switch3

OSI Model Outbound PDU Details
I

PDU Formats

Elhemeﬂl

HARDWARE TYPE:0x0001 PROTOCOL TYPE:0x0800

HLEN:0x06 PLEN:0x04 ‘OPCODE:0x0001

SOURCE MAC :000C 85C3 64B6

SOURCE IP :192.168.72.254

TARGET MAC:0000.0000.0000

TARGET IP:192.168 72 254
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Switch>enable
switch#configure terminal

Enter configuration commands, one per line. End with CNTL/Z.
Switch (config) #hostname SwIMyFirstSwitch
SwIMyFirstswitch(config)#no hostname

Switch (config) #hostname Ashleigh

Ashleigh(config) #exit

Ashleight

$SYS-5-CONFIG_I: Configured from console by console

Ashleighfexit
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Ashleigh>enable

Ashleighfconfig terminal

Enter configuration commands, one per line.
Ashleigh(config)#line console 0
Ashleigh(config-line)#password ciscol23
Ashleigh(config-line)#login
Ashleigh(config-line)#exit

End with CNTL/Z.
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Ashleigh(config) #line vty 0 15
Ashleigh(config-line) #password 1Cisc3
Ashleigh(config-line)#login
Ashleigh(config-line)#exit




image4.png
Ashleigh(config) #Enable password cisco
Ashleigh(config)#
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Switch#show running-config
Building configuration...

Current configuration : 1249 bytes

version 12.2

no service timestamps log datetime msec
no service timestamps debug datetime msec
service password-encryption

'

hostname Switch

enable secret 5 $1SmERr$hxS5rVt7rPNoS4wgbXEXTmO
enable password 7 0822455D0A16

spanning-tree mode pvst
spanning-tree extend system-id

—-More-—-—
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interface FastEthernet0/23

interface FastEthernet0/24
'

interface GigabitEthernet0/1

interface GigabitEthernet0/2

interface Vlanl
no ip address
shutdown

line con 0

password 7 0822455D0A16544541
login

'

line vty 0 ¢

password 7 08706F473A1A56
login

line vty 5 15

password 7 08706F473A1A56
login

end




