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Objective
The objective of this project is to design, test and manufacture a microcontroller based system that can;
· Measure the level of moisture in the soil
· Dispense water to correct the moisture levels in the soil
· Use Solar power and a helio-stat to maximise energy collection
· Contain a water collection system and sensors to detect how much water is available for the system to use – before it uses water from the home. 
Additionally, a design will be made for domestic and industrial settings which a difference of features and cost to suit the consumers for different applications on small and large scale.
Problem and solution
A huge percentage of plants that are grown end up dying due to a lack or a surplus of water, in the form of the soil moisture percentage. This is a huge problem that is not yet widely recognised, as forecasts for the future predict mass food shortages due to a lack of water availability worldwide. A warning of this was the droughts that the USA experienced in 2012, where a 26% decrease in maize yield occurred leaving people struggling for food [1]. Worryingly, this was not a one off occurrence and it is projected that the failure rate of maize growth will rise by “4.5 times by 2030 and up to 25 times higher by 2050” [2].
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Figure 1
Figure 1 shows the massive increase in rice failure across Asia in the years 2021,2030 and 2050. This could lead to huge worldwide food shortages and is widely regarded as inevitable by researchers unless changes are made both regarding water use, successful crop yield percentages and the CO2 emissions worldwide.
My solution to this global issue is to design and manufacture a system that controls the water intake of plants, ensuring that they remain at an optimal level to massively increase the crop yield for both domestic and industrial use in the future. Did you know that agriculture uses approximately 65% of the worlds total fresh water intake each year?
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Figure 2

Schroders research concludes that 45% of the water used by agriculture is wasted through poor irrigation systems, this is an unbelievable 2.66 trillion cubic meters of water each year being used with 1.2 trillion cubic meters of water being wasted each year. That is an astronomical number which could be massively reduced to repurpose this water for more productive purposes for human consumption, or to increase crop yield worldwide. Schroders research also concludes that agricultural crop yields double where irrigation systems are used, leaving a massive expanse for innovation and development within the crop irrigation industry.
The system that this project will be dedicated to will be a domestic implementation of an automatic irrigation system with the aim to expand on the design in the future to produce a more efficient, large scale system to control the water flow for farms and mass crop producers, in order to both reduce water consumption, produce energy in an eco friendly way, and finally to increase the health and yield percentage of the crops. 
This system will be constructed using a few main components;
It will use three microcontrollers that will use I2C to communicate to one another, with a central microcontroller controlling the operation of the system. Firstly, a solar panel will be used to power the circuit, potentially using a heliostat to track the suns rays and maximise its efficiency, this power will then be used for the circuit. The main function of the system is to measure the soil moisture level and react upon that basis, deciding weather to turn on the irrigation system, and for what duration of time to correct the levels for optimal plant growth. This will utilise two probes placed in the soil which will send and receive a signal, the strength of this signal will alternate depending on the moisture level in the soil as it will become stronger as more water is present. This then needs to be tested and carefully calibrated to make it an effective system. Research shows that most plants have a range of around 20% that is their optimal moisture level, so a resolution of around 5% could be acceptable to maintain within the boundary, however for future designs and improvements the aim will be 2% or lower.
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Figure 3
Figure 3 shows a basic concept drawing of the design including the water tank that will have built in sensors allowing the microcontroller to detect the amount of stored water in order to decide weather it should use the collected rain water, or the water connected via a hose attachment from a house or tap. This small feature will reduce the water usage of the system slightly, however across a large scale this would make a noticeable difference.
The irrigation aspect of the design will be simple, using industrial irrigation systems as inspiration. A hose or pipe will be installed across a frame that stands above the crops, this pipe will have holes in increments at different angles to ensure an even spread of water falls onto the crops when it is turned on, simulating natural rainfall over the bed of crops. For larger crop patches, multiple pipes could be used, or a single hose in a snaking formation across the entirety of the crop bed. 


To summarise the design, the key features are;
· Microcontrollers to receive signals and control the hardware
· Solar panel to power the device
· Water collection system with sensors
· Probes to continuously measure the soil moisture levels
· Irrigation system to simulate rainfall onto the crops
· A control system for the user to input the crop and its optimal settings, also to display key information such as the soil moisture, the temperature, the power level and time
A future scaled up design could incorporate a roof or cover that is able to be opened and closed by the microcontroller depending on the soil moisture, as some plants die from drowning. The rainfall on the closed roof could then be collected and re-distributed amongst the plants when needed, effectively creating the optimal conditions for plan growth on a large scale. This would drastically improve the crop quality and yield for the farmers, helping to lower food costs and create a surplus in areas to allow for food donations to areas of need, being the homeless, areas affected by famine or even areas of conflict where it is difficult to obtain food. 

Methodology
This is a large scale project that will take a number of months to complete to ensure an high level, efficient system is designed, thoroughly tested and completed to a high standard. The Gantt Chart shown in Figure 4 details the process of designing, testing and manufacturing the process across a span of 28 weeks. 
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Figure 4 [4]
As shown in Figure 4, the initial plan for the project is to complete it within a 28 week period. This is made easier by using the Gantt chart to dedicate time to each major task that needs to be competed. These tasks can be separated into 6 main categories that are colour coded in the chart. The largest aspects of the project will span a number of weeks, with research, circuit and physical design, construction and finally testing having the bulk of the time allocated throughout the project period.
Goals & Key Performance Indicators
It is crucial to be able to measure thew success of the project through the means of setting goals and key performance indicators that can be compared with the final results to determine how successful the project was, what went well and what could be improved in the future. It is important to set goals that are ambitious, yet achievable, therefore the three KPI’s that have been set for this project increase in challenge as they progress, they are;

1. To successfully design and manufacture a fully functional system, powered by solar power, that can detect soil moisture levels and control the function of an irrigation system to correct this to a set level.

2. To successfully use the microcontroller and sensors to detect the level of rainfall that’s collected, and to use this to reduce overall water usage to grow the test crops. Reducing the water usage by 20% through the use of collected rainwater is the set goal. [5]

3. To improve the percentage of crop yield using the automated irrigation system when compared to the ‘control’ test. A percentage increase of 50% would indicate that the system is a effective however a 100% increase in crop yield is the goal set as this is the number that has been cited from Schroders research.

These goals are ambitious yet achievable, and in future designs and improvements of the system as a whole, these would be worked upon further to maximise the efficiency of the system. Saving 20% of the water used could make a huge difference to industrial farming operations, while also saving local people money on their water bill. The solar power also is essentially free for the customer and a fourth goal for the future would make the device fully sustainable in parts of the word with a high rainfall, as is experienced in the United Kingdom and Wales.
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