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Topology: 
   
Topology 1                                                   Topology 2 
LAB Objectives 
After designing the above home network, we have to configure the network and make a successful network.  
 
Topology 1: 
1. Using Windows Calculator to determine the IP address of the hosts in the network. 
2. Configure the Intermediate L2 device to the network and test the network. Troubleshoot if required. 
 
Topology 2:  
1. Configure wireless network and enhance security. 
 
Requirements 
 Use Packet Tracer to create the above recommended topology 
 
 
 
 
 
Use for reading 
Intermediate Devices: (Switch, Routers) 
The two most common methods to access the command line interface of any intermediate devices are console and SSH. For a console, a PC/ Laptop needs to be directly connected to the console port of the network device to configure. For SSH, a pre-configuration is required to access. 
Switch: Layer 2 Device 
When the switch is on, the power-on self-test (POST) begins.  
During POST, the LEDs blink while a series of tests determine that the switch is functioning properly.  
POST is completed when the SYST LED rapidly blinks green.  If the switch fails POST, the SYST LED turns amber. 
 
Memory 
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Router 
  

All routers are essentially computers. Just like computers, routers also require operating systems (OS), central processing units (CPU), random-access memory (RAM), read-only memory (ROM), and nonvolatile random-access memory (NVRAM).  
Every Cisco router has the same general hardware components, and these connections: console ports, 2 LAN interfaces, and enhanced high-speed WAN interface card (EHWIC) slots. 
  

 
 
 
 
 
 
Task 1: Switch Configurations (Use Topology 1) Create the Topology as given in Packet Tracer. 
Configure IP Address and Subnet Mask for PC0, 1, 2, 3  
	Device 
	Interface 
	IP Address 
	Subnet Mask 

	PC0 
	NIC 
	11000000.10101000.01001000.00011110 
192.168.72.30
	/24 

	PC1 
	NIC 
	11000000.10101000.01001000.00101000
192.168.72.40
 
	/24 

	PC3 
	NIC 
	11000000.10101000.01001000.00110010 
192.168.72.50
	/24 

	PC4 
	NIC 
	11000000.10101000.01001000.01000110
192.168.72.70
	/24 


 
Basic Switch Configurations 
1. User Mode, Privilege Mode, Global Configuration Mode: 
2. Give a Host Name: SwTMyFirstSwitch 
Swt1(config)#hostname SwTMyFirstSwitch 
The NO Command  
To remove a command, use “no” before the executing command Eg: no hostname 
3. Passwords (Basic Security) 
Configure console password: cisco123  
	 	 	 	>enable 
 	 	 	# Config t  	 	 	Line console 0  	 	 	password cisco123 
 	 	 	login  	 	 	Exit 
	 	 	 	# 
Configure vty password: 1CiSc3 
>enable 
 	 	 	# Config t  	 	 	Line vty 0 15  	 	 	password 1CiSc3 
 	 	 	login  	 	 	Exit 
	 	 	 	# 
Enable Privileged Password: Password 
>enable 
	 	 	 	# Config t 
	 	 	 	Enable password cisco 
 
	Observe the running configuration of your switch and note the 

	configuration 
 SwTMyFirstSwitch(config-if)#Line console 0
SwTMyFirstSwitch(config-line)#password cisco123
SwTMyFirstSwitch(config-line)#login
SwTMyFirstSwitch(config-line)#Exit
SwTMyFirstSwitch(config)#
SwTMyFirstSwitch(config)#Line vty 0 15
SwTMyFirstSwitch(config-line)#password 1CiSc3
SwTMyFirstSwitch(config-line)#login
SwTMyFirstSwitch(config-line)#Exit
SwTMyFirstSwitch(config)#Enable password cisco
SwTMyFirstSwitch(config)#
 
 
 
Is your privileged password shown in running-configuration? (Yes/No) If Yes, how is it displayed? 
 Yes shown in IOS commands
 


 
Now, remove the privileged password. To do that, go to config mode 
(Privileged Executive mode) 
	  	 	 	# Config t 
	 	 	 	No enable password cisco 
	 	 	 	And Type 
	 	 	 	enable secret cisco 
 
	Observe the running configuration of your switch again and note the 

	difference between password and secret 
 Switch(config)#line console 0
Switch(config-line)#password cisco123
Switch(config-line)#login
Switch(config-line)#exit
Switch(config)#line vty 0 15
Switch(config-line)#password 1CiSc3
Switch(config-line)#login
Switch(config-line)#exit
Switch(config)#No enable password
Switch(config)#enable secret cisco
Switch(config)#exit
Switch#
%SYS-5-CONFIG_I: Configured from console by console
 
 
How are the other passwords? 
 
 


Now, go to config mode (Privileged Executive mode) again 
# Config t 
	 	 	 	Service password-encryption 
	Observe the running configuration of your switch again and note the 

	difference now 
 Switch>Service
Translating "Service"...domain server (255.255.255.255)
 


 
The DO Command  
Allows you to execute any EXEC mode command from within any configuration mode Eg:  
# Config t 
Do show running-configuration 
4. IP Address  
SwTMyFirstSwitch > en 
SwTMyFirstSwitch # config t 
SwTMyFirstSwitch (config)#interface vlan 1 SwTMyFirstSwitch (config-if)# 
ip address 192.168.72.254 255.255.255.0 
SwTMyFirstSwitch(config-if)#no shut 
SwTMyFirstSwitch(config-if)#exit 
 
5. Show Commands 
Show running-config show interfaces show arp 
show version 
 
Erase startup-config  
Reload 
	The BANNER Display your banner banner motd " 
Enter TEXT message. End with the character '"' 
Welcome to Switch GF " 


6. Save the Configurations 
copy run startup write memory 
 

Try out!!! 
Add a router to your network and do the same configurations and record your reflections 
 
 
 
  
 

	References: 
Ipconfig - ipconfig /all - ipconfig /release and ipconfig /renew ping netstat tracert nslookup 
Understand: 
If pings to both the name and IP address are successful, but the user is still unable to access the application, then the problem most likely resides in the application on the destination host 
If neither ping is successful, then network connectivity along the path to the destination is most likely the problem 
If the ping to the default gateway is successful, the problem is not local. If the ping to the default gateway fails, the problem resides on the local network. 
A ping may fail due to the firewall on the sending or receiving device, or a router along the path blocking the pings. 


 
 
 
 
 
 
 
 
 
 
 
 
 

Task 2: Wireless Configurations (Use Topology 2) Create the topology using Cisco packet Tracer. 
In your wireless router (WRT 300N), do the following configurations 
· Set up Router IP Address 192.168.10.1 
· Enable DHCP 
· Set Start IP as 192.168.10.20  Maximum No. of users: 3  Save the configuration. 
· Set the Network mode: Mixed 
· Name your network: MyNetwork 
· Enable Broadcast 
· WPA2 Personal Security 
· Encryption AES 
· Passpharse: 123456789 
· Router Password: Cisco 
· Enable Remote Management 
Connect all the end devices as per the topology to the Wireless router. 
	Did all the laptops successfully connected to the wireless router? 
	

	 Yes all connected ok
 
If NO, Troubleshoot until all the hosts successfully connects and record your troubleshooting methods here. 
 
 
Did all the laptops gain DHCP IP address? 
 3 laptops had an address
 
Record your understanding, why all the laptops could not get IP address assigned from the DHCP. 
 Maximum IP reached
 
 
 
Disable and enable the DHCP IP Configurations in the Laptop and check the status. 
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Collect the MAC address of any two laptops and go to wireless mac filter option in the wireless router and set MAC Addressing FILTERING to prevent them to connect the network. 


[image: ] 
 
	Observe the changes in the network and record your reflections about MAC 

	Filtering and enhancing the security in Wireless Networks. 
 
 MAC addresses added to prevent PC’s to connecting to wireless network.
Makes them unable to pickup an IP.
 
 
 
 
 
 
 
 


 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
Learnings from this lab: 
· Build a home Network  
· Understand and configure IP Address 
· Use Ping/ Trace route Utility to check the connection status 
· Use ipconfig /all command to determine the MAC address of a Windows computer on an Ethernet network. 
· Analyze a MAC address to determine the manufacturer. 
· Analyze the Wired and Wireless Network connection. 
· Analyze Address Resolution Protocol (ARP). 
· Connect to a Wireless Router and configure the basic settings in a wireless router and add security features. 
· Use nslookup command to understand the url to ip conversion. 
· Configure basic connectivity settings in Intermediate devices (Switch/ Router). 
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