Specific Stream Submission Tom Schultze 1802180
5th Engine Workshop Session with John Kinsella
29th October 2019
Engine Workshop 

Reassembly of Inline 4 CBR 600R Engine

Health and Safety
-ALWAYS before entering workshop wear appropriate safety equipment. 
Equipment worn this session:
	-Eye protection: safety goggles
	-Protective clothing: dust coat provided by uni and steel toe caps

· Put in generator 1x14mm
· Put on generator cover 8x8mm
· Put on top end 10x12mm
· Put in coolant pump 2x10mm
· Different sized bolts left one is the longer bolt
· To put in cam shafts put the first piston at top dead centre (TDC) and put in cams and cam timing chain like in fig1.
[image: ]
Figure 1: Picture of camshaft position with timing chain
· To put piston at TDC remove spark plug, put in screwdriver in spark plug hole and turn motor until screwdriver starts dipping again => piston is at TDC
· Put back rocker housing 16x10mm
· [image: ]Watching out for inner and outer bolt lengths (Fig. 2)Figure 2: Rocker housing


· Put on clutch cover 14x10mm
· Put on top 4x10mm

Engine is fully rebuilt again! (Fig.3)
[image: ]Figure 3: Fully rebuilt engine













[image: ]As the session was not qu[image: ]ite finished John let us take apart the forks of the CRF 450 (Fig. 4 & 5) Figure 5: Inner workings of the fork
Figure 4: Opening the CRF forks




End of session
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