R1#show run
Building configuration...

Current configuration : 948 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524ECZQ-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 description Link to PC1
 ip address 185.95.3.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/3/0
 description Link to R3
 ip address 185.95.23.2 255.255.255.252
!
interface Serial0/3/1
 description to R0
 ip address 185.95.13.2 255.255.255.252
 clock rate 9600
!
interface Vlan1
 no ip address
 shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThiis is a secure!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
End
……….
R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.3.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/3/0            185.95.23.2     YES manual up                    up 
Serial0/3/1            185.95.13.2     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down

………
R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C       185.95.3.0/24 is directly connected, GigabitEthernet0/0
L       185.95.3.1/32 is directly connected, GigabitEthernet0/0
C       185.95.13.0/30 is directly connected, Serial0/3/1
L       185.95.13.2/32 is directly connected, Serial0/3/1
C       185.95.23.0/30 is directly connected, Serial0/3/0
L       185.95.23.2/32 is directly connected, Serial0/3/0
………………….
………………….
………………….
R1#show run
Building configuration...

Current configuration : 952 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15248U6P-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 description Link to PC2
 ip address 185.95.1.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/3/0
 description Link to R0
 ip address 185.95.12.1 255.255.255.252
 clock rate 9600
!
interface Serial0/3/1
 description Link to R3
 ip address 185.95.13.1 255.255.255.252
!
interface Vlan1
 no ip address
 shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
End
………..
R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.1.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/3/0            185.95.12.1     YES manual up                    up 
Serial0/3/1            185.95.13.1     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down
……………..
R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C       185.95.1.0/24 is directly connected, GigabitEthernet0/0
L       185.95.1.1/32 is directly connected, GigabitEthernet0/0
C       185.95.12.0/30 is directly connected, Serial0/3/0
L       185.95.12.1/32 is directly connected, Serial0/3/0
C       185.95.13.0/30 is directly connected, Serial0/3/1
L       185.95.13.1/32 is directly connected, Serial0/3/1
…………………………………………
………………………………………………
………………………………………………….
R0#show run
Building configuration...

Current configuration : 949 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R0
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15247L0V-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 description Link PC0
 ip address 185.95.2.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/3/0
 description Link to R1
 ip address 185.95.23.1 255.255.255.252
!
interface Serial0/3/1
 description Link to R3
 ip address 185.95.12.2 255.255.255.252
 clock rate 9600
!
interface Vlan1
 no ip address
 shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure!^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
 login
!
!
!
End
…………………….
R0#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.2.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/3/0            185.95.23.1     YES manual up                    up 
Serial0/3/1            185.95.12.2     YES manual up                    up 
Vlan1                  unassigned      YES unset  administratively down down
……………………..
R0#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C       185.95.2.0/24 is directly connected, GigabitEthernet0/0
L       185.95.2.1/32 is directly connected, GigabitEthernet0/0
C       185.95.12.0/30 is directly connected, Serial0/3/1
L       185.95.12.2/32 is directly connected, Serial0/3/1
C       185.95.23.0/30 is directly connected, Serial0/3/0
L       185.95.23.1/32 is directly connected, Serial0/3/0
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Packet Tracer BC Command Line 1.0
>ping 185.55.2.3

Pinging 185.95.2.3 with 32 byves of dava:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping scavistics for 185.95.2.3:

Packets: Sent = 3, Received = 0, Lost

Co\sping 185.55.2.3
Pinging 185.95.2.3 with 32 byves of dava:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping scavistics for 185.55.2.3
Packets: Sent = 4, Received = 0

Co\sping 185.55.1.3
Pinging 185.95.1.3 with 32 byves of dava:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping scavistics for 185.55.1.3

Packets: Sent = 4, Received = 0, Lost

4 (1008 1oss),

Tost = 4 (1008 loss),

4 (1008 1oss),

L

A B dx ENG

1251
200209 B





image2.png
Packet Tracer BC Command Line 1.0

C:\>ping 185.55
Ping request could not find host 185.95. Please check the name and try again.

Co\oping 185.55.3.3
Pinging 185.95.3.3 with 32 byves of dava:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping scavistics for 185.95.3.3:
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