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Description automatically generated]12. DHCP was unsuccessful at giving IP address to both PC’s this may be due to configuring trunking and port access in the switches wrong.
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Description automatically generated]

Pinging Ra1 from Ha2(unsuccessful due to DHCP not working)
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Description automatically generated]

18.
The configuration of on Rc1 is shown below. I could not connect to the router using ssh due to the password being incorrect. I used the same password that I set when creating the user ‘admin1’, but still unsuccessful.
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DHCP not working, due to this Hc2 could not connect.
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Description automatically generated]
DHCP not working, due to this Ha1 could not connect.[image: Graphical user interface, text, application, email

Description automatically generated]















DHCP not working, due to this Ha2 could not connect.
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Description automatically generated]
19. Due to question 18 not being successful the connection was unsuccessful for all connections

Results
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C:\>ssh -1 adminl 209.1€5.201.1

—
% Login invalid

(Connection to 205.165.201.1 closed by foreign host]
cove|
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