INTEGRATED PROJECT – PAD FOOTING CALCULATIONS
· Calculations followed for pad footing relating to the pile caps that are used on Matchstick Arena, as agreed with the client.
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Pad footing size acceptable
Reinforcement to be used is C10 @100mm c/c
image1.png
_Jﬁss..»ma eignt = 10k
| Tored ‘Decd boed T loosEoo =400 .

Qoox | + |Sox1 = lOSo
050 x5 190 = G Nm®
5 5% i %

Provde  2-5m% bete

Mw A fosting —> Assuwe  GoOrm
25 -2 :x0wxze = Wkuit tooene ok /

IVTEENES

REwpinG  REINFORLEMEDT

INMATE LA





image2.png
~Effecrue depih e
= A >

&= so 3 £
600 - 50 -20 = S30 . s o
- (s
_®. 156 x 35 x 1000 x 530% X 1O = 1S3y knom
M= (31 > Mu T (S3%  No comprtie
tqwn.o’.

Main  Skeed it

Bl.bx10° 7 0.01%3%
35 x 1000 x 530"

Ssogbs+ Z[D&:

S i 1l oA S
Y 0.9Sd = Sok = 2z = Sobmm &3

o onad 131.6 %10° = Goo >
0. 87 x 500 % 504

ASmin = 0137 bl © 01D X1000 X (oo = I§Omm”
€00 < I§0ma  As 2 ATOme wiv)€

 Provite  HIO @ 100 I fc . « 1





image3.png
LUx 3c0+¥xl.5%x 3530 = T560mnm

Boot+tax530): = 3.57x10%= 3 57Tm"™

s 2m o @) 52> ueve.

B ses o’ = ouuA - 04SSO |mn”
S0 x S30 =
5 Y b 118 ¢ i
=ixks=l 100%x3750 = Q. 141 -
b R o A
~ (oo0xS30

i~
15

= 034 x (Bsb.si = 0.37N|mn"
\ 3% CLA VRSN 3% W] meF 1

VS O.MiS < vc= 03%

Punchag fosiloe i onkiboly





image4.png
V= oo ( ) =
0. 6 Lsxm 2%%.3
8z

i

25%.82 <00 o)
3 0:32%

2500 x 530

e i fsel

N
O Sheor | Reimovanant
<4w





