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Spill Response Procedure

If the spill cannot be safely contained or if the spill is causing a threat to

life, evacuate the area and call 999 from a safe location

IF SAFETO DO SO

STOP > CONTAIN > NOTIFY > CLEAN-UP
STOP

* Stop work immediately
* Stop the leak or elimimate the source of the spill

* Eliminate ignition sources and provide natural ventilation

CONTAIN

* Use pollution control equipment (e.g. spill kits, drip trays, bunds of earth and sand) to contain the spill
* Check the spill has not reched any drains, water courses or other sensitive areas

« Coverall drains / manholes to prevent the spill from entering the drainage system

NOTIFY

* Oncethe spill has been contained notify your emergency contact. Details at the bottom of the page:.

CLEAN-UP

* Attempt to soak up the spill using absorbent material

« Always follow your Duty of Care for waste when disposing of contaminated materials including
spill kit/equipment.




