EXHIBITION FRAME SPACING & HANGING
Measure the wall (A)
Measure width of the frames (B)
(B) x the number of frames = (C)
(A) – (C) = (D)
(D) – number of spaces = (E)
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A – C = D
D / 4 = E

[bookmark: _GoBack]FRAME HEIGHT
Measure 60” from the floor – this is the mid point of the frame.
Measure the frame to find half the height. 
Add this value above the 60” to find where to mark the top of the frame.

FOR BATTONS
As above then measure the distance from the top of the print to the bottom of the wall baton
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