Method Statements
Project: Single, two storey detached domestic building.
Date of works: May 6th 2020
[bookmark: h.1kmozguib79q]Description of activity
Working from a scaffold at height to complete 3rd and 4th lift of blockwork and gables
Involves:
· Moving materials up scaffold
· Laying of blockwork
· Use of tools on scaffold
· Telehandler to assist in moving materials


Access on-site to be after hours between 8:00-16:00.
[bookmark: h.ygmyk6vg3h9j][bookmark: h.ocmnip9mxfv8]Training
All operatives are adequately trained to carry out required tasks.
All site operatives hold current certification and have the following training:
· CSCS certification
· Minimum level 3 qualification in brickwork 
· Working at heights training
[bookmark: h.r46xzs9m3ioz]Legislation
· Health and Safety Work Act 1974
· The Management of Health and Safety at Work Regulations 2006
· Workplace (Health, Safety and Welfare) Regulations 1992
· Provision and Use of Work Equipment Regulations (PUWER) 1998
· The Work at Height Regulations 2005
· The Personal Protective Equipment at Work Regulations 2002
· The Manual Handling Operations Regulations 1992
· The Construction (Design and Management) Regulations 2015
[bookmark: h.2cpfsm4rqcx7]Working at height
When working at height, site operatives must ensure that the working area is cleared on a period basis to ensure that there is continually a clear and safe working area to prevent slips trips and falls.
[bookmark: h.ddte95cmjn8g]PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
· Safety glasses (When cutting angles in blockwork for gables)
[bookmark: h.jjom1h6ke549]Welfare
Welfare arrangements are supplied by the client UWTSD.
These should be in line with Schedule 2 of the Construction Design & Management Regulations 2015
(CDM). All sites are to have a minimum amount of welfare facilities available for workers, which include the
Following:
· Toilets
· Washing facilities
· Drinking water
· Changing rooms and lockers
· Heating
· Rest facilities
Project: Single, two storey detached domestic building.
Date of works: May 6th 2020
Description of activity
Excavation of trenches for foundation to be poured
Involves:
· Excavator used to dig trenches
· Manual digging of trenches
· Banksman for each machine
· Pouring of concrete 
· Levelling of concrete to give flat surface for blockwork
Access on-site to be after hours between 8:00-16:00.
Training
All operatives are adequately trained to carry out required tasks.
All site operatives hold current certification and have the following training:
· CSCS certification
· NVQ in Groundwork
· Excavator license
Legislation
· Health and Safety Work Act 1974
· The Management of Health and Safety at Work Regulations 2006
· Workplace (Health, Safety and Welfare) Regulations 1992
· Provision and Use of Work Equipment Regulations (PUWER) 1998
· The Personal Protective Equipment at Work Regulations 2002
· The Manual Handling Operations Regulations 1992
· The Construction (Design and Management) Regulations 2015

The Construction (Design and Management) Regulations 2015
When digging excavations all practicable steps must be taken to ensure no part of the trench collapses, no materials or people fall into the trench. Inspections of the excavations must be carried out on a regular basis, any work that is unsatisfactory must be rectified prior to any further work commencing within the excavated area.
PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
· Safety glasses 
Welfare
Welfare arrangements are supplied by the client UWTSD.
These should be in line with Schedule 2 of the Construction Design & Management Regulations 2015
(CDM). All sites are to have a minimum amount of welfare facilities available for workers, which include the
Following:
· Toilets
· Washing facilities
· Drinking water
· Changing rooms and lockers
· Heating
· Rest facilities
Project: Single, two storey detached domestic building.
Date of works: May 6th 2020
Description of activity
Manual Handling of materials around site, from stores, up scaffolding.
Involves:
· Moving materials from stores to place of use
· Moving materials up and or down scaffolding
· Moving of materials up and or downstairs
· Lifting equipment
· Lifting of tools
· Lifting of machinery
Access on-site to be after hours between 8:00-16:00.
Training
All operatives are adequately trained to carry out required tasks.
All site operatives hold current certification and have the following training:
· CSCS certification
Legislation
· Health and Safety Work Act 1974
· The Management of Health and Safety at Work Regulations 2006
· Workplace (Health, Safety and Welfare) Regulations 1992
· Provision and Use of Work Equipment Regulations (PUWER) 1998
· The Personal Protective Equipment at Work Regulations 2002
· The Manual Handling Operations Regulations 1992
· The Construction (Design and Management) Regulations 2015
The Manual Handling Operations Regulations
Please see Appendix C risk assessment with regard to manual handling.
PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
Welfare
Welfare arrangements are supplied by the client UWTSD.
These should be in line with Schedule 2 of the Construction Design & Management Regulations 2015
(CDM). All sites are to have a minimum amount of welfare facilities available for workers, which include the
Following:
· Toilets
· Washing facilities
· Drinking water
· Changing rooms and lockers
· Heating
· Rest facilities

