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	EXERCISE SPECIFICATION 



	Student name:
	     
	Student ID number:
	

	Programme:
	

	Module:
	Safety & Hazard Assessment

	Module code:
	ACDB5013
	Contribution to Overall Module Assessment (%):
	0 - UNMARKED

	Lecturer:
	SSO PE Ltd
	Internal Verifier:
	

	Assignment Title:
	Hazard Identification (Exercise)
	Word count (or equivalent):
	N/A

	Submission deadline:
	N/A
	Return date of provisional marks & written feedback:
	N/A

	Submission method:
	No submission required.

	Academic honesty / referencing:
	Academic honesty is required. In the main body of your submission you must give credit to authors on whose research and ideas your work is based. Append to your submission a reference list that indicates the books, articles, etc. that you have used, cited or quoted in order to complete this assessment.  



	
TASK DESCRIPTION



Group Exercise:
Produce, as part of a small group, a high-level risk assessment covering major hazards for either an air launch munition (e.g. Brimstone 2), personal weapon (e.g. AK-47), armoured vehicle system (e.g. AJAX), sea launch munition (e.g. Sea Wolf), or large calibre gun system (e.g. 155mm).

Group 1 (Brimstone 2):
· Jack Frampton
· Thomas Lumsden
· Andrew Campbell
· Lucius Galloway
· Jack Twaddle

Group 2 (AK-47):
· Cameron Lane
· Callum Doherty
· Conor Nolan
· Ellie Martin
· Idora Musa

Group 3 (AJAX):
· Shaun Malone
· Elias James
· Rory Bowen
· Bethan Davies-Jones
· Kieran Howells
· Eryn Legg

Group 4 (115mm Large Calibre Gun):
· Charlotte McCombe
· Pippa Shay
· Joseph Nelhmas
· James Burton
· Thomas Creswell
· George Butcher

Important: This is an exercise and not a marked assignment; however, the assignment will be based on this work.

Step 1 - Generate a Risk Classification Matrix to determine the risk levels presented by the Hazards. It is acceptable to utilise industry experience; however, the work must remain non-proprietary and unclassified. By the end of this stage, the chosen hazards should be assigned a risk class from the matrix.

Step 2 - The group should perform Hazard Identification to capture the major hazards for their given system. The group should discuss why the chosen hazards were deemed the most important. 

It may be helpful to narrow down the scope of the Hazards to a single phase in the Manufacture to Target Disposal Sequence (MTDS) if the Hazard applies to multiple phases. A formal Hazard Identification technique (as spoken about in lectures) may be too onerous, it is suggested this is done in a brainstorming session. Referring to historical evidence and information from industry may help.

Step 3 - Following from the initial Hazard Identification, the group should aim to identify all credible Accidents and Causes (i.e. causal pathways) that may lead to the Hazard.

Step 4 - Next, the group should consider and estimate the risk for each of their Hazards, prior to any controls being implemented. 


Summary – The group should produce the beginnings of a Risk Assessment.

Full system knowledge is not expected; however, you should be able to identify the major Hazards of each system. 

All information utilised must be unclassified and open source.

This work is not an assignment and is NOT MARKED.
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