ACBA 5003 Class Questions

Question 1 (50 mins)
On Moodle a designer has provided drawings to calculate the initial budget cost for a domestic dwelling for a local housing developer. Spons should be used to price the dwelling (use Spons 2020 also on Moodle). The construction of the walls should be assumed to be render (15mm), Block (100mm), Cavity (25mm), insulation, (75mm) and block (150mm).

· You need to measure the dwelling provided on Moodle and use this to calculate the GIFA and therefore a budget cost total. Sate any assumptions made.

· Explain to the client the types of budget estimates available and the NRM1 rules for calculating.



Question 2 (50 mins)
· Why do we use standard forms of measurement for construction works and what are the types?
· What are the three common methods for obtaining construction prices, when producing a budget estimate?
· How can we improve the accuracy of the estimate as the design develops?



