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The Electronic Components Store and Technical Data Library occupies room MH507A in the Main Building occupied by the Faculty of Applied Design and Engineering. It is the main source of components and technical data for Staff and Electronics Students pursuing constructional activities.

This catalogue contains several new additions and supercedes all other versions which should be discarded.

---

The Electronic Components Store maintains a constant stock of over 650 different electronic components - mainly those which, are the essential 'bread-and-butter' of circuit design and development or, which experience has shown to be useful additions. 

---

The Technical Data Library, which is housed in the same room, is constantly updated with printed datasheets and CD-ROMs from a wide range of manufacturers. At present, over 18,750 documents are available for inspection and photocopying.

---

The Stores provides a number of other important facilities which are described in the following pages.

---

Ordering Components from Store stock :
You should treat any request made from the Store as if they are being made from an outside Supplier.  A standard form is used which can be obtained from the Store or your Project Tutor / Supervisor. Ensure that all the details requested are entered correctly - in particular, ensure that the correct three-digit order code for each item is used. The form must be signed by you Tutor / Supervisor.

Just as with an outside supplier, incorrect orders or incomplete details may cause delay or require you to resubmit the order.

Ordering Components from recognised Suppliers :
The Faculty deals with a specific group of electronics suppliers, namely :

· Rapid Electronics

· RS Components

· Farnell Electronic Components

· Maplin Electronics

In general, one of these suppliers will be able to satisfy your requirements. 

Orders to an outside Supplier are handled by the Faculty Office and the Institute Finance Office - hence, all references to delivery times in suppliers catalogues should be ignored.

Use the correct Outside Order Form, used which can be obtained from the Store, Faculty Office or your Project Tutor / Supervisor, to make your request. Ensure that all information required on the form is provided. In particular :

· the form must be signed by your Project Tutor / Supervisor

· all costs, subtotals, grand total and delivery charges must be shown

· you must use the supplier's current catalogue

It is your responsibility to ensure that your order is correct - although the order is checked by the Faculty Office, corrections are not made on your behalf.

It is usually uneconomic to request the return or replacement of items arising from an incorrect order - you have to reorder.

Your completed form should be passed to the Store for processing - when the goods arrive, your name and course details will be posted on the notice board found on the

corridor door of room MH507A.

 Requesting Technical Data from the Library :
Note that the Technical Data Library is nothing to do with the Institute's Mount Pleasant Engineering Library ! They cannot cater for the specialised nature of this facility which has been developed within the Faculty since the mid-1980's.

Due to the amount of information available, it is no longer feasible to produce an annual list of all the datasheets and documents available - the last print run of 1994 ran to over 150 pages.

Instead, an Intranet Web Server is maintained which, amongst other things, provides a simple search facility for interrogating the Technical Data Library Database. Every entry in the latter is identified by a unique library code which should be quoted when requesting photocopies - there is no written request form for this facility: verbal or your own written requests suffice.

Requesting Technical Data from other sources :
Verbal or written requests to the Store will be dealt with either from one of the Faculty's recognised Suppliers or an Internet search will be made. Whatever printed matter is obtained will be duplicated and placed in the Library for future use.

Electronic Printed Circuit Board Manufacturing :
The Store is responsible for the processing and manufacture of electronic printed circuit boards. Unless otherwise stated by your Project Tutor / Supervisor, all designs should be created using the Zuken-Redac software available in the Faculty - this ensures a constant level of manufacturing quality. Hand-created masks, those printed from other software or obtained by duplication from magasines cannot be guaranteed to be of 100% quality - indeed, it may not be possible to manufacture the board.

All designs should be submitted to the Store by 4.30pm on Monday. Boards are manufactured on Tuesday and, unless there is a particularly heavy demand, your board will be ready for collection by 4.30pm on Tuesday.

Note that YOU are responsible for drilling and 'finishing' the board !

Arizona Microchip PIC Microcontroller Development Software :
These microcontrollers are now standard for teaching Microprocessor-Based Systems and are the preferred choice for use in project work requiring such devices. The manufacturer's data CD-ROM, which contains the necessary editor, assembler and simulator software for IBM-PC computers is available free of charge from the Store.

Arizona Microchip PIC 19C74 and 16F84  Microcontroller circuit boards :

Ready-made (not drilled or 'finished' ! ) printed circuit boards for the above two microcontrollers are available from the Store. Each board is designed for the minimum component requirement for either microcontroller and is intended to be used with wire links to external circuitry or to be plugged into a 'solderless' breadboard.

Electronic Components Store & Technical Data Library Website : 


note : to avoid confusion arising from printing quality, the '(' symbol and 'k' multiplier replace the decimal point in the values shown for resistors and their associated components, e.g.  :
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note : no other values are stocked or available - if the result of a calculation calls for a non-standard value then you should make it from the available values or use a preset potentiometer to achieve the required resistance.

Fixed Value Resistors : WIREWOUND, 2.5W, 10%
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Fixed Value Resistors : Surface Mount R1206, 0.125W, 5%, 2% or 1%
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Fixed Value SIL and DIL Resistor Packs
note : the 220( (321) pack is a 14-pin dual-in-line (integrated circuit) package intended for use with 7-segment LED displays. All others comprise eight resistors in each single-in-line pack with a common terminal to each element. The common terminal is that end of the package nearest to a white or black spot adjacent to the value.
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Horizontal Mount Preset Potentiometers : CARBON FILM, 0.1W, 20%
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Panel Mount Rotary Potentiometers : CARBON FILM, LOG TRACK, 0.1W, 20%
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Fixing nuts
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Fixing washers
573
Panel Mount Slider Potentiometers : CARBON FILM, LOG TRACK, 0.1W, 20%
47k(
590
Miniature Fixed Value Capacitors  : CERAMIC, Medium K, 100v dc, 2%
note : to avoid confusion arising from printing quality, the 'n', '(' and 'p' multiplier symbols replace the decimal point in the values shown for resistors and their associated components, e.g.  :
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Moulded Fixed Value Capacitors  : POLYESTER, 63v dc, 20%
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Fixed Value Capacitors  : ELECTROLYTIC, 16v dc minimum, 20%
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Horizontal Mount Preset Capacitors  : POLYESTER FILM, 100v
2-22pF

361

5-65pF

301

Surface Mount Fixed Value Capacitors  : CERAMIC 50v, 0805
22pF  


722
39pF 1206 

O.O.S 


47pF 5% COG/NPO 
777
82pF 5% COG/NPO
781
1n5 10% X7R

777
10nF 10% X7R 

777
47nF –20/+80% Y5V
781
100nF 20% Z5U

785
Surface Mount Fixed Value Capacitors  : Tantalum
470nF 25V 1608 
792
1uF 25V 1608

789
4u7 35V 3216

797
10uF 25V Case D
793
33uF 16V 1812
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SEMICONDUCTORS : 74LS series TTL Digital Logic
74LS00
4 x 2-input NAND gate
205

74LS02
4 x 2-input OR gate
201

74LS04
6 x inverter gate
198

74LS05
6 x open-collector output inverter gate
200

74LS08
4 x 2-input AND gate
186

74LS10
3 x 3-input NAND gate
187

74LS11
3 x 3-input AND gate
214

74LS13
4 x 2-input NAND Schmitt-trigger input gate
203

74LS14
6 x inverter Schmitt-trigger input gate
184

74LS20
2 x 4-input NAND gate
213

74LS21
2 x 4-input NAND gate
212

74LS27
3 x 3-input NOR gate
211

74LS30
8-input NAND gate
223

74LS32
4 x 2-input OR gate
206

74LS33
4 x 2-input open-collector output OR gate
222

74LS42
BCD to decimal decoder
209

74LS47
BCD to seven-segment LED display decoder/driver
199

74LS72
Master J-K flip-flop
354

74LS73
2 x J-K flip-flop
190

74LS74
2 x D-type flip-flop
197

74LS75
4-bit bistable latch
193

74LS76
2 x J-K flip-flop
210

74LS78
2 x J-K flip-flop
189

74LS85
4-bit comparator
220

74LS86
4 x 2-input EXOR gate
204

74LS90
4-bit decade counter
196

74LS93
4-bit binary counter
202

74LS95
4-bit shift register
265

74LS96
5-bit shift register
188

74LS121
Monostable
208

74LS123
Dual monostable
192

74LS125
4 x tristate buffer
229

74LS132
4 x 2-input NAND Schmitt-trigger input gate
195

74LS133
13-input NAND gate
217

74LS138
3-to-8 line decoder
191

74LS139
Dual 2-to-4 line decoder
207

74LS148
8-input priority encoder
261

74LS151
8-input to-1 output multiplexer
255

74LS154
4-to-16 line decoder
218

74LS155
Dual 2-to-4 line decoder
185

74LS157
4 x 2-input to-1 output multiplexer
224

74LS163
4-bit synchronous counter
330

74LS165
8-bit parallel to serial shift register
226

74LS174
6 x D-type flip-flop
353

74LS193
synchronous up/down dual clk counters, binary with clr 
464

74LS244
8 x tristate buffer
219

74LS245
8 x tristate bus transceiver
221

74LS273
8 x tristate latch
215

SEMICONDUCTORS : 4000 series CMOS Digital Logic
4000
2 x 3-input NOR gate
533
4001
4 x 2-input NOR gate
534
4002
2 x 4-input NOR gate
535
4006
16 stage shift register
536
4011
4 x 2-input NAND gate
537
4012
2 x 4-input NAND gate
538
4013
2 x D-type flip-flop
539
4014
8-stage shift register
540
4015
2 x 4-bit shift register
541
4016
4 x analogue SPST switch
275

4017
5 stage Johnson counter
542
4018
4-bit divide by 'n' counter
543
4020
14-stage ripple counter
544
4023
3 x 3-input NAND gate
545
4025
3 x 3-input NOR gate
546
4027
2 x J-K flip-flop
547
4029
4-bit binary/decade counter
552
4030
4 x 2-input EXOR gate
553
4042
4 x D-type flip-flop
554
4046B
phase locked loop
264

4047
Monostable/astable multivibrator
555
4049
6 x inverter gate
556
4060
14-stage ripple counter & oscillator
571
4068
8-input NAND gate
557
4071
4 x 2-input OR gate
558
4072
4 x 4-input OR gate
559
4073
3 x 3-input NAND gate
560
4075
3 x 3-input OR gate
561
4081
4 x 2-input AND gate
562
4082
2 x 4-input AND gate
563
4508
2 x 4-bit latch
564
4510
4-bit BCD counter
565
4528
Dual monostable
566
4585
4-bit comparator
567
40106
6 x inverter Schmitt-trigger input gate
568
SEMICONDUCTORS : DIODES and RECTIFIERS
1N914 / 1N4148
small signal switching diode
146

OA91
small signal RF detector Germanium diode
273

1N4001
power rectifier, 100v/1A
140

1N4007
power rectifier, 1000v/1A
140

Bridge rectifier
100v/1A
143

Bridge rectifier
200v/2A
145

SEMICONDUCTORS : ZENER DIODES, 400mW
note : to avoid confusion arising from printing quality, the 'v' voltage indicator replaces the decimal point in the values shown, e.g.  5V1 == 5.1V

5v1
164
5v6
326
6v2
333
8v2
365
9v1
458

10v
162
12v
165
15v
163

SEMICONDUCTORS : CRYSTALS
note : some devices may be 'second hand' having been removed from equipment  - all will be in working order

32.768kHz
379
1MHz
161
1.8432MHz
576
2MHz
306
3.58MHz
585
4MHz
314

4.096MHz
578
4.333619MHz
586
6MHz
160

6.5536MHz
577
7.156MHz
587
8MHz
574
15MHz
575
assorted crystals & crystal oscillators
460

SEMICONDUCTORS : TRANSISTORS
BC107/8/9
NPN general purpose SILICON
157

BC212
PNP general purpose SILICON
134

BC461
NPN SILICON
156

BFY50
NPN general purpose, medium power, SILICON
158

BFY52 
NPN general purpose, medium power, SILICON
443

TIP29A
NPN power, SILICON
150

TIP31A
NPN power, SILICON
150

TIP30A 
PNP power, SILICON
154

TIP32A 
PNP power, SILICON
154

2N2646
Unijunction
989
2N2905A
PNP general purpose, 60V 600mA TO5, SILICON
1197
2N2907A
PNP low power, 60V 200Ma TO5, SILICON
1196
2N3053
NPN general purpose, medium power, SILICON
382

2N3055
NPN power, SILICON
381

2N3819
N-channel FET
281

VN10K
N-channel power FET
599
ZTX500
PNP general purpose transistor
420 

2SC106D
scr
149

TIC106 
scr 
149

SEMICONDUCTORS : MICROPROCESSORS & SUPPORT DEVICES
6502 CPU
1107
6522 VIA
1106
6551 UART
1106
8085 CPU
1066
8255 PIA
1066
Z80 CPU
1103

Z80 PIO
1105
Z80 CTC
1104

1488 RS232C transmitter
570
1489 RS232C receiver
225

PIC12F509
1312

PIC12F629
1312

PIC12F675
1312

PIC16C74A
1312

PIC16F628
1312

PIC16F675
1312

PIC16F685
1312

PIC16F73
1312

PIC16F84
1312

PIC16F84 (SO8 package)
1312

PIC16F871
1312

PIC16F872
1312

PIC16F873
1312

PIC16F873-04
1312

PIC16F875
1312

PIC16F876-04
1312

PIC16F877
1312

PIC16F877 ICEBREAKER
1068
PIC16F88
1312

PIC16F685
1312

PIC17C44
1312

SEMICONDUCTORS : LINEAR ICs
4046B
phase locked loop
264

709
uncompensated operational ampliifer
292

710
voltage comparator
270

723
variable voltage power supply regulator
580
741
operational ampliifer
173

7805
+5v/1A regulator
148

78L05
+5v/100mA regulator
359

7812
+12v/1A regulator
147

7815
+15v/1A regulator
152

7905
-5v/1A regulator
151

79L05
-5v/100mA regulator
358

7912
-12v/1A regulator
155

7915
-15v/1A regulator
153

CA3080
transconductance operational amplifier
582
LM311
voltage comparator
262

LM317T
adjustable regulator
592
LM324
4 x operational amplifier
322

LM339
4 x comparator
581
LM348
quad operational amplifier
322

NE555
Monostable/astable mulivibrator/timer
172

NE556
dual monostable/astable mulivibrator/timer
268

NE565
phase locked loop
108

NE567
tone decoder
258

TBA820
audio power amplifier
339

TL072
dual JFET operational amplifier
579
TL074
quad JFET operational amplifier
569
ULN2003A
7 open-collector high voltage drivers
259

ULN2803A
octal open-collector high voltage drivers
399

OPTOELECTRONICS
7-segment LED display - RED, common anode
130

7-segment LED display - GREEN, common anode
131

7-segment LED display - YELLOW, common anode
132

0.2" LED indicator - RED
139

0.2" LED indicator - GREEN
137

0.2" LED indicator - YELLOW
138

0.2” LED indicator – ORANGE
136

240v ac panel mounting neon indicator - RED
234

Standard ring/clip LED mounting
141

Through-panel push-fit LED mounting
452

3-digit LCD display with annunciators
584
Light dependent resistor
360

Infra-red emitter
311

Infra-red detector
363

Slotted opto-coupler (single led, single transistor) SY508
601
Slotted opto-coupler (single led, single transistor) Honeywell HOA0708-D01
649
RF COMPONENTS
Ferrite rod, 100mm x 8mm
403

5mm diameter polythene coil former
159

Ferrite core for above
159

7mm diameter plastic coil former
159

Ferrite core for above
159

Variable capacitor, tuning, two section.
417

CIRCUIT CONSTRUCTION
0.1" spaced stripboard
412

Standard tagstrip
tba

CONSTRUCTIONAL HARDWARE
Black pointer knob
249

Brushed aluminium round knob with pointer marking
459

Knob, black, aluminium skirt with pointer marking
589
Printed circuit board mounting pillar, 16mm
178

Printed circuit board mounting pillar, 10mm
432

Push-fit printed circuit board mounting pillar
439

Self-tapping screw, 10mm
tba

Self-tapping screw, 5mm
408

Grommet, 5mm bore
397

Grommet, 10mm bore
396

Grommet, sleeved, 10mm bore
398

Strain relief bush
tba

Self-adhesive feet
678
Cable tie, large
591
Cable tie, small
679
Self-adhesive cable tie base
n/a

1.25" in-line fuseholder, cable mounting
433

20mm fuseholder, pcb mounting
338

Cover for above
304

Heatsink, TO3
1032
Heatsink, TO5
253

Heatsink, TO18
351

Heatsink, TO220
344

8ba screw 
530
8ba nut
530
Crinkle washer 4ba
530
SOUNDERS
Loudspeaker, 8(, 66mm diameter
716
Crystal insert earpiece
419

Piezo buzzer, flying leads, external drive
583
Mechanical buzzer, 12v dc operation
529
Piezo, 12V self oscillating
550
Piezo sounder, small, pcb mounting, external drive
605

BATTERY HOLDERS & CONNECTORS
PP3 battery connector, wire ended
182

PP9 battery connector, wire ended
308

'AA' cell holder, single
390

'AA' cell holder, single, pcb mounting (Box 1)
1071
'AA' cell holder, single, pcb mounting (Box 2)
1072
'AA' cell holder, dual
377

'AA' cell holder, quad
369

PP3 holder, printed circuit mounting
676
PRINTED CIRCUIT BOARD CONNECTORS
Turret tag, 2mm insert
277

Turrett tag, 2.7mm insert
278

Solder tag, 0BA
402

Solder tag, 2BA
335

Solder tag, 4BA
401

Solder tag, 6BA
362

Solder tag, 6BA
404 Solder tag, 8BA
406

PCB mount fuseholder clips (20mm)
434

Stripboard pin, single sided
272

Stripboard pin, single sided, standard
n/a

Stripboard pin, double sided
276

Stripboard pin, double sided, standard
n/a

10-way pin strip connector - male
180

10-way pin strip connector - female
181

8-pin dual in-line socket
174

14-pin dual in-line socket
128

16-pin dual in-line socket
127

18-pin dual in-line socket
235

20-pin dual in-line socket
329

20-pin single in-line socket
247

24-pin dual in-line socket
237

28-pin dual in-line socket
230

40-pin dual in-line socket
236

90 deg 10w square pin connector male
183

CONNECTORS
40-way cable mounting IDC socket
171

14-way IDC DIL plug
167

16-way IDC DIL plug
166

Screw terminal block, printed circuit board mount, 2-way.
328

Screw terminal block, printed circuit board mount, 3-way.
327

Polythene insulated screw terminal strip
135

DIN 5-pin 180o chassis mounting socket
712

DIN 5-pin 180o cable mounting plug
719

RCA phono socket, chassis mounting
375

RCA phono plug, cable mounting, black
729

RCA phono plug, cable mounting, red
731

RCA phono socket, cable mounting, black
728

RCA phono socket, cable mounting, red
730

2.54mm jack socket, panel mounting
254

2.54mm jack plug, cable mounting
374

jack plug, ¼ inch
442

jack, line socket, ¼ inch
431b

UHF coaxial television socket, panel mounting
n/a

UHF coaxial television
n/a

SO-259 socket, panel mounting
707

PL-259 plug, cable mounting
708

BNC socket, chassis mounting
315

BNC plug, cable mounting
340

Crocodile clip, uninsulated
456

Crocodile clip cover, BLACK
331

Crocodile clip cover, RED
380

Crocodile clip, miniature, sleeved, RED
309

Crocodile clip, miniature, sleeved, BLACK
310

Banana plug, 4mm, BLACK
336

Banana socket, 4mm, BLACK
294

Banana plug, 4mm, RED
337

Banana socket, 4mm, RED
296

Banana plug, 4mm, GREEN
400

Banana socket, 4mm, GREEN
288

Banana plug, 4mm, YELLOW
341

Banana socket, 4mm, YELLOW
290

Banana plug, 4mm, BLUE
283

Banana socket, 4mm, BLUE
289

Banana plug, 4mm, WHITE
263

Banana socket, 4mm, WHITE
295

4mm binding post, panel mounting, BLACK
286

4mm binding post, panel mounting, RED
284

4mm binding post, panel mounting, YELLOW
287

4mm binding post, panel mounting, BLUE
285

4mm binding hook connector, BLACK
414

4mm binding hook connector, RED
415

Push on 'LUCAS' sleeve connector, crimp type, large
364

25-way 'D' plug
345

25-way 'D' socket
239

25-way 'D' socket, printed circuit board mounting
243

25-way 'D' connector shell
tba

9-way 'D' plug
228

9-way 'D' socket
227

36-way 'Centronics' socket, printed circuit board mounting
805
36-way 'Centronics' plug
805
Power connector, low voltage dc, pcb mounting 
607

Power connector, low voltage dc, cable jack 
608

DIN 41612 connectors, pcb.
548
DIN 41612 connectors
718
DIN 41612 connectors
719
Assorted IDC box headers
551
SWITCHES
8 x SPST dual-in-line package
129

SPST push to MAKE, RED button
447

SPST push to BREAK, BLACK button
440

2-pole, changeover slide
427

Mains single-pole rocker with integral neon indicator
411

1-pole, 12-way rotary with adjustable stop
449

2-pole, 6-way rotary, white 
453

2-pole, 6-way rotary with adjustable stop
454

3-pole, 4-way rotary with adjustable stop
462

4-pole, 3-way rotary with adjustable stop
463

Makaswitch wafers
1403
Makaswitch mechanism
1404 

Sub-miniature interlocking switches
1404
Button, large, black, for sub-miniature interlocking switch
717
Bracket, for sub-miniature interlocking switch
717
Keyswitch, pcb mounting
602
Cap, keyswitch (for 602)
603
Microswitch, pcb, sub-miniature
604

Keyswitch, tactile, 3mm button
606

240V panel mounting (rectangular cutout) circuit breaker 2.5A
372

Microswitch, miniature
973
Microswitch, miniature, lever roller actuator
840
Microswitch, miniature, pcb mounting
633
Microswitch, roller lever, Z-15GW22-B
1306

Microswitch, sub miniature
978
Microswitch, subminiature, lever operated
868
Microswitch, subminiature, long operating lever
675
Microswitch, Subminiature, pcb mounting F910-582
623
Microswitch, V3, long lever
652
Microswitch, V3, roller lever
823
Switch latch and mounting assembly for interlocking
532
Switch, decade thumbwheel
992
Switch, Decade
890
Switch, Decade, miniature
923
Switch, decade, miniature
949
Switch, DIL
921
Switch, DIL
923
Switch, DIL, 4 pole 2W
963
Switch, DIL, 4W
937
Switch, DIL, assorted
690
Switch, Hexadecimal rotary, pcb mounting
645
Switch, Inductive proximity
932
Switch, interlocking
686

Switch, interlocking, pcb mounting
844
Switch, Keyboard, Black
636
Switch, Keyboard, Blue
638
Switch, Keyboard, Green
637
Switch, Keyboard, Red
639
Switch, latching, round button, pcb mounting
686
Switch, latching, square button, pcb mounting
686
Switch, mains on/off pushbutton
1088
Switch, mains, indicator
844
Switch, mercury tilt
610
Switch, multipole pushbutton, pcb mounting
958
Switch, panel mount, SPST, dual
1213

Switch, pcb mounting
938
Switch, Pushbutton, latching
644
Switch, Pushbutton, latching, pcb mounting
645
Switch, pushbutton, n/o
982
Switch, pushbutton, push to break, n/c
610
Switch, Reed proximity
932
Switch, Reed, changeover contacts
960
Switch, rocker
927
Switch, rotary, hexadecimal, 0 to F
937
Switch, slide, 3 position
944
Switch, Slide, 90deg, pcb mounting
686
Switch, Slide, DPDT
937
Switch, slide, DPDT, pcb mounting
944
Switch, Slide, miniature SPDT, pcb mounting
655
Switch, Slide, pcb mounting
635
Switch, Slide, pcb mounting
686
Switch, slide, SPDT
944
Switch, Sub miniature toggle
921
Switch, Thumbwheel
620
Switch, Toggle
921
Switch, toggle, pcb mounting
696
Switch, toggle, SPDT
944
CABLE
Standard 7 x 0.2mm stranded hook up wire in the following colours :

BLACK
RED
WHITE
GREEN
BROWN
YELLOW

CYAN
BLUE
ORANGE
PINK
GREY
VIOLET

Standard 1 x 0.6mm solid hook up wire in the following colours :

BLACK
RED
WHITE
GREEN
BROWN
YELLOW

CYAN
BLUE
ORANGE
PINK
GREY
VIOLET

Extra-flexible test lead cable, 55 x 0.1mm :
BLACK
RED
YELLOW

Enamelled copper wire :
0.25mm
0.315mm
0.56mm
1.25mm

PVC sleeving :
BLACK
RED

40-way insulation displacement (IDC) ribbon cable

RG59U coaxial cable

Twin core, unscreened loudspeaker cable

1 x 0.44mm silver plated wirewrap wire

Additionals:

rs262-028 Triac Z0105DA (discontinued part)
299

n/a



156

n/a



159

4416-15 dram 


413

n/a ---



175

n/a PCB mounting pillar 16mm n/a

178

n/a ---



179

n/a ---



216

n/a ---



231

BCY461 N/A



232

n/a ---



233

n/a ---



282 

n/a



291

n/a



297

n/a



302

n/a



312

n/a



313

n/a



332

to3 h/s n/a



343

n/a unijunction 2n2646 n/a


352

smes 12v lamp


366

n/a



367

n/a



368

n/a



370

240V / 12V 3VA + 12V 3VA transformer

371

n/a



373

n/a 



376

n/a ---



391

n/a ---



392

n/a ---



393

n/a ---



394

n/a ---



405

n/a ---



407

n/a ---



416

n/a ---



418 

n/a ---



421

n/a ---



422

n/a ---



423

n/a 5 pin din couldn’t find


428

n/a ---



429

n/a ---



430

Reed relay operating coil


431A

n/a 1.25 in inline fusholder not found

433

n/a ---



435

n/a ---



436

n/a ---



438

n/a ---



444

n/a ---



448

n/a ---



455 

n/a ---



457

n/a ---



461

n/a



467

n/a



468

n/a



532 

Assorted high voltage electrolytic capacitors
588
ZN1034E



717
n/a ---



554

n/a



555

n/a



556

n/a



557

n/a



558

n/a 



559

10K linear slide potentiometer, 66-0105,

549

Capacitor, variable, single section, tuning
590

Capacitor, variable, two section, tuning

590

Capacitor, variable, 100pF panel mount

590

Capacitor, variable, 360pF panel mount

590
Relay 6V coil, sp, 3A, pcb mounting

600
74LS193, synchronous up/down dual clk counters
464

0.01R (10 milliohm bare resistor)

465

SE95 
temperature sensor IC, SO8
465

74LS373
octal D type latch

468
 XR2206
Function generator

468
74LS166
8 bit shift register

468
NE531N High slew rate opamp 

468
 BCY70 PNP transistor –40V 200mA

468
D gender bender shell, 25W

551
Socket, panel mount, 3mm, yellow

609

Socket, panel mount, 3mm, white

609

Socket, panel mount, 3mm, blue

609

Socket, panel mount, 3mm, black

609

Switch, mercury tilt


610

Switch, pushbutton, push to break, n/c

610

Thermistor, 1k NTC disc


610

Ultrasonic distance sensor “Ping)))”


611

Plug, 2mm black


612

Assorted dil & sil resistor packs

613
MJE340
NPN transistor, 300V 500mA
614
2mm pcb testpoints


614
759 
Power OpAmp RS303-258

614
RT matched thermistor 100k RS151 243

614
Radial leaded bobbin inductor

615
RS307-979, Opto-isolator 20% current transfer
616

RC725DE, “Precision” Opamp (equiv LM725)
616

7417, Hex buffer driver open collector 15V
616

74LS122, Retrigger able monostable with clr
616

74LS192, BCD synchronous up/down counter
616

74LS257, Quad data selector

616

74LS283, 4-bit binary full adder

616

74LS365, Hex bus driver


616

74LS49, BCD to 7 segment decoder opn coll o/ps
616

74LS92, Divide by 12 counter

616

DM8131N, 6-bit comparator

616

RC4152N, Voltage to Frequency converter
616

MP7524AAN, 8-bit multiplying D2A converter
616

UA9637A
Dual differential line receiver
616

443, Zero voltage switch RS307-985

616

MOC3020, Opto isolated triac marked 3020
616

10nF ceramic capacitor


617
100pF ceramic capacitor


617
10nF, 2kV ceramic capacitor, DEBF33D103ZA3B
617

Aluminium compensated strain gauge

618
Miniature BNC 50R 


618
D connector, 9W, male, 90deg, pcb mounting
618
D connector, 26W, female, 90deg, pcb mounting
618
15nF box polyester capacitor 100V

619
5R wirewound 5W


620
Switch, Thumbwheel


620
Seven Segment display, Red, 1 inch

621
Seven segment display, yellow, 0.6 inch, dual
621
AM9128-15 2k x 8 static ram

622
Rotary encoder


623
Microswitch, Subminiature, pcb mounting F910-582
623
LM35DZ ic temperature sensor (SO8)

624
LM2940CT-5 voltage regulator

624
220R sil resistor 


624
MAX232CPE
 RS232 IC


625
SP232ACP RS232 IC


625
LE50CZ voltage regulator 5V 100mA 2% TO92
626
TL082CN
Opamp


626
Sn7414



626
74ls39



626
74C93



626
Melody IC “It’s a small world”

627
Melody IC “Happy Birthday”

627
Melody IC “Jingle Bells”


627
DS1669-010



628
Relay, SIL, AX161A-2


628
200k multiturn pot


629
SAA1027
Stepper motor driver

629
MICRF102BN UHF ASK tx


629
MICRF 002BN LP UHF rx


629
HT6320
Holtek IC


630
HT12F
Holtek decoder

630
HT12A
Holtek encoder

630
UM3750
Programmable encoder/decoder
630
HT6350
Holtek IC


630
HT12D
Holtek decoder

630
24LC256 
EEPROM, 256k bit

630
40W latch/eject DIL socket


630
TIP126
PNP darlington 80V 5A

631
10K 8 pin sil 4 resistor pack

631
Loudspeaker



632
UM661-GBL ic


632
Microswitch, miniature, pcb mounting

633
Rotary encoder, F328-2296

633
Piezo sounder,  small, pcb mounting, external drive
634
Switch, Slide, pcb mounting

635
Switch, Keyboard, Black


636
Switch, Keyboard, Green


637
Switch, Keyboard, Blue


638
Switch, Keyboard, Red


639
1uF polyester radial


640
D connector, 9W, male, 90deg, pcb mounting
641
TIP132
NPN darlington 100V 6A

642
Ultrasonic transmitter, plastic case

642
Ultrasonic receiver, plastic case

642
Relay, Omron DPDT, G5V-2 G5L-114P-PS
643
Relay, reed



643
Relay, miniature


643
MM53200N
Encoder/Decoder 12 i/o

644
IRF9Z34
P channel Power Mos –60V –13A
644
Switch, Pushbutton, latching

644
Switch, Hexadecimal rotary, pcb mounting
645
Switch, Pushbutton, latching, pcb mounting
645
Tx module



645
Subminiature solenoid


646
15nF 100V box polyester capacitor

647
TIP2955
PNP power transistor

647
TIP3055
NPN power transistor

647
Pulse transformer F148-917

648
Reflective object sensor, InfraRed, ISTS708
649
Binding post, Red & Black pair

649
HOA708 reflective opto sensor

649

LM1458N
Opamp, dual


650
IR remote control receiver IS1U60 RS577-897
650
Zero ohm link


650
L298N 
Dual full bridge motor driver
651
Microswitch, V3, long lever


652
LED, HUVL400-510B, UV, 5mm, 10 DEG
653

LED, clear, multicolour, 5mm

653
LED, clear, multicolour, 3mm

653
IR receiver HIM602V, F414-2822

653
LXHL-MX05 collimating optic F432-6015

654
LED, luxeon, white, high power

654
LED, white, water clear, 5mm

654
Switch, Slide, miniature SPDT, pcb mounting
655
10k precision pot. F136-360

656
Ultrasonic transmitter, sealed

657
Ultrasonic receiver, sealed


657
10k pot, pcb mounting


657
TA78L005AP

voltage regulator
657
500k 10 turn trim pot


657
1M 10 turn trim pot


657
BC547B 
transistor


658
BC548
transistor


658
IRF530
Power FET 100V 14A

659
LED, HE RED, 3mm, 5V Rapid 56-1400

660
LED, HE RED, 3mm, 12V Rapid 56-1450
660
MICRF002BN lowpower UHF rx

661
MICRF102BN UHF ASK tx


661
Pins, gold plated


662
Plug, 2mm, BLACK


663
SIL socket, wire wrap


664
Molex socket, 3W


665
Molex crimp



665
Jack socket, 3.5mm, 90deg pcb mounting
666
Molex header, 3W, pcb mounting

667
Jack, stereo, 3.5mm


668
Jack, mono, 3.5mm


668

LED, RED, 20mm diameter, Kingsbright DLC2/61D
669
Relay, OMRON GRL-2 12V DPDT

670
L293D 
quad push/pull motor driver with diodes
671
L293E 
quad push/pull motor driver
671
Electrolytic capacitors, assorted

672
Assign contents
IDC box header, 50W, 90deg pcb mounting
673
MC75491N
Display driver

674
MC75492N
Display driver

674
IDC cable connector, 20W


674
Microswitch, subminiature, long operating lever
675
Ferrite bead



675
PP3 holder, printed circuit mounting

676

Assorted preset pots, skeleton; 10 turn etc
677

500k preset 10turn


677

10k preset 10 turn


677

2k2 skeleton preset


677

4k7 skeleton preset


677

2M2 skeleton preset


677

22k skeleton preset


677

100R moulded preset


677

1k moulded preset


677

1M preset 10 turn


677

200k preset 10 turn


677

Self-adhesive feet


678

Cable tie, small


679

Solderless LED holder,
 2.54 mm

679

TIP121
NPN darlington 80V 5A

680
LM386
Low voltage audio Power amplifier
680
LM393
voltage comparator, dual

680
Relay, solid state, MP240D4-7 

681
Header, square pin


682
HP3700 340 optocoupler?


683
TLP521-4 NPN phototransistor/quad optocoupler
683

TIP3055
NPN power transistor

683
Hex 2.5mm standoff


683
Turned pin sockets


683
LM380 IC audio amplifier


684
LM1496 double balanced mixer

685
Switch, Slide, pcb mounting

686
Switch, Slide, 90deg, pcb mounting

686
Switch, latching, square button, pcb mounting
686
Switch, latching, round button, pcb mounting
686
Switch, interlocking


686
Order

Trimpot, multiturn, assorted (used)

687
ZN458A
2.45V precision reference (used)
688
TBA625BX5



688
AD581JH



688
BF981 
dual gate mosfet

689
J310
Jfet


689
3n201
dual gate mosfet

689
Switch, DIL, assorted


690
Relay, 6V, Schrack RP420008

691
Assign contents
30R wirewound


692
LED, strip, 90deg


692
BFY50
NPN transistor (used)

692
2N3053
NPN transistor (used)

692
Resistor, wirewound


692
Standoff, pcb, Teflon


693
MI-6508B-9 IC, Harris


694
1uF capacitor, polyester, radial

695
Switch, toggle, pcb mounting

696
Bridge rectifier, Semicron SKB2/02

697
D connector, 25W, male, IDC

697
Wirewound ceramic cement resistor, 270K(, 10W
697

CD4022
Octal counter/divider

698
RC4558 
Opamp, DIL8, dual 741

698
LM13600N
Dual Transconductance amplifier
698
LM358AN
Dual Opamp, low power

698
BF494 
NPN transistor

699
4N25
Optoisolator


700
10R 1206 2%


701
HM6116LP-3, 8-bit high speed CMOS SRAM
702

6116
16k (2k x 8) static ram

702

HM6116

16K static ram 2k x 8
702

HM6264

64k static ram 8k x 8
702

HM6264LP-15 
64k static ram 8k x 8
702

TC5565P
static ram 64k 8k x 8

702

TMM2016
static ram 2k x 8

702

UM6116-2 
2k x 8 static ram

702

UM6264A-10
 8k x 8 static ram

702

120R 1206 2%


703
430R 1206 2%


704
1K3 1206 2%


705
11R 1206 2%


706
D43256AC-10 32K x 8 static ram

707

GM76C256C1L-70 
32k x 8 static ram
707
K6T1008
128k x 8 static ram

707

KM62256BLP 
32K x 8 static ram
707

LH52256L-90 
256K static ram 32K x 8
707

M5M51008AP-70L 
128k x 8 static ram
707

SRM20256LC10 
32k x 8 static ram
707

V62C256BP15L  32k x 8 static ram

707

130R 1206 2%


708
470R 1206 2%


709
1K5 1206 2%


710
15R 1206 2%


711
12R 1206 2%


711
47R 1206 2%


712
160R 1206 2%


713
510R 1206 2%


714
1K6 1206 2%


715
Meter, edge reading


716

Meter, 100uA fsd


716

Meter, 1mA fsd


716

Meter, 100uA fsd, scaled 0 – 3V, 0 –10V

716

16R 1206 2%


720
51R 1206 2%


721
capacitor (supplied in error for)

722
180R 1206 2%


722
560R 1206 2%


723
1K8 1206 2%


724
18R 1206 2%


725
56R 1206 2%


726
200R 1206 2%


727
750R 1206 2%


728
620R 1206 2%


728
2k 1206 2%



729
20R 1206 2%


730
62R 1206 2%


731
220R 1206 2%


732
820R 1206 2%


733
2k2 1206 2%



734
22R 1206 2%


735
68R 1206 2%


736
240R 1206 2%


737
910R 1206 2%


738
2k4 1206 2%



739
24R 1206 2% 


740
75R 1206 1%


741
270R 1206 2%


742
0R0 1206 2%


743
3k0 1206 2%



744
2k7 1206 2%



744
27R 1206 2%


745
82R 1206 2%


746
300R 1206 2%


747
13R 1206 2%


748
3k3 1206 2%



749
30R 1206 2%


750
91R 1206 2%


751
330R 1206 2%


752
680R 1206 2%


753
3k6 1206 2%



754
33R 1206 2%


755
100R 1206 2%


756
360R 1206 2%


757
1k0 1206 2%



758
3k9 1206 2%



759
36R 1206 2%


760
110R 1206 2%


761
390R 1206 2%


762
1k1 1206 2%



763
4k3 1206 2%



764
6M8 1206 5%


765
7M5 1206 2%


765
33uF 16V tantalum capacitor 1812

766
LM311 
Voltage comparator SO8

767
Pushbutton, surface mount


767
Connector, SMB, pcb mounting (through hole)
768
9M1 1206 5%


769
8M2 1206 2%


769
NE555N
timer


770

NE555D
timer SO8


770
Screw terminal, 3W, pcb mounting, through hole
771
Screw terminal, 2W, pcb mounting, through hole
772
10M 1206 2%


773
6M2 1206 5%


773
Bridge rectifier, surface mount

774
TS68000CFN8 cpu


775
Zener diode, SOT23, code V2

776
Zener diode, SOT23, code Z9

776
Zener diode, SOT23, code Z2

776
Zener diode, SOT23, code W6

776
10nF 50V 10% X7R 0805


777
1n5 50V 10% X7R 0805


777
47pF 50V 5% COG/NPO 0805

777
BAS16/T1 
diode, coded A6

778
MK6823Q-8D


779
Zener diode, SOT23, code Y2

780
Zener diode, SOT23, code Z4

780
82pF 50V 5% COG/NPO 0805

781
47nF 50V –20/+80% Y5V 0805

781
LED, IR, sidebeam, ceramic, smd

782
LM3900, Quad Norton input Opamp

783
CA3081, CA3082, Transistor array

784
100nF 50V 20% Z5U 0805


785
LED, Yellow, ceramic, smd


786
PLCC socket, smd


787
Zener diode, SOT23, coded Z3

788
1uF 25V tantatlum capacitor 1608

789
Photodiode, ceramic, smd


790
PLCC socket, smd


791
470nF 25V tantalum capacitor 1608 case A
792
10uF 25V tantalum capacitor Case D

793
BC857B transistor, SOT23, coded 3F

794
741
opamp


795

LM741C 
opamp SO8


795
Relay, 12V 280R, 250V 10A SPST

796
4u7 35V tantalum capacitor 3216?

797
BCF32 transistor SOT23


798
Crystal, 4MHz, SM


799
Crystal, 6MHz, SM


799
Crystal, 8MHz, SM


799
Crystal, 3.579MHz, SM


799
Crystal, 16MHz, SM


799

Relay, 12V 280R SPST


800
D connector, 9W, female, 90deg pcb mounting
801
3mm pan head screw


802
Pan head self tapper


803
Relay 6V coil, sp, 5A, pcb mounting

804

Relay, 6V, SPST, Kam Ling KU1T-F, 5A

804

Relay, Omron SPDT, G5L-114P-PS, 12V coil
804

Relay, Omron SPDT, G5LE – 14, 12V coil
804

Relay, Omron SPDT, G5LE 1-5, 5V coil

804

36-way 'Centronics' socket, PCB mounting
805

36-way 'Centronics' plug


805
Centronics connector 36W plug

806

74HC175
quad D type flip flops, common clear
807

EF6809EP cpu


807

Display, Vacuum Fluorescent, 16 char 7x5 dots
807

2R7 resistor 25W 5%


807

25k pot



807

100R pot



807

5K pot



807

2k pot



807

DC power connector, large


807

DC power receptacle,large, chassis

807

DIN socket, 6W, line, 270 deg

807

DIN socket, 5W, chassis, 270 deg

807

Antenna, 7 section telescopic

807

Antenna, whip


807

Probe Clip, Red


808
10k pot, pcb, enclosed


809
Socket, 4mm, Red


810
Socket, 4mm, Red


811

Socket, 4mm, Black


812
Socket, 4mm, Black


813

Plugs, 3mm, Red


814
Sockets, 3mm, Red


814
Plugs, 3mm, black


815
Sockets, 3mm, Black


815
Isolated BNC bulkhead socket

816
LM309
Regulator, 5V

817

Socket, ZIF, 28W


818
Socket, ZIF, 14W


818
Plastic wheel



819
Plastic lever



819
D connector, 25W, female, IDC

820
D connector, 15W, female, IDC

820
BPW34 photodiode


821

IS471FE, Optical Light Detector, IR, 4 lead
821

Phototransistor, TEPT4400, 570nm (green)
821

Tept4400 phototransistor 570nm

821

Ultrasonic transmitter


822

Ultrasonic receiver


822

10k 0.125W



823

Microswitch, V3, roller lever

823

1k5



824

150k



824

2k



824

16k



824

47(



825

5k1



825

50k miniature skeleton pot


825

30k



826

270k



826

3k3



827

BC479



828

22uF tantalum bead capacitor

829

2200uF 25V axial electrolytic capacitor

829

100nF 



829

4700uF 50V radial electrolytic capacitor

830

1000uF 63V axial electrolytic capacitor

830

1000uF 35V radial electrolytic capacitor

830

1000uF 25V radial electrolytic capacitor

830

1000uF 10V axial electrolytic capacitor

830

Plug, 2mm, Red


831

TIC106M, SCR Thyristor, 600V, 5A

832

CTB-34, Schottky Barrier Diode Center Tap, 40V
832

140uF 100V axial electrolytic capacitor

833

47uF 100V axial electrolytic capacitor

833

33nF 400V



834

10nF 750V



835

1nF 1kV box polyester capacitor

835

1nF 1kV ceramic


835
Assign contents
Plug, 2mm, Black


836

1uF 250V 10% capacitor


836
Assign contents
100nF ceramic disk capacitor

837

10nF ceramic disk capacitor

837

PET100 chassis socket


838

PET100 cable plug


838

Clip, probe, black


839

Microswitch, miniature, lever roller actuator
840

74LS83AN



840

GET114 
germanium transistor

841
Assign contents

TDA2540
TV IF amplifier & demodulator
841
Assign contents

TBA540Q
TV IC


841
Assign contents

TCA800Q
TV IC


841
Assign contents

TBA520
Chroma demodulator

841
Assign contents

TCA270
TV ic


841
Assign contents

BTX18
Thyristor 1A


842

OA210
400V 5A rectifier

842

AC127
Germanium transistor

842

AC176
Germanium transistor

842

AF116
Germanium transistor

842

PXB103
Germanium transistor

842

AC153
Germanium transistor

842

BFY50
NPN transistor 35V 1A

842

BCZ11
Bidirectional transient suppressor
842

TIC116M
SCR 9A 800V

842

BC113
NPN transistor



842
BC115
NPN transistor 30V 100mA
842

BC187
PNP transistor

842

BF180
NPN transistor UHF

842

BF594
NPN transistor 

842

BF596
NPN transistor UHF

842

OC71
PNP germanium transistor

842

BZX61C16
Zener diode 16V

842

BZX61C18
Zener diode 18V

842

BZX61C20
Zener diode 20V

842

BZX61C22
Zener diode 22V

842

BZX61C24
Zener diode 24V

842

BZX61C27
Zener diode 27V

842

BZX61C30
Zener diode 30V

842

BZX61C33
Zener diode 33V

842

BZX61C36
Zener diode 36V

842

BZX61C39
Zener diode 39V

842

BZX61C47
Zener diode 47V

842

BZX61C56
Zener diode 56V

842

BZX61C68
Zener diode 68V

842

BZX61C72
Zener diode 72V

842

74HC4040AP 12 stage binary counter

843

74HC4024N
7 stage binary counter

843

74HC4053N
triple 2 channel multiplexer

843

74HC153N
dual 4 input multiplexer

843

CA3306E
flash 6 bit A2D converter

843

74177BP
presettable binary counter

843
Verify item

LM6361N
high speed opamp

843
Switch, mains, indicator


844

Switch, interlocking, pcb mounting

844

SL6270DP



845

1800pF 50V ceramic capacitor

845

10nF 50V ceramic capacitor

845

560pF 50V ceramic capacitor

845

330pF 50V capacitor


845

1500pF 50V capacitor


845

390pF 50V ceramic capacitor

845

220pF 50V ceramic capacitor

845

470pF 50V ceramic capacitor

845

1000pF 50V ceramic capacitor

845

1000pF 100V ceramic capacitor

845

120pF 100V ceramic capacitor

845

2700pF 50V ceramic capacitor

845

50k preset 10turn


845

Pots, assorted, dual, with/ without switch

846

EPSD12/250, DC power supply, PCB, +-12V, 250mA
847

DL411AT, Elektra, DC/DC converter, PCB
847

NMXD1215S0, DC/DC converter, PCB

847
ASYKO, DC/DC converter, VVCF 24-2-18-100, PCB
847
PTF14A-E, Relay socket, 14-pin, 240v, 10A
847
PTF08A-E, Relay socket, 8-pin, 240v, 15A
847

Diodes, assorted


1210

Rectifiers, assorted


1210

KBPC2502 bridge


1210

OA202



1210

BZY88C3V2



1211

1N5349B



1211

BZY88C10



1211

BZX61C24



1211

BZX61C30



1211

BZY88C8V2



1211

BZX61C7V5



1211

BZX61C13



1211

BZX61C15



1211

Assorted zeners


1211

Screw, self tapping, cross head, 6mm

848
93C46N
eeprom, 1k bit, microwire bus
849
Ultrasonic transmitter


850
Ultrasonic receiver


850
Nylon gear (small)


851
Nylon worm gear


852
Nylon pulley, large


853
Nylon pulley, small


854
Nylon gear, large


855
Nylon Pulley, very small


856
Nylon gear, medium


857
Axle



858
Nylon worm gear, long


859
Nylon gear (medium)


860
Nylon gear, medium


861
Nylon gear, different from all the rest

862
Clip, probe, for IC leg


863
TO3 socket



864
0.1” shorting links


864
Assorted 10 turn trim pots


865
IDC cable skt, 34W


866

MES batten lamp holder


1258

Hex standoffs


1258

LED, Red, square


867
Microswitch, subminiature, lever operated
868
Assorted screws


869
Assorted screws


870
BD680
PNP darlington transistor 80V 4A
871
BD679 
NPN darlington transistor 80V 4A
871
BNC jacks



872
Assorted fuses


872
Hooked blade contact terminal crimps

873
Chocolate block


873
BC557 
PNP transistor

874
Self adhesive pads for tiewraps

875
Disposable knife blade refills

875
LED, IR, TSUS5402, 950NM, 22DEG, 5MM,
876

LED, Green, 1300mcd 525nm, L-7083ZGD
877
78L09
Voltage regulator, 9V

878
Thermocouple connectors


879
Assign contents
79L06
Voltage regulator, -6V

880
Pins, very long


881
79L15
Voltage regulator, -15V

882

79L12
Voltage regulator, -12V

883
79L05
Voltage regulator, 5V

884
78L06
Voltage regulator, 6V

884

D connector fixings


885
100R Wirewound Resistor


886

Chrome holders for LEDS


887
LM323K
voltage regulator, 5V 3A TO3
888
2N6059
NPN darlington 100V 12A TO3
888
2N3055
NPN transistor 60V 15A TO3
888
2N6673
NPN transistor 400V 8A TO3
888
LT1003CK
Voltage regulator, 5V 5A TO3
888
2SC1413
NPN transistor 500V 5A TO3
888
2N2219A
NPN transistor 40V 800mA TO5
888
2N2905A
PNP transistor 60V 600mA TO5
888
TIP145
PNP darlington 60V 10A TO3
888
BNC termination


889
Switch, Decade


890
DIL Wirewrap sockets, 40W

891
Double row female pin header, 100-way 2.54mm
892
30mm M3 hex F-F spacer


893
5mm hex standoff


894
8mm hex standoff


895
`
5mm M3 hex standoff


896
16mm M3 hex standoff


897
M3 hex standoff with external thread

898
25mm nylon hex standoff


899
M3 nylon nut



900
M3 nylon washer


901
M3 nylon screw 6mm


902
M3 nylon screw 16mm


903
M3 nylon screw 20mm


904
M3 steel nut



905
M3 steel washer


906
M3 crinkle washer


907
M3 steel screw 6mm


908
M3 steel screw 12mm


909
M3 steel screw 20mm


910
Ferrule



911
TIP122
NPN darlington 60V 5A

912
D connector, 9W, female, 90deg, pcb mounting
913
14mm hex standoff


914
Probe gripper for DIL lead


915

Photodiode, TO18, rs305-462 IPL10020BW 
916

3NA5111A 5mm Infrared 15° 850nm Water Clear
917

High Speed Infrared Emitting Diode, 850 nm
918

OPB706B reflective object sensor

919

KTIR0821
Reflective photointerruptor

919

L-610MP4BT/BD
dual phototransistor, IR
919

LED, IR, LD274-3


919
Order
SFH309 T1
Phototransistor, IR, filtered

919

SFH309-5 T1 Phototransistor, visible light
919

LED, Red



920

Keyswitch



921

Switch, Toggle


921

Switch, DIL



921

Switch, Sub miniature toggle

921

P8255A  
Programmable I/O ic

922

Reed relay



922

LM1881M
video sync separator

922

MP0820JN
8 bit A2D with track & hold

922

AD7110KN
?audio attenuator

922

Coil



922

Switch, DIL



923

LED



923

78H05K 
Voltage regulator, 5V

923

Switch, Decade, miniature


923

AD536AJH
True RMS converter

923

HP2300



923

TDA8444P
octuple 6 bit D2A with IIC i/f
923

LED, IR



923

Optosensor



923

INA101HP
Instrumentation Amplifier

924

MC3450
quad differential line receiver
924

LED BAR



924

Relay, 6V 80R coil


924

Reed relay



924

7 segment display


924

TDA2030H
14W audio amplifier

924

LS141T
op amp


924

SL490
IR remote control transmitter
924

TBA120
FM demodulator for tv

924

MC14511BCP
7 seg display driver
924

HCF4511

7 seg display driver
924

8211CPA
programmable voltage detector
924

HIP5500IP
half bridge driver

924

MAX705CPA
 microprocessor supervisor
924

93C46ABI
eeprom, microwire i/f

924

MM74C922N
 keypad encoder 16/20 keys
924

XR4136
OPAMP


924

OP421HP
quad opamp


924

TL81



924

ZN416E
AM radio receiver (trf)

925

ZN425E
8 bit A2D/D2A converter

925

ZN427E
8 bit successive approx A2D converter
925

ZN439E
8 bit successive approx A2D converter
925

ZN428E
8 bit latched i/p D2A converter
925
Order

ZN448E
8 bit successive approx A2D converter
925

ZNA234E
TV sync pulse generator

925
HD46505SP (6845 equiv)


925

HD68P01V07 (piggy back 4k rom hd6801)
925

HD68P01M0 (piggy back 8k rom hd6801)
925

V62C256BP15L
32k x 8 static ram
926
Order

HM6264LP-15
8k x 8 static ram
926
Order

AD537KH
Voltage to frequency converter
926
LM308
Opamp


926
Order

LS141T
Opamp, TO99 metal can

926
TI543
??


926
2N3906
PNP transistor

926
2N3904
NPN transistor

926
Order

2N3705
NPN transistor

926
2N3703
PNP transistor

926
Order

2N3706
NPN transistor

926
UGN3020
hall effect device

926
Order

DAC0800LCN
8 bit D2A converter
926
Order

ICL8038
waveform generator sine/sq/triangle
926
PMI DAC08
high speed multiplying 8 bit D2A
926
2K 10 turn trimpot


926
10k 10 turn trimpot


926
Order

HP HDSP-7301 0.5” 7 Segment display

927
Order

Switch, rocker


927

LED, assorted


927
TLC772CP
??


928
Order

MAX665
1.5 to 8V voltage converter

928

CD14067BCP 16 channel analogue multiplexer
928

CD14051
8 channel multiplexer

928

CD4040
12 stage binary counter

928
Order

CD14024
7 stage binary counter

928

100nF ceramic


929

LED, Red, square


930

LED holder, 8mm


931

Switch, Reed proximity


932
Order
Magnet



932
Order
Inductive pickup


932
Switch, Inductive proximity


932
40W IC testclip


933

IDC box header


934

IDC cable connector


934

LCD character modules, assorted

935

Keypads



935

UM6116-2 
static ram


936
Order

SRM20256LC10 static ram

936
Order

HM6116
static ram


936
Order

OKI M6926
FSK modem


936

LM3302N
quad comparator

936

NE521N
high speed dual comparator/sense amp
936

ICL7650
chopper stabilised opamp

936

75162AN
GPIB bus transceiver

936

AD7525TD
12 bit A2D converter

936

N6264N
64k 8k x 8 static ram

936
Order

RC4195N
dual tracking regulator +/-15V
936

AD654JN
voltage to frequency converter
936

AD620AN
instrumentation amplifier

936

7555IPA
cmos 555


936

SG531 4MHz oscillator


936

SG531 12MHz oscillator


936

SG531 8MHz oscillator


936

907-979 7922 single opto isolator

936

RS307-064, quad opto isolator



936

LM566CN
voltage controlled oscillator
936
Order

Switch, Slide, DPDT


937

Switch, DIL, 4W


937

Relay, 6V, SPST


937

Switch, rotary, hexadecimal, 0 to F

937

Switch, pcb mounting


938

2716
16k (2K x 8) eprom

939

CA3130
cmos opamp


940

CA3140E
cmos opamp


940

KF351
JFET opamp


940
Order

ICM7209IPA
Clock generator

940
Order

RS305-478(AC1165)


940

MC3357P
Motorola NBFM IF IC

940

Reed relay



940

Panel socket for microphone

941
Order

7 segment display, Kingsbright SC03-11HWA
941

BT152-400R
scr


941

2N3904
transistor


941

2N3903
transistor


941
Order

74LS251N
Data selector, tristate o/ps

942

DS75161N
GPIB bus transceiver

942

LF356N
Wideband JFET opamp

942

RC4194N
Dual tracking regulator, adjustable
942

DP8304N
bi-directional transceiver, tristate
942

INS8208BN
?dynamic ram controller?

942
Order

DS75160A
GPIB bus transceiver

942

DIN plugs 5W 270deg


943

DIN plugs 6W 270deg


943

Switch, toggle, SPDT


944

Switch, toggle, SPDT 317-099

944

Switch, slide, SPDT


944

Switch, slide, DPDT, pcb mounting

944

Switch, slide, 3 position


944

Connector, 4W, pcb mounting

944

LED, Blue, 12000mcd, OSUB5111P, rapid 55-2482
945

LED, Blue/clear, 2200MCD, rapid 55-1662
945

LED, Green/clear, 4500MCD, rapid 55-1668
945

LED, Red/clear, 4500MCD, rapid 55-72-8992
945

Pressure transducer


946

Data sheet for above


946

Fuseholder, pcb mounting


946

EXO34L 16MHz oscillator


946

74LS688N
8 bit magnitude comparator
946

74HC04
hex inverter, cmos

946
Order

74LS573
octal tristate noninverting latch
946

UMC UM5100
Voice processor 
947

7 segment display, dual, Kingsbright DC56-11EWA
947

ADDAC80
12 bit D2A converter

947

IDC connector, 50W


947 
Order

IDC connector, 20W


947 
Order

Crystal, cylindrical, 32kHz?

947 
Order

IDC box header, 14W, pcb mounting, extract levers
948

1M miniature skeleton pot, with shaft

948

Switch, decade, miniature


949

Relay, 6V, miniature, pcb mounting

950

Resistor networks


950

79L12 voltage regulator, 12V

951

10 pin IC and transistor socket

951

Terminal block, pcb mounting

952

D connector, 25W, male, IDC

952

10k skeleton pot, ceramic


952

D connector, 15W, female, IDC

953

D Connector, 25W, female, pcb mounting
953

D connector, 15W, male, solder bucket

953

Capacitor, trimmer


953

DIN connector, 5W, 180deg,  90deg pcb mounting
954

RCA phono socket, 90deg pcb mounting

955

SG531P 4MHz oscillator


956

MAX680
+5V to +/-10V converter

956

7 segment display, quad, intelligent, 0.16”, red
957

LED, Red, 5mm


957

Switch, multipole pushbutton, pcb mounting
958

Keyswitch with key, pcb mounting

958
Order

Piezo sounder, pcb mounting, external drive
958

Piezo sounder, external drive

958

Optosensor, reflective


958

Temperature sensor, SLS


958

IDC box header, 50W


959

IDC box header, 20W


959

IDC socket, 40W


959

Bridge rectifier


960

Switch, Reed, changeover contacts

960

Relay, SPDT 3A, 6V, RS346-637

960

Reed operating coil


960
Order

HPIB connector, 90deg pcb mounting

961

IDC transistion header


961
Order

PCF8574B
I/O expander, IIC

962

L297
stepper motor controller

962

UCN5804B
Stepper motor driver

962

ZTX689B
transistor


963

LP2950CZ-5
5V regulator 100mA

963
Order

Thermistor, NTC, 10k, disc


963

Switch, DIL, 4 pole 2W


963

100k trim pot, 10turn


963

MCP2120-TP
Infrared encoder/decoder
963

Crystal, 20MHz


964

Crystal, 4MHz


964

Crystal, 10MHz


964

PCF8583P
Clock/calendar

965

SP8629DP



965

PCF8591P
A2D and D2A converter, IIC
965

ADC0804LCN
8 bit A2D converter
965

HEF4753VP
Universal timer module

965

7660S
Switched capacitor voltage converter
965

ICL7135CPI
4.5 digit A2D converter

966

ICL7106CPL
3.5 digit A2D converter

966

ICM7217AIPI
4 digit up/down counter LED driver
966

SCN2674BC4N40
Video controller
966

7107
3.5 digit A2D converter

966

D7220D, NEC
crt Graphics controller
967

ICL7235A
VFD driver?


967

TMS9914ANL
GPIB interface ic
967

7486
quad 2 i/p XOR

967

ICM7211AIPL
4 digit LCD driver
967

TDA1097
Bucket brigade delay line

967

PCF8584P
Bus controller, IIC

967

74191
binary synchronous up/down counter
967

7216A
8 digit multifunction counter/timer
967

PCF8573P
Clock/calendar with power fail
968

ICL7224
4.5 digit A2D converter LCD driver
968

TBA2800
IR preamplifier

968

LE50CZ 
regulator, 5V 100mA

969

2SR330C 
Regulator


970

Resonator, 455kHz


970

Resonator, 500kHz


970

L2269, Ferrule set 1000-micron miniature range
971

STAR-CMB-06, Buzzer, 6V, PCB mount

971

Video/audio transmitter 2.4GHz

972
Verify content

Video/audio receiver 2.4GHz

972
Verify content

RF600T EasyRadio IC RS232 controller

972
Verify content

Audio/video TX module, 2.4GHz

972

Microswitch, miniature


973

Pins, pcb?



973

Thermistor, 1k miniature bead

973

D connector, 25W, male, 90deg pcb mounting
973

IDC header, 36W, pcb mounting

973
Order

HD64A180ROP  cpu


974

HN27C64G-15, General Purpose Dynamic RAM
974

PALC22V10, Reprogrammable CMOS

974

HM50464P-15, DRAM


974

DC Jack socket, 3mm


974

24LC64 

EEPROM, 64k bit
975

24C64C-FU

EEPROM, 64k bit
975

24LC256 

EEPROM, 256k bit
975

24LC02 

EEPROM, 2k bit
975

24LC04 

EEPROM, 4k bit
975

TL7705
Power supply supervisor

975

ST485CN
RS485 interface IC

975
HEF4076BP
quad D type with tristate o/ps
975

MC14025BCP Triple 3–Input NOR Gate

975

MC14072BCP dual 4 i/p OR

975

MC14078BCP 8 input NOR

975

MC14011BCP Quad 2−Input NAND Gate
975
GAL16V8-25QNC


975

AY-1-1370



975

AM9513PC



975

MC6845
CRT controller

975

AM2812DC



975 
Order

AM9519APC



975 
Order

AM9322PC



975

ICM7218DIJI
 uP compatible 8 digit LED driver
975

AM9517A-5 PC multimode DMA controller
975

TMS9901NL
programmable systems interface
975

MC6843P
Floppy disk controller, nmos
975

CDP6818E
CMOS RTC with ram (like MC146818)
975

TMS9902ANL uart for tms9900

975

SAD1024A
bucket brigade analogue delay line
975

PX0-1000
crystal oscillator

975
MJ2841
plessey 64 word fifo

975

SFH610
opto isolator


975

AD536AJH



975

PAL20RA10



975

PAL16L8



975

PAL16R8



975

PAL16R6



975

PAL16R4



975

DS1307
RTC, IIC i/f


975

HEF4539



975

HEF4585
cmos 4 bit magnitude comparator
975

Z8470ABI
Z80 DART


975

TLE2022CP



975

TLE2072CP
opamp


975

MK4801AN-1 
1k x 8 static ram
975

IM6402IPL



975 

AD7581JN
8 bit 8 channel A2D converter
975

NE5539
High frequency opamp

975

AM25LS252IPC 8 bit “equal to” comparator
975

TCA650



975

74LS684
8 bit magnitude comp, totem pole o/p 
975

MCM6264CP35 
8k x 8 static ram
975

IMS1420s55
4k x 4 static ram

975

Plug 1mm red


976

Plug 1mm black


976

Socket 1mm red


976

Socket 1mm black


976

LM741CH metal can


977

Fuse 3A 600V HRC


977

Microswitch, sub miniature


978

Pen, plotter



979

LED, red, flashing, 8mm


980

LED, red, 3mm, 


981

LED, green, 3mm


981

LED, yellow, 3mm


981

Piezo sounder, kingstate KPE-222

982

Switch, pushbutton, n/o


982

Reedswitch magnet


983

Reedswitch



983

TO3 mica & fixings (2nd user)

984

Piezo shock transducer F731-973

985

Thumb Joystick, analogue, 10k pots plus switch
986

Thumb Joystick pcb for above

986

MF10CN
Dual universal switched cap filter
987

Thermistor, miniature bead, 47k RS151-158
987

LM3914N



987

TC9400CPD
Volt to Freq/Freq to Volt converter
987

LTC1063



987

LED, green, rs586-453


988

LED, red, rs586-447


988

Link, shorting, 2mm


989

74S40 rs308-095


989

WN1013 Siliconix special FET

989

BC337



989

BC212L



989

2N2646



989

BD131



989

Delay line, PAL 64us


990

Delay line, luminance, 270ns

990

Modulator, UHF


990

IDC, 26W cable plug


991

Crystal socket


992

ICM7240IJE



992

Switch, decade thumbwheel

992

500R cermet trimmer (min)


993

2k cermet trimmer (min)


993

500K preset pot, 270 deg cermet

993

BD135
NPN transistor 45V 

994

BD136
PNP transistor 45V 1.5A

994

BD437
NPN transistor 45V 4A

994

Grommet, rubber, sealed


995

Knob, pushon, skirt, black 20mm

996

Knob, pushon, skirt, black 20mm

997

Knob, pushon, skirt, black 20mm

998

Knob cap for 676, blue


998

Knob cap for 676, green


998

Knob cap for 676, yellow


998

Knob cap for 676, red


998

Knob cap for 676, grey


998

Knob cap for 676, black (gloss)

998

Socket, 2mm, red


999

Socket, 2mm, black


1000

Socket, 2mm, white


1001

Plug, 2mm, black, 444-472


1002

Probe clip, red


1003

Probe clip, black


1003

Potentiometer, linear plunger actuation rs317-780
1003

Order

Resistor, carbon film, high stability, 0.5W, 110(
1004
Resistor, carbon film, high stability, 0.5W, 200(
1004

Resistor, carbon film, high stability, 0.5W, 360(
1004

Resistor, carbon film, high stability, 0.5W, 510(
1004

Resistor, carbon film, high stability, 0.5W, 620(
1004
Resistor, carbon film, high stability, 0.5W, 750(
1004

Resistor, carbon film, high stability, 0.5W, 1k6(
1005

Resistor, carbon film, high stability, 0.5W, 2k4(
1005

Resistor, carbon film, high stability, 0.5W, 3k6(
1005

Resistor, carbon film, high stability, 0.5W, 4k3(
1005

Resistor, carbon film, high stability, 0.5W, 5k1(
1005

Resistor, carbon film, high stability, 0.5W, 6k2(
1005

Resistor, carbon film, high stability, 0.5W, 7k5(
1005

Resistor, carbon film, high stability, 0.5W, 13k(
1006

Resistor, carbon film, high stability, 0.5W, 16k(
1006

Resistor, carbon film, high stability, 0.5W, 30k(
1006

Resistor, carbon film, high stability, 0.5W, 43k(
1006

Resistor, carbon film, high stability, 0.5W, 62k(
1006

Resistor, carbon film, high stability, 0.5W, 75k(
1006

Resistor, metal oxide, 0.5W, 12(

1007

Resistor, metal oxide, 0.5W, 18(

1007

Resistor, metal oxide, 0.5W, 180(

1007

Resistor, metal oxide, 0.5W, 220(

1007

Resistor, metal oxide, 0.5W, 270(

1007

Resistor, metal oxide, 0.5W, 430(

1008

Resistor, metal oxide, 0.5W, 470(

1008

Resistor, metal oxide, 0.5W, 1k8(

1008

Resistor, metal oxide, 0.5W, 5k6(

1008

Resistor, metal oxide, 0.5W, 6k8(

1008

Resistor, metal oxide, 0.5W, 33k(

1008

Resistor, metal oxide, 0.5W, 68k(

1008

Resistor, metal oxide, 0.5W, 1M(

1008
Resistor, carbon, 0.5W, 430k(

1009
Resistor, wirewound, 23W, 1(

1009
Resistor, 0.1%
100k(

1010
Resistor, 0.1%
500k(

1010

Resistor, 0.1%
1M(

1010

Relay, pcb mounting, F103 291

1011

BTW68-600, Thyristor 600V 30A

1011

Metal cased resistor, R20 5W 5%

1011

TICP106D
silicon-controlled rectifier

1011
Order

1k preset, 10 turn


1012

5k preset, 10 turn


1012

MC3423P1
Overvoltage sensing IC 

1012

Socket, Chassis, microphone type, 4W

1013

Socket, Chassis, microphone type, 7W

1013

Toko coils/inductors, shielded, assorted
(Box 1)
1014

Toko coils/inductors, shielded, assorted
(Box 2)
1015

Toko coils/inductors, shielded, assorted
(Box 3)
1016

Toko coils/inductors, shielded, assorted
(Box 4)
1017

Toko coils/inductors, shielded, assorted
(Box 5)
1018

IDC box header, 16W, pcb mounting, 90deg, ears
1019

IDC cable skt, 16W 
(Box 1)

1020

IDC cable skt, 16W 
(Box 2)

1021

Strain gauge, AL compensated,

1022

Centronics connector 36W pcb mounting socket
1022

D connector, 25W, IDC, female

1023

D connector, 25W, IDC, male

1024

BNC plugs



1025

D connector, 37W, male, solder bucket

1026

IDC DIL 24W



1027

UGN3020T hall effect IC


1028

25K pot, linear, with mains on/off switch

1029

500K pot, linear, with mains on/off switch
1029

Resistor pack, DIL, Beckman 898-3-R100
1030

Hex pillar



1031

Heatsink, TO3, TO220, etc. assorted (Box 1)
1032

Heatsink, TO3, TO220, etc. assorted (Box 2)
1033

T03, T0220 PGT mounting kits, assorted
1034

Z80A
cpu


1035

Z8
microcontroller, piggyback rom
1035

8750CJ



1035

HEF4738V
IEEE488 I/F ic

1035

Z80PIO



1035

Z8430



1035

COM8251A
UART
?

1035

HN482764G-2


1035

DG538DJ
video multiplexer

1035

IM6402IPC
uart


1035
HM6264
64k static ram

1036
Order 

UCN5810AF
open drain driver with serial i/f
1036

14021BCP



1036

ICM7556IPD
NE556 timer


1036

TC4427CPA
Dual mosfet driver 1.5A

1036

LTC1288CN8
12 bit A2D converter SO8
1036

6116
16k 2k x 8 static ram

1036
Order

M5M51008AP-70L static ram

1036 
Order

K6T1008
static ram


1036 
Order

GM76C256C1L-70 static ram

1036 
Order

ICM7209IPA
Timebase generator

1036 
Order

REF102AP
Precision voltage reference
1036

RC4200N
Analogue multiplier

1036

LM301N
Opamp


1036

AD509H
high speed fast settling opamp
1036

AD518JH
wideband opamp

1036

ICL8013
Analogue 4 quadrant multiplier
1036

DG307ACJ
quad analogue switch

1036

DG200ACJ
quad analogue switch

1036

HI200
quad analogue switch

1036

Relay, FEME MKP A 001 46 05

1037

Relay, 5V, Erni Rel14-A1-5.5 SPDT

1037
Relay, 12V, Reed, metal case SPDT National
1038

Relay, 24V, Reed, metal case SPDT SDS relays
1038

Relay, 12V, 8A, SPNO, Zettler 692-07-54k
1039

Relay, 24V, ST1-DC24V AR201404 pcb mounting c/o
1040

Socket, 4mm, panel mounting, Red

1041

Socket, 4mm, panel mounting, Black

1042

SD/MMC card breakout board with socket
1043

SD/MMC micro card breakout board with socket
1043

D headers, pcb mounting


1044

DIN connectors, pcb mounting

1044

IDC headers, pcb mounting
(Box 1)
1045

IDC headers, pcb mounting
(Box 2)
1046

IDC headers, pcb mounting
(Box 3)
1047

7 segment display CS-513

(Box 1)
1048

7 segment display CS-513

(Box 2)
1049

7 segment display ELS-505RWB

1050

7 segment display SC-05


1051

7 segment display LT547R


1052

7 segment display LN516RK

1053

MJ2955
PNP transistor 60V 15A TO3
1054

2N3771
NPN transistor 40V 30A

1055

MJH6285
PNP darlington, 60V 20A

1055

MJ11015
PNP darlington, 120V 30A

1056

MJ11016
NPN darlington, 120V 30A

1056

Fuse, Wikman, 100mA


1057

Fuse, Wikman, 200mA


1057

Fuseholder, Wikman


1057

MUX-16 analogue multiplexer

1058

BR1941M
Baudrate generator

1059

COM8116T 
Dual baud rate generator

1059

AM2910DC
Microprogram controller 

1060

IM6100IPL
PDP8 compatible microprocessor
1060

D8035LC IC Microcontroller

1060

MAB8031-12P
Microcontroller
1060

MC68A701L
Microcontroller (UV erase)

1060

MK3801-N
Z80 STI (Serial, Timer, Interrupt control)
1061

S1602P
UART


1061

DP8212N
8 bit I/O port


1062

IDM29705JC
16 word x 8 bit dual port register file/ram
1062

N82S09N
576 bit bipolar ram, 64 x 9 bits
1062

P8251A
PCI, programmable comms i/f
1063

P8253-5
PIT, programmable interval timer
1063

P8243
I/O expander


1063

MK3883-4
Z80 DMA


1064

Z8410PS
Z80 DMA


1064

6116
16k (2k x 8 static ram

1065

6264
64k (8k x 8) static ram

1065

D8085
8085 CPU


1066

P8255A-5
Programmable I/O ic

1066

MC/EF6821P Peripheral interface adapter
1067

Icebreaker PICs


1068
TL431CZ voltage reference/shunt regulator TO92
1069

CCTV camera, pcb, monochrome

1070

ADLX202JQC-1 accelerometer

1070

AA single cell holder, pcb mounting
(Box 1)
1071

AA single cell holder, pcb mounting
(Box 2)
1072

Socket, ZIF, 24W


1073

Socket, lock & eject, 40W


1074

Distance Sensor, IR, analogue output, rapid 58-0986
1075

Distance Sensor, IR, digital output, rapid 58-0982
1075

Pressure pad, resistive, 6mm dia, rapid 50-3702
1075

PIR module, rapid 61-1516


1076

Switch, panel mount, SPST, dual
(Box 1)
1077

Switch, panel mount, SPST, dual
(Box 2)
1078

BR100
Diac


1079

133
Diac (equivalent to BR100)

1079

T2850D
Triac, 400V 8A, TO220AB

1079

BRY39
Programmable Unijunction

1079

BTX18-400
Thyristor 400V 1A TO39

1080

C106D
Thyristor, 400V, 4A, TO225
1080

C106D1
Thyristor, 400V, 4A, TO202
1080

TIC116M
Thyristor, 9A 800V

1080

TICP106D
Thryristor, 400V, 2A, TO92

1081

TICP206D
Thryristor, 400V, 1.5A, TO92
1081

BTY79-400R
Thyristor 400V 10A stud mounting
1082

THY500-12
Thyristor, 500V 12A

1082

Stud mounting thyristors (Assorted)

1082

PN2222A
NPN transistor 30V 800mA

1083

2N4922
NPN transistor 60V 1A


1083

BC107
NPN transistor 



1083

Order
BC108
NPN transistor



1083

BC109
NPN transistor



1083

BC117
NPN transistor 120V 50mA

1083

BC184L
NPN transistor



1083

TIP41C
NPN transistor 100V 6A

1083
ZTX300
NPN transistor



1083

2N4037
PNP transistor 60V 1A

1084

BC178
PNP transistor (complement to BC108)
1084
BC179
PNP transistor (complement to BC109)
1084
BC214L
PNP transistor



1084
BC477
PNP transistor, low noise


1084

BC478
PNP transistor, low noise


1084

BFX88
PNP transistor 40V 150mA


1084
TIP42C
PNP transistor –100V 6A

1084

ZTX751
PNP transistor 60V 2A


1084
2N2160
Unijunction transistor


1085

AC128
Germanium transistor

1085
VN10KM
Mospower FET N channel, 60V 200mA
1085

Order

3 way transistor socket


1085

Heatsink Transistor Mount Kit for TO-220
1085
Knob, pointer, classic bakelite
(Box 1)
1086

Knob, pointer, classic bakelite
(Box 2)
1087

Switch, mains on/off pushbutton

1088

Fuse, thermal


1089

Sleeve, rubber, small
(Box 1)

1090

Sleeve, rubber, small
(Box 2)

1091

Sleeve, rubber, large


1092
Crocodile clip cover, red


1093

Crocodile clip cover, black 


1094

Crocodile clip, miniature, with red cover

1095

Crocodile clip, miniature, with black cover
1095

BNC plug



1096 

Test probe, screw on, red


1097

Test probe, screw on, black

1097

Crocodile clip, medium


1097

LCD, 3.5 digit RS587-298


1098

LCD, 3.5 digit RS588-572


1099

LED bar display


1100

LED dot matrix 1” high 7 x 5

1100

LED display filter


1100

Z8442
Z80 SIO


1101

Z8470
Z80 DART


1101

MC68661PB
SIO (6800/68000 bus)

1102

Z80A
CPU


1103

Z80 CTC
MK3882N


1104

Z8420
Z80 PIO


1105

R6551P
6502 ACIA (SIO)

1106

R6522
6502 VIA (PIO)

1106

R6502
6502 CPU


1107

L78S09
9V regulator


1108

L7805ACV
Positive voltage regulator

1108

Relay, NEC, MR24-24S4


1109

Relay, OMRON G2R-1112P-FD-V-US

1110

EVOX metallised polypropylene film capacitor, 100nF
1111

KONEK metallised polypropylene capacitor, 0.1µF
1111

(TDA)2085A
RS303-220 Phase control ic (DS4608)
1112

DS8629
RS307-474 150MHz prescaler
1112

MC14566BCP Timebase Generator (div by 50 or 60)
1112

2N3702
PNP transistor 25V 500mA

1113
Order

2N5060
Sensitive gate thyristor TO92 200V 0.8A
1113

BC327
PNP transistor 45V 500mA


1113

BPW41
Photodiode, IR

1113
Order

H24A1
Optocoupler


1114

680nF box polyester capacitor

1115

Crystal, 11.059MHz


1116

Crystal, 12MHz


1116

Crystal, 22.18MHz


1116

Crystal, 25MHz


1116

Crystal, 26.790MHz


1116

Crystal, 27.245MHz


1116

Relay, FBR20 21D05, Fujitsu, miniature pcb
1117

AT89S4051-24, 8051 microcontroller
1001
1118

AT89S2051-24, 8051 microcontroller
1018
1119

2N5454
Dual n channel fet



1120

VP0808
Mospower FET P channel, -80V 1A
1120

Circuit breaker, thermal, 2A

1121

Circuit breaker, thermal, 1A

1122

MCP2551-I/P CAN interface

1123

100nF tantalum capacitor


1124

220nF tantalum capacitor


1124

1uF tantalum capacitor


1125

2u2F tantalum capacitor


1125

1uF tantalum capacitor


1126

10uF tantalum capacitor


1126

22uF tantalum capacitor


1126

47uF tantalum capacitor


1126

100uF tantalum capacitor


1126

10nF polyester capacitor (mullard)

1127

15nF polyester capacitor (mullard)

1127

22nF polyester capacitor (mullard)

1128

33nF polyester capacitor (mullard)

1128

47nF polyester capacitor (mullard)

1129

68nF polyester capacitor (mullard)

1129

100nF polyester capacitor (mullard)

1130

150nF polyester capacitor (mullard)

1130

220nF polyester capacitor (mullard)

1131

330nF polyester capacitor (mullard)

1132

470nF polyester capacitor (mullard)

1132

1uF polyester capacitor (mullard)

1133

1u5F polyester capacitor (mullard)

1133

2u2F polyester capacitor


1134

10uF polyester capacitor


1134
Order

Mica capacitor, 5pF


1135

Mica capacitor, 47pF, 5%


1135

Mica capacitor, 200pF, 1%


1135

Mica capacitor, 560pF, 1%


1135

Mica capacitor, 1000pF, 1%

1135

Mica capacitor, 1800pF, 1%

1135

Mica capacitor, 4700pF, 1%

1135

Mica capacitor, 6800pF, 1%

1135

Mica capacitor, 8200pF, 1%

1135

1nF ceramic capacitor


1136

1n5F ceramic capacitor


1136

2n2F ceramic capacitor


1137

3n3F ceramic capacitor


1137

4n7F ceramic capacitor


1138

10nF ceramic capacitor


1139

47nF ceramic capacitor


1139

100nF ceramic capacitor


1140

Switch, joystick 4 position RS516-031

1141

Switch, joystick, 8 direction RS516-306

1141

Switch, joystick, 8 direct + centre pb RS249-3381
1141

Switch, float Farnell 177-5048

1142

MC6FD014-30P1 socket IDC, 109-9237

1143

MC6FD016-30P1 socket IDC, 109-9238

1144

100(F 35V radial electrolytic capacitor

1145

FT0102A
Triac, logic level, 400V TO-92
1146

3 Level LED R,Y,G, Kingsbright L-4060XH/1|1Y1GD
1146

DC power socket DC10A 2.1mm

1147

DC power plug DCPP1 2.1mm

1148

Jack socket, 3.5mm, stereo, panel mtg

1149

Switch, pushbutton, push to make n/o, larger
1150

Switch, pushbutton, SPST, momentary, square
1151

Fuse holder, panel mount, 20mm, 10A, 250V (RC)
1152

Fuse holder, Finger RLS, 32mm, 10A, 250V (RC)
1153

Switch, pushbutton, SPST, on/off, black

1154

Switch, pushbutton, SPST, round, red

1155

Switch, pushbutton, SPST, square, red

1156

Switch, On/Off, rectangular, black, DPDT
1157

Switch, On/Off, large red illuminated lever, 12V
1158

Fuse, 20mm, 50mA


1159

Fuse, 20mm, 100mA, (A/S) and (Q/B)

1159

Fuse, 20mm, 80mA, (A/S)


1160

Fuse, 20mm, 120mA, (A/S)

1160

Fuse, mains, 25mm, 2A


1160
Fuse, mains, 25mm, 3A


1161

Fuse, mains, 25mm, 5A


1161

Fuse, mains, 25mm, 13A


1161

Fuse, Hitachi CTVs, 20mm, 3, 15A

1161

Fuse, 20mm, 500mA, (A/S)

1162

Fuse, 20mm, 1A, (Q/B)


1162

Fuse, 20mm, 1.25A, (A/S)


1163
Fuse, 20mm, 1.6A, (A/S) and (Q/B)

1163
Fuse, 32mm, 2A, (A/S)


1164

Fuse, 32mm, 2.5A, (A/S)


1164

Fuse, 32mm, 3A, (A/S)


1164

Fuse, 32mm, 10A


1165

Fuse, 32mm, 15A


1165

Fuse, 32mm, 16A


1165

Fuse, 32mm, 60mA, (Q/B)


1166

Fuse, 32mm, 100mA, (Q/B)

1166

Fuse, 32mm, 150mA, (A/S)

1166

Fuse, 32mm, 250mA, (A/S)

1166

Fuse, 32mm, 500mA, (A/S)

1167
Fuse, 32mm, 600mA, (Q/B)

1167
Fuse, 32mm, 600mA, (A/S)

1167

Fuse, 32mm, 750mA, (A/S)

1168

Fuse, 32mm, 850mA, (A/S)

1169

Fuse, 32mm, 1.25A, (A/S)


1169

Fuse, 32mm, 1.5A, (A/S)


1169

Fuse, 32mm, assorted values (A/S) and
(Q/B)
1170
Fuse, mains, HRC, 20mm, 100mA

1171

Fuse, mains, HRC, 20mm, 250mA

1171

Fuse, 20mm, 2A, (A/S)


1171

Fuse, 20mm, 50mA (Q/B)


1172

Fuse, 20mm, 125mA, (Q/B)

1173

Fuse, 20mm, 250mA


1173

Fuse, 20mm, 630mA, (Q/B)

1173
Fuse, 20mm, 2A


1174

Fuse, 20mm, 2.5A


1174

Fuse, 20mm, 3.15A


1174

Fuse, 20mm, assorted values

1174

Fuse, 20mm, 3.15A, (Q/B)


1175

Fuse, 20mm, 10A, (Q/B)


1175

Fuse, 20mm, 2A, (S/B)


1175

Fuse, 20mm, 2.5A, (S/B)


1175

Fuse, 20mm, 3.15A, (S/B)


1175

Fuse, 20mm, 250mA


1176

Fuse, 20mm, 500mA, (S/B)

1176

Fuse, 20mm, 315mA, (Q/B)

1176

Fuse, 20mm, 500mA, (Q/B)

1176

Fuse, 20mm, 500mA, (A/S)

1176

Fuse, 20mm, 50mA, (S/B)


1177

Fuse, 20mm, 100mA, (S/B)

1177

Fuse, 20mm, 250mA, (S/B)

1177

Fuse, 20mm, 500mA, (S/B)

1177

Fuse, 20mm, 1A, (S/B)


1177

Fuse, 20mm, 1.6A, (S/B)


1177

Fuse, 20mm, 5A, (S/B)


1177

Fuse, 20mm, 6.3A, (S/B)


1177

Fuse, 20mm, 50mA, (Q/B)


1178

Fuse, 20mm, 100mA, (Q/B)

1178

Fuse, 20mm, 250mA, (Q/B)

1178

Fuse, 20mm, 500mA, (Q/B)

1178

Fuse, 20mm, 1A, (Q/B)


1178

Fuse, 20mm, 1.6A, (Q/B)


1178

Fuse, 20mm, 2A, (Q/B)


1178

Fuse, 20mm, 3.15A, (Q/B)


1178

Fuse, 20mm, 5A, (Q/B)


1178

Fuse, 20mm, 6.3A, (Q/B)


1178

LITTELFUSE, BLS003, fast acting, I.R. 10,000A
1179
74S04
hex inverter


1180

74LS390
dual decade counter

1180

74LS221
dual nonretriggerable monostable
1180

74LS175
quad D type flipflop

1181

7400
quad 2 i/p NAND

1181

7410
triple 3 i/p NAND

1181

7408
quad 2 i/p AND

1182

7432N
quad 2 i/p OR

1182

74126
quad bus buffer, tristate o/ps
1182
SN5405J
Hex inverter, open collector o/ps
1182
CD4007ubp
dual complementary pair plus inverter
1183

LF351 
op amp RS308-528

1183
LF353 
wideband JFET opamp RS308-534
1183
LF355
op amp


1183
RS306-982
op amp


1183

304-201
quad op amp


1183
TL507C
7 bit single slope A2D conveter
1183
74LS126
quad bus buffer, tristate o/ps
1184

NE5080
High speed FSK modem transmitter
1184
NE5081
High speed FSK receiver

1184

7438
quad 2 i/p NAND open collector o/ps
1184

LF398N
Monolithic sample & hold

1184

TL074
Opamp, FET, quad

1184

NE567N
tone decoder/phase-locked loop
1184

RS305-478
NE555N


1184
Order

RS303-422
Octal darlington

1184 
Order

DAC0832LCN 
8 bit D2A converter
1185

AT89C2051-24
8051 microcontroller
1185

IRFD110
N channel power mos 100V 1A DIL4
1185

LM3909
LED flasher IC

1186

HEF40244
cmos octal buffer

1186

CD4511
BCD to 7 segment latch/decoder/driver
1186

CD4066
transmission gate

1186

74LS259
8 bit addressable latch

1186
Order

TL084CN 
Opamp, FET, quad, RS304-201
1186

CD4021
8 stage static shift register

1186

74HCT86
quad 2 i/p XOR

1186

MC14529BCL dual 4 channel analogue data selector
1187

CD4069
Hex inverter


1187

CD40374
Octal latch (74HC374 equivalent)
1188

CD4050
Hex buffer, non-inverting

1188

CD4518
Dual BCD up counter

1189

74LS166
8-bit shift register

1189

HCF4538
dual monostable multivibrator
1189

CD4538
Dual precision monostable

1189 
Order

CD4040
12 stage binary counter

1190

TL084
Opamp, FET, quad

1190

74LS393
dual 4-bit binary counter

1190

CD4017
5 stage Johnson counter

1191

CD4023
3 x 3 i/p NAND gate

1191

CD4001
4 x 2 i/p NOR gate

1191

CD4528
Dual monostable

1191

CD4520
Dual Binary up counter

1191
Order
CD4070
quad XOR gate

1191

ZVP2110A
Mospower FET



1192

ZVP3306A
Mospower FET



1192

BS170
N channel mospower, 60V 500mA
1193

BC549
NPN transistor

1194

BC559
PNP transistor 30V, 100mA
1195

2N2907A
PNP transistor 60V 200mA TO18
1196

2N2905A
PNP transistor 60V 600mA TO5
1197

2SA1943
PNP transistor

1198

2SC5200
NPN transistor

1198

LE33CZ
voltage regulator 3V3 100mA 2% TO92
1199

UA78M33C
positive-voltage regulator

1199

FZT605
NPN 120V 1.5A SOT223

1200

Fuse, Wireended, pcb 5A fast

1201

Fuse, Wireended, pcb 5A slow

1201

RS analogue ammeter, MAX: 100(A 259-561
1202

General purpose film capacitor, 6800pF, 2.5%
1203

Capacitor, Electrolytic, Radial, 0.1(F, 50V
1204

Capacitor, Electrolytic, Radial, 0.22(F, 50V
1205

Capacitor, Electrolytic, Radial, 0.47(F, 50V
1206
Capacitor, Electrolytic, Radial, 1(F, 50V

1207
Capacitor, Electrolytic, Radial, 1(F, 63V

1208
Capacitor, Electrolytic, Axial, 1(F, 63V

1209

Capacitor, Electrolytic, Radial, 2.2(F, 63V
1210
Capacitor, Electrolytic, Axial, 2.2(F, 63V

1211
Capacitor, Electrolytic, Axial, 4.7(F, 63V

1212
Capacitor, Electrolytic, Radial, 33(F, 35V
1213
Capacitor, Electrolytic, Axial, 47(F, 63V

1214

Capacitor, Electrolytic, Radial, 47(F, 16V
1215
Capacitor, Electrolytic, Radial, 100(F, 25V
1216

Capacitor, Electrolytic, Radial, 100(F, 63V
1217

Capacitor, Electrolytic, Axial, 100(F, 16V, (Box 1)
1218

Capacitor, Electrolytic, Axial, 100(F, 16V, (Box 2)
1219

Capacitor, Electrolytic, Radial, 220(F, 35V
1220
Capacitor, Electrolytic, Radial, 470(F, 16V
1221

Capacitor, Electrolytic, Radial, 470(F, 25V, (Box 1)
1222
Capacitor, Electrolytic, Radial, 470(F, 25V, (Box 2)
1223

Capacitor, Electrolytic, Radial, 1000(F, 35V, (Box 1)
1224

Capacitor, Electrolytic, Radial, 1000(F, 35V, (Box 2)
1225

Capacitor, Electrolytic, Radial, 1000(F, 35V, (Box 3)
1226

Capacitor, Electrolytic, Axial, 2200(F, 16V, (Box 1)
1227

Capacitor, Electrolytic, Axial, 2200(F, 16V, (Box 2)
1228
Capacitor, Electrolytic, Radial, 2200(F, 25V, (Box 1)
1229

Capacitor, Electrolytic, Radial, 2200(F, 25V, (Box 2)
1230

Capacitor, Electrolytic, Radial, 2200(F, 35V, (Box 1)
1231

Capacitor, Electrolytic, Radial, 2200(F, 35V, (Box 2)
1232

Capacitor, Electrolytic, Axial, 4700(F, 25V, (Box 1)
1233

Capacitor, Electrolytic, Axial, 4700(F, 25V, (Box 2)
1234

77A suppression coil, 10000(H, 0.3A

1235

68MH2200R series inductor

1235
BC508A, Transistor, NPN


1236

KSD1616AYTA, NPN Epitaxial Silicon Transistor
1237

VN2222LL-G, N-Channel MOSFET, 60V

1238

2N3055H
NPN transistor, T03

1238
Resistor, metal film, 0.5W 22K(

1239

Resistor, metal film, 0.5W 27K(

1240

Resistor, metal film, 0.5W 33K(

1241

Resistor, metal film, 0.5W 39K(

1242
Resistor, metal film, 0.5W 47K(

1243

Resistor, metal film, 0.5W 56K(

1244

Resistor, metal film, 0.5W 68K(

1245

Resistor, metal film, 0.5W 82K(

1246

Resistor, metal film, 0.5W 100K(

1247

Resistor, metal film, 0.5W 120K(

1248

Resistor, metal film, 0.5W 150K(

1249

Resistor, metal film, 0.5W 180K(

1250
Resistor, metal film, 0.5W 220K(

1251

Resistor, metal film, 0.5W 270K(

1252
Resistor, metal film, 0.5W 330K(

1253

Resistor, metal film, 0.5W 390K(

1254

Resistor, metal film, 0.5W 470K(

1255

Resistor, metal film, 0.5W 560K(

1256

Resistor, metal film, 0.5W 680K(

1257

Resistor, metal film, 0.5W 820K(

1258

Resistor, metal film, 0.5W 1M(

1259

Resistor, metal film, 0.5W 470(

1260

Resistor, metal film, 0.5W 910(

1261

Resistor, metal film, 0.5W 1K(

1262

Resistor, metal film, 0.5W 2K(

1263

Resistor, metal film, 0.5W 2K4(

1264

Resistor, metal film, 0.5W 10K(

1265

H8800VA, rocker switch, SPST, black

1266

R13-234I-05, (on-off-on) rocker switch, SPDT, black
1267
R13-234D-05, (on-off-on) rocker switch, SPDT, black
1268

R13-502, (off-on) pushbutton switch, SPST, black
1268
CW1300-1, tilt switch


1269
PKG.M0.8GL.LG, circular connector, panel, grey
1269

PAG.M0.8GL.AC65N, cable mount plug, 8 contacts
1269
DCPP1, DC power connector, 5A, 9.5mm, cable Mt
1269
CN02178, DC power connector, panel mount
1270

9-0160483-1, crimp terminal, female, red
1271

HLMP-CW12-X1000, LED, 5mm, 15DEG, white
1272

FCL-P5DR078G03B12WCCI, LED, 50DEG, RGB
1272
FCL-P115R078G03B12WCCI, LED, 115DEG, RGB
1272

LM317T, IC voltage regulator, ADJ +1,2,37V
1273

LM317LZ, IC voltage regulator, ADJ +1,2,37V
1273
GP75AAHHB, battery, NIMH, 2/3AA

1274
504.413, control knob, setscrew, black

1275

ZHR, connector housing, 4-way

1275

B4B-ZR(LF)(SN), header, top entry, 4-way
1275

CLB300CTP lens cap & SPC125 mount for LED
1275

Sammy screws


1275

L-56BGD, LED, green, 5mm, flashing

1276

L-56BYD, LED, yellow, 5mm, flashing

1276

L-483SRSGW, LED, red/green, flat top, 5mm
1276

L-813ID, LED, red, T3, 10mm, 20mA, 2V
1277

L-819EGW, LED, tri-colour, 10mm

1278
HRS4, relay, PCB SPCD, DC 5V

1279

CD15ED470JO3F, mica capacitor, 47pF

1280

Capacitor, silvered mica, 100pF

1280

RXE050, poly switch, radial, 0.5A

1281
RXE090, poly switch, radial, 0.9A

1281

RUE110, poly switch, radial, 1.1A

1281

Ceramic capacitors, 22 – 82pF

1282

Ceramic capacitors, 100 – 330pF

1283

Ceramic capacitors, 330 – 820pF

1284
Ceramic & polyester capacitors, 1 – 10nF
1285

Capacitors, ceramic, polyester, etc, (assorted)
1286

Capacitors, 33 – 68nF & 330 – 470nF

1287

Capacitors, polystyrene (assorted values)
1288

Wirewound resistors, 0.5W (assorted values)
1289

Wirewound resistors, 1W (assorted values)
1289

Wirewound resistors, 2W (assorted values)
1290

IC sockets, 14, 20 & 28-way

1291

Dual-in line low profile sockets, 8-way

1292

BF981, transistor


1293

Resistor, metal film, 0.5W 10(

1294

Resistor, metal film, 0.5W 12(

1295

Resistor, metal film, 0.5W 15(

1296

Resistor, metal film, 0.5W 18(

1297

Resistor, metal film, 0.5W 22(

1298

Resistor, metal film, 0.5W 27(

1299

Resistor, metal film, 0.5W 33(

1300

Resistor, metal film, 0.5W 39(

1301

Resistor, metal film, 0.5W 47(

1302
Resistor, metal film, 0.5W 56(

1303

Resistor, metal film, 0.5W 68(

1304

Resistor, metal film, 0.5W 82(

1305

Resistor, metal film, 0.5W 100(

1306

Resistor, metal film, 0.5W 120(

1307

Resistor, metal film, 0.5W 150(

1308

Resistor, metal film, 0.5W 180(

1309

Resistor, metal film, 0.5W 220(

1310
Resistor, metal film, 0.5W 270(

1311
Resistor, metal film, 0.5W 330(

1312
Resistor, metal film, 0.5W 390(

1313

Resistor, metal film, 0.5W 560(

1314

Resistor, metal film, 0.5W 680(

1315

Resistor, metal film, 0.5W 820(

1316

Resistor, metal film, 0.5W 1K2(

1317

Resistor, metal film, 0.5W 1K5(

1318

Resistor, metal film, 0.5W 1K8(

1319

Resistor, metal film, 0.5W 2K2(

1320

Resistor, metal film, 0.5W 3K3(

1321

Resistor, metal film, 0.5W 3K9(

1322

Resistor, metal film, 0.5W 4K7(

1323

Resistor, metal film, 0.5W 5K6(

1324

Resistor, metal film, 0.5W 6K8(

1325

Resistor, metal film, 0.5W 8K2(

1326

Resistor, metal film, 0.5W 12K(

1327

Resistor, metal film, 0.5W 15K(

1328

Resistor, metal film, 0.5W 18K(

1329

3386W-101LF, trimmer, 100(

1330

T0916SDAAA, switch, SPND, 140-690

1330
570-0100-132F, LED, 2mm, PCB, R-Y-G
1330

JF15CP2G, tactile switch, round, blue

1330

Led, yellow, 3mm


1330
CR-MS-2, knob, soft touch, splined shaft

1331
SW03238, miniature push button, SPST, off-on, black
1332

SW03239, miniature push button, SPST, off-on, red
1332

SW03240, miniature push button, SPST, off-on, green
1332

SW03241, miniature push button, SPST, off-on, yell
1332

NIMH battery, rechargeable, 30AAAM, 1.2V, 300mAh
1333

NIMH battery, rechargeable, 75AAH, 1.2V, 750mAh
1333

NIMH battery, rechargeable, 380AFH, 1.2V, 3700mAh
1333

NIMH battery, NT60AAAH


1333

DC motors



1334

Capacitor, Electrolytic, Radial, 4.7(F, 63V
1335

Capacitor, Electrolytic, Radial, 22(F, 50V
1336

Capacitor, Electrolytic, Radial, 47(F, 25V
1337

Capacitor, Electrolytic, Radial, 47(F, 50V
1338

Capacitor, Electrolytic, Radial, 100(F, 16V
1339

Capacitor, Electrolytic, Radial, 1000(F, 25V
1340

Capacitor, Electrolytic, Radial, 1000(F, 35V
1341
Capacitor, Electrolytic, Radial, 2200(F, 25V, (Box 1)
1342
Capacitor, Electrolytic, Radial, 2200(F, 25V, (Box 2)
1343
Capacitor, Electrolytic, Radial, 4700(F, 16V
1344

B37575G6102J, capacitor, ceramic, 1nF, 50V
1345

B37986G5103J, capacitor, ceramic, 10nF, 50V
1345

MCCHU5220J6, capacitor, ceramic, 22nF, 50V
1346

Capacitor, ceramic, 10pF


1347

MCCHU7101J5, capacitor, ceramic, 100pF, 50V
1347

2222 680 10129, capacitor, ceramic pl, 12pF, 100V
1348

2222 680 10189, capacitor, ceramic pl, 18pF, 100V
1348

2222 680 34229, capacitor, ceramic pl, 22pF, 100V
1348

2222 680 34279, capacitor, ceramic pl, 27pF, 100V
1348

2222 680 34339, capacitor, ceramic pl, 33pF, 100V
1348

ICBU8472K6, capacitor, ceramic, 4.7nF, 50V
1348

BC213L, transistor, PNP, T0-92

1348
Trimmer capacitors


1349

MJ-355W, socket, 3.5mm jack

1350

ABS-210-RC, speaker, 1W, 8(, 350Hz – 20,000Hz
1351
K 36 WP, waterproof speaker driver, 8( 1W RMS
1351
Winslow, 2.54mm pitch vertical 8-way DIP socket, 5A
1352

RS PRO 80dB, continuous internal piezo buzzer
1352

MJ-069, phone audio connector, 2.5mm, panel Mt
1352
Relay, RS 344-451, 6VDC 80( -+ 10%

1353

Relay, RS 346-621, 12VDC 400(

1353

Relay, MR24-24S4 NEC, 1200(, 15-pin

1353
R13-502, pushbutton switch, 12.7mm, SPST, off-(on)
1354

MCDTS2-4W, tactile switch, 7.3mm

1354

MCDTS2-4R, tactile switch, 7.3mm

1354

B3WN-6002, switch, SPND, PCB

1354
1550265, pushbutton switch, SPDT, on-(on)
1354
R13-527C2-02-BB, pushbutton switch, SPST
1355

Switches, (assorted)


1356

Power Transistors (assorted)

1357

3386W-1-102LF, trimmer, 1K(

1358
3386W-1-103LF, trimmer, 10K(

1358
3386W-1-104LF, trimmer, 100K(

1358
3386W-1-105LF, trimmer, 1M(

1358
SOMC 1603, 16-pin SMD isolated resistor, 470(, 2%
1359

Resistor pack, DIL, Beckman 898-3-R330
1360

Bridge rectifiers


1361
KS, polystyrene film capacitor, 8.2nF

1362

40361, NPN transistor, 30V, 700mA

1363

Jack connector, 2.5mm, (TRRS), cable mount
1364

Universal DC and jack connectors (various sizes)
1364

Jack plug, ¼ inch, mono


1365

RCA phono plug, cable mounting, white

1366

Z0842004PSC, serial input/output controller
1367
RS6402
uart


1367

ICL7106CPL
3.5 digit A2D converter

1367

M27C64A-20F1, IC EPROM, 64 k-bit, parallel
1368
M5L2764K, erasable and electrically reprog’ ROM
1368


27128-25, NMOS 128K (16K x 8) UV EPROM
1368
A80486DX-33, gold ceramic processor chip
1368
DM74181N, TTL 4 Bit Arithmetic Logic Unit DIP24
1369
DM74150, Data selectors/multiplexers

1369
DM74LS139N, Decoder/multiplexer

1369
SN74ALS573CN, Octal D-type transparent latch
1369

SN74LS147N, Priority encoders

1369
SN741N, Quad 2-input positive NAND gate
1370

SN743N, Quad 2-input positive NAND gate
1370

SN74185AN, Binary to BCD code converter
1370
LM1889N, TV video modulator

1370

DM74160AN, 2-line digital multiplexer

1370
CD74HCT251E, 8-input multiplexer, 3 state
1370

DM74180N, Parity generator/checker, TTL/H/
1370

MV601BA, Remote control receiver

1370

DM74194N, 4-bit directional universal shift register
1370

74LS164N, Serial-in parallel-out shift register     
1370

MCP3008, 4-channel/8-channel 10-bit A/D converter
1370

ZN428E-8, D/A converter, single 8-bit, bipolar
1370

XR2211CP, FSK demodulator/tone decoder
1370
MAX275ACPP, Continuous band pass low pass filter
1370
SSM2110, True RMS-to-DC converter

1370
LMF100CIN, Dual switched capacitor filter
1370
7432, Quad 2-input OR gate

1371
7447, BCD to seven-segment decoder/driver
1371

SL486, Infrared remote-control preamplifier
1372

TDA3047, Infrared receiver

1372

SN7451N, AND-OR invert gates

1372
SN7483AN, 4-bit binary full adder, fast carry
1372

MC14076B, 4-bit D-type register (3-state outputs)
1372

MC14008BCP, 4-bit full adder

1372

MC14071BCP, Quad 2-input OR gate

1372

MC14073BCP, Triple 3-input AND gate

1372

LM2917N-8, Frequency to voltage converter
1372

INA111AP, Instrumentation amp (hi-speed FET-in)
1372

AD9523, Jitter cleaner and clock generator (14-diff)
1372

Attenuator,
coaxial,
3dB

1373

Attenuator,
coaxial,
6dB

1373

Attenuator,
coaxial,
12dB

1373

Capacitor, Electrolytic, Radial, 2200(F, 35V
1374

Capacitor, Electrolytic, Axial, 4700(F, 25V, (Box 1)
1375

Capacitor, Electrolytic, Axial, 4700(F, 25V, (Box 2)
1376
Capacitor, Electrolytic, Axial, 4700(F, 25V, (Box 3)
1377

WIMA, Capacitor, Polyester, Radial, 1nF

1378

RCA,
phono plug,
black

1379

RCA,
phono plug,
red

1380
Fuse holder,
6.3 x 32 mm


1381

Fuse holder,
6.3 x 32 mm


1382

Wire contact for fuse holder, 6.3 x 32 mm
1382

LED, RGB, Piranha


1383

LED, flat top, 2 mm, red


1383

LED, red, diffused, rectangular

1384

LED, HLMP-CB37-RU000, 5 mm, 30DEG, blue
1385
LED, L-53PBC, 
5 mm, water clear blue
1386

LED, L-7113QBC-D, 
5 mm, water clear blue
1386

LED, L-1513SFC-F,
5 mm, clear red
1387

LED,

5 mm, bright yellow trans
1387

LED,

5 mm, water clear white
1387

LED, 55-1904, 5 mm, rainbow, clear

1388

LED, 55-0670, 5 mm, diffused multi-coloured
1388

LED, 5 mm, full colour, water clear, 60°

1388

LED, 55-0370, 3000MCD, 10 mm, ultrabright red
1389

LED, 247-1527, 10 mm RGB

1389

LED, 10 mm, yellow


1389

LED, NSPW 300BS, 3 mm, ultra-white, 25°
1389

LED, 228-5988, 5 mm, red


1389

LED, 5 mm, red, flashing


1389

LED, 586-475, 
5 mm, red

1390
LED, 587-232, 
5 mm, constant current
1390

LED, 587-844,
5 mm, yellow

1390

LED, 587-822
5 mm, high intensity, red
1390

LED, 586-396, 
red

1390

LED holder for through hole LED

1390

LED, 

5 mm, clear blue
1391
LED, 

5 mm, clear red
1391

LED, 

5 mm, clear white
1391

LED, assorted colours and sizes

1392

78-0770, Mercury tilt switch

1392

LED holder for through hole LED, 16 mm
1393

KSS 5R1, Sectional grommet

1394

Open grommet, panel: 7 mm, cable: 9 mm
1395

Open grommet, panel: 20 mm, cable: 16 mm, (Box 1)
1396
Open grommet, panel: 20 mm, cable: 16 mm, (Box 2)
1397

Sleeve, rubber, various sizes

1398

1N5338B, surmetic 40 silicon Zener diode, 5W
1399

Electrolytic Capacitors (Assorted)

1400

18-pin dual in-line socket (Box 1)

1401

18-pin dual in-line socket (Box 2)

1402

Makaswitch wafers


1403

Majaswitch mechanism


1404

Sub-miniature interlocking switches

1404

Knob, brushed aluminium, 15 mm diameter
1405

Knob, brushed aluminium, 18 mm diameter
1405

Knob, brushed aluminium, 22 mm diameter
1405

Knob, brushed aluminium, 28 mm diameter
1405

Knob, brushed aluminium, 35 mm diameter
1406

Knob, brushed aluminium, 38 mm diameter
1406

Knob, aluminium and plastic, 19 mm diameter
1407

Knob, aluminium and plastic, 24 mm diameter
1407

Knob, aluminium and plastic, skirt, 36 mm diameter
1407

Knob, aluminium and plastic, skirt, 43 mm diameter
1407

Knob, plastic, black, 29 mm diameter

1407

Knob, plastic, black/silver, lever, 20 mm diameter
1407

Knob, plastic, black, lever, 13 mm diameter
1408

Knob, plastic, black, skirt, 15 mm diameter
1408

Knob, plastic, black, skirt, 20 mm diameter
1408

Knob, plastic, black, 21mm diameter

1409

Knob, PKL, plastic, black, 499-703, 0.5” diameter
1409

CCTV camera, pcb, monochrome

1306

Microswitch, roller lever, Z-15GW22-B

1306

Microphone, electret


1306

Microphone, electret, on suction cup

1306

Wire



1307

N/a



1308

PIC16F628

PIC microcontroller
1312

PIC17C44

PIC microcontroller
1312

PIC16F877

PIC microcontroller
1312

PIC16F871

PIC microcontroller
1312

PIC16F84

PIC microcontroller
1312

PIC16F873

PIC microcontroller
1312

PIC16F629

PIC microcontroller
1312

PIC16F872

PIC microcontroller
1312

PIC16F875

PIC microcontroller
1312

PIC16C74A

PIC microcontroller
1312

PIC16F84 (SO8)
PIC microcontroller
1312

AD654JN voltage to frequency converter
1330
Plug, stackable, 4mm, Red


1353

Plug, stackable, 4mm, Black

1353

2N3819 jFET



1356

2N3904



1356

Flexinol wire



1358
D8251AFC



531
P8088 CPU



531
GF0E1A1139 Opto thingy


531
MJE210



531
Switch latch and mounting assembly for interlocking
532
PIC16F877-04
PIC microcontroller
1281

Find item
PIC16F873-04
PIC microcontroller
1281

Find item
Fixed Value Resistors : CARBON FILM, 0.25W, 5%








