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Objectives 

Using Packet Capturing tools and network monitoring tools.  
Tasks 

1. Use Nmap to scan 2.  
Required Resources 

· PC with Ubuntu 16.0.4 LTS installed in a VirtualBox or VMware virtual machine. (Alternatively, Any Linux Platform) 
· Internet Connection to refer the outcomes o References: https://nmap.org/ 
 
Task 1 

· Login as User Cisco. 
· Go to Terminal and Type the following commands and examine  o To do that we are using Nmap.  
 Network Mapper, or Nmap, is an open source utility used for network discovery and security auditing. Administrators also use Nmap for monitoring hosts or managing service upgrade schedules.   Nmap determines  
· what hosts are available on a network,  
· what services are running,  
· what operating systems are running,  • What packet filters or firewalls are running? 
o So, basically if you could get all the above details using Nmap, you could get few information which could be used later in performing attacks or mitigating attacks.  
 
 
 
 
 
 
 
 
 
 
 
 
· Commands to execute o Step 1: 
 nmap localhost 
(This is a scan performed to get information about the services that are bound to the localhost) 
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o Step 2: 
 Replace the above command with your IP Address and other hosts (if connected/ else ignore) in your network to check the outcomes. 
Type the command you used to find out your host IP Address 
ifconfig
Type the command you used to scan after finding your host IP Address
Nmap 10.0.2.15 
Record the outcomes of the above command here 
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 o Step 3: Analyse the outputs/outcomes from Step 1 and 2 and record your reflections. (Hint: Analyse what is the difference between local host and ip address of the host, If ports displayed are different, Why is it different? etc (not limited to the hints)) 
	 Commands are the same  outputs were the same.
Local host command ran abit faster. No ports were listed differently ( see screenshot above).
 
 
 


· Step 4: Why is the nmap scan only scans the first 1000 ports? What will be the command to scan all the ports? 
	 Command to scan all ports is nmap ( IP address)-p-
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· Step 5: Scan the UDP Ports 
· nmap –sU localhost 
(This is a scan performed to get information about the UDP ports and to execute this command you need root privileges. So, try) 
· sudo nmap –sU localhost 
Record the outcomes of the above command here (Hint: what Uports could you find open through your scan) 
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· Step 6: From the above outcomes select any ports which is open 
 sudo nmap –p137 localhost  
(Change the port number 137 to any port which you found as open in the previous step (5).) 
Record the outcomes of the above command here (Hint: Is the port open or closed? Why? Also, record the use of –p command) 
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 Port is now closed. So assuming that the -p closes it.
 
 
· Step 7: Try other port related commands and record its purpose. 
· sudo nmap –pportnumber host_ip 
· sudo nmap –pportnumber_startrange-portnumber_endrange host_ip 
· sudo nmap –pportnumber,portnumber host_ip 
· not limited to the above (Do a google search, refine your search and find out other port related commands, Hint:nmap.org) 
Record the outcomes of the above commands here
1) scan specific ports  
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2) scan a range[image: ]
3) Scan multiple ports
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 Good site that I visited for nmap https://securitytrails.com/blog/top-15-nmap-commands-to-scan-remote-hosts
· Step 8: Detecting the version is a very important part of information gathering. Try to find out the version.  nmap –sV localhost  
Record the outcomes of the above commands here  
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· Step 9: Try other commands to detect other versions and record its purpose. 
· Command to identify the Operating System version 
Record the outcomes of the above commands here 
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· Command to identify the Service Version 
Record the outcomes of the above commands here 
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Learnings from tutorials so far:  
Part 1 (Packet Tracer, Host Machines) 
· Build a home Network  
· Understand and configure IP Address 
· Use Ping/ Trace route Utility to check the connection status 
· Use ipconfig /all command to determine the MAC address of a Windows computer on an Ethernet network. 
· Analyze a MAC address to determine the manufacturer. 
· Analyze the Wired and Wireless Network connection. 
· Analyze Address Resolution Protocol (ARP). 
· Connect to a Wireless Router and configure the basic settings in a wireless router and add security features. 
· Use nslookup command to understand the url to ip conversion. 
· Configure basic connectivity settings in Intermediate devices (Switch/ Router). 
· Work with SBA Packet Tracer Files/ environment 
· Configure ftp, web, email, dns, ntp and aaa Servers Part 2 
· Set up a virtual lab environment  
· Troubleshooting the virtual lab environment 
· Working with virtual machines 
· Authentication, Authorization and Accounting 
· Threats and Vulnerabilities – Using NMAP 

	2 	n.kaliyamurthy@uwtsd.ac.uk                                                                                                           
 
	2 	n.kaliyamurthy@uwtsd.ac.uk                                                                                                           
 
image3.png
$ nmap localhost

cisco@ubunt

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:08 CST
Nmap scan report for localhost (127.6.0.1)

Host is up (0.000037s latency).

Not shown: 997 closed ports

PORT  STATE SERVICE

22/tcp open ssh

23/tcp open telnet

631/tcp open ipp
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cilsco@ubuntu:~$ nmap 10.0.2.15

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:15 CST
Nmap scan report for 10.0.2.15

Host is up (0.000037s latency).

Not shown: 998 closed ports

PORT  STATE SERVICE

22/tcp open ssh

23/tcp open telnet

Nmap done: 1 IP address (1 host up) scanned in .19 seconds
ciscogubuntu:~$ nmap localhost

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:16 CST
Nmap scan report for localhost (127.6.0.1)

Host is up (0.000036s latency).

Not shown: 998 closed ports

PORT  STATE SERVICE

22/tcp open ssh

23/tcp open telnet

Nmap done: 1 IP address (1 host up) scanned in ©.14 seconds
cisco@ubuntu:~$ I
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/clsco@ubuntu:~5 nmap 10.0.2.15 -p-

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:20 CST
Nmap scan report for 10.0.2.15

Host is up (0.000037s latency).

Not shown: 65533 closed ports

PORT  STATE SERVICE

22/tcp open ssh

23/tcp open telnet

Nmap done: 1 IP address (1 host up) scanned in 2.31 seconds
cisco@ubuntu:~$ I
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cisco@ubuntu:~$ sudo nmap -sU localhost
[sudo] password for cisco:

starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:32 CST
Nmap scan report for localhost (127.0.6.1)

Host is up (0.6000040s latency).

Not shown: 997 closed ports

PORT STATE SERVICE

68/udp  open|filtered dhcpc

631/udp open|filtered ipp

5353/udp open|filtered zeroconf

Nmap done: 1 IP address (1 host up) scanned in 2.74 seconds
cisco@ubuntu:~$ i
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cisco@ubuntu:

$ sudo nmap -p5353 localhost

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:35 CST
Nmap scan report for localhost (127.6.0.1)

Host is up (0.000060s latency).

PORT STATE  SERVICE

5353/tcp closed mdns

Nmap done: 1 IP address (1 host up) scanned in ©.29 seconds
cisco@ubuntu:~$ i
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cisco@ubuntu:~$ sudo nmap -p5353 10.0.2.15

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:37 CST
Nmap scan report for 10.0.2.15

Host is up (0.000018s latency).

PORT STATE  SERVICE

5353/tcp closed mdns

Nmap done: 1 IP address (1 host up) scanned in ©.32 seconds
cisco@ubuntu:~$ i
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cisco@ubuntu:~$ sudo nmap -p 1-65535 localhost

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:43 CST
Nmap scan report for localhost (127.6.0.1)

Host is up (0.0000030s latency).

Not shown: 65533 closed ports

PORT  STATE SERVICE

22/tcp open ssh

23/tcp open telnet

Nmap done: 1 IP address (1 host up) scanned in 6.15 seconds
cisco@ubuntu:~$ i
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cisco@ubuntu:~$ sudo nmap -p 100,200 localhost

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:45 CST
Nmap scan report for localhost (127.6.0.1)

Host is up (0.000018s latency).

PORT  STATE SERVICE

100/tcp closed newacct

200/tcp closed src

Nmap done: 1 IP address (1 host up) scanned in ©.26 seconds
cisco@ubuntu:~$ i
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ciscogubuntu:~$ nmap -sV localhost

Starting Nmap 7.01 ( https://nmap.org ) at 2020-11-16 08:47 CST

Nmap scan report for localhost (127.6.0.1)

Host is up (0.000038s latency).

Not shown: 998 closed ports

PORT  STATE SERVICE VERSION

22/tcp open ssh OpenSSH 7.2p2 Ubuntu 4ubuntul (Ubuntu Linux; protocol 2.6)
23/tcp open telnet Linux telnetd

Service Info: 0S: Linux; CPE: cp

inux: linux_kernel

Service detection performed. Please report any incorrect results at https://nmap.org/submit/ .
Nmap done: 1 IP address (1 host up) scanned in 1.40 seconds
cisco@ubuntu:~$ i
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cisco@ubuntu:~$ uname -a
Linux ubuntu 4.4.@-24-generic #43-Ubuntu SMP Wed Jun 8 19:27:37 UTC 2016 x86_64 x86_64 x86_64 GNU/Linux
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cisco@ubuntu:~$ uname -
4.4.0-24-generic
cisco@ubuntu:~S i
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