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Tue Nov 14 10:25:00   Router1   Router>enable
Tue Nov 14 10:25:10   Router1   Router#configure terminal
Tue Nov 14 10:25:21   Router1   Router(config)#hostname Router1
Tue Nov 14 10:25:32   Router1   Router1(config)#interface gigabitEthernet 0/0
Tue Nov 14 10:25:43   Router1   Router1(config-if)#no sh
Tue Nov 14 10:25:54   Router1   Router1(config-if)#exit
Tue Nov 14 10:26:05   Router1   Router1(config)#interface gigabitEthernet 0/0.10
Tue Nov 14 10:26:16   Router1   Router1(config-subif)#encapsulation dot1Q 10
Tue Nov 14 10:26:27   Router1   Router1(config-subif)#description ***VLAN 10*** 
Tue Nov 14 10:26:38   Router1   Router1(config-subif)#ip address 192.168.10.1 255.255.255.0
Tue Nov 14 10:26:49   Router1   Router1(config-subif)#exit
Tue Nov 14 10:27:00   Router1   Router1(config)#interface gigabitEthernet 0/0.20
Tue Nov 14 10:27:11   Router1   Router1(config-subif)#encapsulation dot1Q 20
Tue Nov 14 10:27:22   Router1   Router1(config-subif)#ip address 192.168.20.1 255.255.255.0
Tue Nov 14 10:27:33   Router1   Router1(config-subif)#description ***VLAN 20*** 
Tue Nov 14 10:27:44   Router1   Router1(config-subif)#exit
Tue Nov 14 10:27:55   Router1   Router1(config)#interface gigabitEthernet 0/1
Tue Nov 14 10:28:06   Router1   Router1(config-if)#no shutdown 
Tue Nov 14 10:28:17   Switch1   Switch>en
Tue Nov 14 10:28:28   Switch1   Switch#conf t
Tue Nov 14 10:28:39   Switch1   Switch(config)#v
Tue Nov 14 10:28:50   Switch1   Switch(config)#hostname Switch1
Tue Nov 14 10:29:01   Switch1   Switch1(config)#vlan 10
Tue Nov 14 10:29:12   Switch1   Switch1(config-vlan)#name V10
Tue Nov 14 10:29:23   Switch1   Switch1(config-vlan)#vlan 20
Tue Nov 14 10:29:34   Switch1   Switch1(config-vlan)#name V20
Tue Nov 14 10:29:45   Switch1   Switch1(config-vlan)#exit
Tue Nov 14 10:29:56   Switch1   Switch1(config)#interface range fastEthernet 0/23
Tue Nov 14 10:30:07   Switch1   Switch1(config-if-range)#shutdown 
Tue Nov 14 10:30:18   Switch1   Switch1(config-if-range)#no shutdown 
Tue Nov 14 10:30:28   Switch1   Switch1(config-if-range)#exi
Tue Nov 14 10:30:39   Switch1   Switch1(config)#interface range fastEthernet 0/23-24
Tue Nov 14 10:30:50   Switch1   Switch1(config-if-range)#switchport mode trunk 
Tue Nov 14 10:31:01   Switch1   Switch1(config-if-range)#exi
Tue Nov 14 10:31:12   Switch1   Switch1(config)#interface gigabitEthernet 0/1
Tue Nov 14 10:31:23   Switch1   Switch1(config-if)#switchport mode trunk 
Tue Nov 14 10:31:34   Switch1   Switch1(config-if)#exit
Tue Nov 14 10:31:45   Switch1   Switch1(config)#interface range fastEthernet 0/23-24
Tue Nov 14 10:31:56   Switch1   Switch1(config-if-range)#channel-group 1 mode active 
Tue Nov 14 10:32:07   Switch1   Switch1(config-if-range)#exi
Tue Nov 14 10:32:18   Switch1   Switch1(config)#interface range fastEthernet 0/1-22
Tue Nov 14 10:32:29   Switch1   Switch1(config-if-range)#switchport mode access 
Tue Nov 14 10:32:40   Switch1   Switch1(config-if-range)#switchport access vlan 10
Tue Nov 14 10:32:51   Switch1   Switch1(config-if-range)#exit
Tue Nov 14 10:33:02   Switch1   Switch1#wr
Tue Nov 14 10:33:13   Switch2   Switch>enable
Tue Nov 14 10:33:24   Switch2   Switch#configure terminal
Tue Nov 14 10:33:35   Switch2   Switch(config)#hostname Switch2
Tue Nov 14 10:33:46   Router2   Router>enable
Tue Nov 14 10:33:57   Router2   Router#configure terminal
Tue Nov 14 10:34:08   Router2   Router(config)#hostname Router2
Tue Nov 14 10:34:19   Router2   Router2(config)#interface gigabitEthernet 0/0
Tue Nov 14 10:34:30   Router2   Router2(config-if)#no shutdown 
Tue Nov 14 10:34:41   Router2   Router2(config-if)#ip address 192.168.30.1 255.255.255.0
Tue Nov 14 10:34:52   Router2   Router2(config-if)#description ***VLAN 30***
Tue Nov 14 10:35:03   Router2   Router2(config-if)#exit
Tue Nov 14 10:35:14   Router2   Router2(config)#interface gigabitEthernet 0/1
Tue Nov 14 10:35:25   Router2   Router2(config-if)#no shutdown 
Tue Nov 14 10:35:36   Router2   Router2(config-if)#ip address 10.10.10.2 255.255.255.252
Tue Nov 14 10:35:46   Router2   Router2(config-if)#description ***Connection with Router1***
Tue Nov 14 10:35:57   Router2   Router2(config-if)#exit
Tue Nov 14 10:36:08   Router1   Router1(config-if)#ip address 
Tue Nov 14 10:36:19   Router1   Router1(config-if)#ip address 10.10.10.1 255.255.255.252
Tue Nov 14 10:36:30   Router1   Router1(config-if)#description ***Connection with Router***
Tue Nov 14 10:36:41   Router1   Router1(config-if)#exit
Tue Nov 14 10:36:52   Router1   Router1(config)#do sh ip rou c
Tue Nov 14 10:37:03   Router1   Router1(config)#router eigrp 1
Tue Nov 14 10:37:14   Router1   Router1(config-router)#no auto-summary 
Tue Nov 14 10:37:25   Router1   Router1(config-router)#network 192.168.10.0 0.0.0.255
Tue Nov 14 10:37:36   Router1   Router1(config-router)#network 192.168.20.0 0.0.0.255
Tue Nov 14 10:37:47   Router1   Router1(config-router)#network 10.10.10.0 0.0.0.3
Tue Nov 14 10:37:58   Router1   Router1(config-router)#passive-interface gigabitEthernet 0/0.10
Tue Nov 14 10:38:09   Router1   Router1(config-router)#passive-interface gigabitEthernet 0/0.20
Tue Nov 14 10:38:20   Router1   Router1(config-router)#end
Tue Nov 14 10:38:31   Router1   Router1#write 
Tue Nov 14 10:38:42   Router2   Router2(config)#do sh ip rou c
Tue Nov 14 10:38:53   Router2   Router2(config)#router eigrp 1
Tue Nov 14 10:39:04   Router2   Router2(config-router)#no auto-summary 
Tue Nov 14 10:39:15   Router2   Router2(config-router)#network 192.168.30.0 0.0.0.255
Tue Nov 14 10:39:26   Router2   Router2(config-router)#network 10.10.10.0 0.0.0.3
Tue Nov 14 10:39:37   Router2   Router2(config-router)#passive-interface gigabitEthernet 0/0
Tue Nov 14 10:39:48   Router2   Router2(config-router)#end
Tue Nov 14 10:39:59   Router2   Router2#write 
Tue Nov 14 10:40:10   Router2   Router2#show ip route 
Tue Nov 14 10:40:21   Router2   Router2#wr
Tue Nov 14 10:40:32   Router1   Router1#conf t
Tue Nov 14 10:40:43   Router1   Router1(config)#ip dhcp pool VLAN_10
Tue Nov 14 10:40:54   Router1   Router1(dhcp-config)#no ip dhcp pool VLAN_10
Tue Nov 14 10:41:05   Router1   Router1#wr
Tue Nov 14 10:41:15   Switch3   Switch>enable
Tue Nov 14 10:41:26   Switch3   Switch#configure terminal
Tue Nov 14 10:41:37   Switch3   Switch(config)#hostname Switch3
Tue Nov 14 10:41:48   Switch3   Switch3(config)#interface range fastEthernet 0/1-24, gi0/1-2
Tue Nov 14 10:41:59   Switch3   Switch3(config-if-range)#switchport mode access 
Tue Nov 14 10:42:10   Switch3   Switch3(config-if-range)#switchport access vlan 30
Tue Nov 14 10:42:21   Switch3   Switch3(config-if-range)#exit
Tue Nov 14 10:42:32   Switch3   Switch3(config)#vlan 30
Tue Nov 14 10:42:43   Switch3   Switch3(config-vlan)#name V30
Tue Nov 14 10:42:54   Switch3   Switch3(config-vlan)#exit
Tue Nov 14 10:43:05   Switch3   Switch3(config)#end
Tue Nov 14 10:43:16   Switch3   Switch3#copy running-config startup-config 
Tue Nov 14 10:43:27   Switch2   Switch2#show vlan brief 
Tue Nov 14 10:43:38   Switch2   Switch2#conf t
Tue Nov 14 10:43:49   Switch2   Switch2(config)#vlan 10
Tue Nov 14 10:44:00   Switch2   Switch2(config-vlan)#name v10
Tue Nov 14 10:44:11   Switch2   Switch2(config-vlan)#name V10
Tue Nov 14 10:44:22   Switch2   Switch2(config-vlan)#vlan 20
Tue Nov 14 10:44:33   Switch2   Switch2(config-vlan)#name V20
Tue Nov 14 10:44:44   Switch2   Switch2(config-vlan)#exit
Tue Nov 14 10:44:55   Switch2   Switch2(config)#interface range fastEthernet 0/23-24
Tue Nov 14 10:45:06   Switch2   Switch2(config-if-range)#switchport mode trunk 
Tue Nov 14 10:45:17   Switch2   Switch2(config-if-range)#channel-group 1 mode passive 
Tue Nov 14 10:45:28   Switch2   Switch2#show etherchannel summary 
Tue Nov 14 10:45:39   Switch1   Switch1>en
Tue Nov 14 10:45:50   Switch1   Switch1#show etherchannel summary 
Tue Nov 14 10:46:01   Switch1   Switch1#write 
Tue Nov 14 10:46:12   Switch2   Switch2#show etherchannel summary 
Tue Nov 14 10:46:23   Switch2   Switch2#write 
Tue Nov 14 10:46:33   Switch2   Switch2#show vlan brief 
Tue Nov 14 10:46:44   Switch2   Switch2#conf t
Tue Nov 14 10:46:55   Switch2   Switch2(config)#interface range fastEthernet 0/1-22
Tue Nov 14 10:47:06   Switch2   Switch2(config-if-range)#switchport mode access 
Tue Nov 14 10:47:17   Switch2   Switch2(config-if-range)#switchport access vlan 20
Tue Nov 14 10:47:28   Switch2   Switch2#show etherchannel summary 
Tue Nov 14 10:47:39   Switch2   Switch2#show vlan brief 
Tue Nov 14 10:47:50   Switch2   Switch2#write 
Tue Nov 14 10:48:01   Switch2   Switch2#write 
Tue Nov 14 10:48:12   Router1   Router1>en
Tue Nov 14 10:48:23   Router1   Router1#wr
Tue Nov 14 10:48:34   Router2   Router2>en
Tue Nov 14 10:48:45   Router2   Router2#wr
Tue Nov 14 10:48:56   Switch1   Switch1#write 
Tue Nov 14 10:49:07   Switch2   Switch2#we
Tue Nov 14 10:49:18   Switch2   Switch2#write 
Tue Nov 14 10:49:29   Switch3   Switch3#write 
Tue Nov 14 10:49:40   Router2   Router2>en
Tue Nov 14 10:49:51   Router2   Router2#conf t
Tue Nov 14 10:50:02   Router2   Router2(config)#ip dhcp pool VLAN30
Tue Nov 14 10:50:13   Router2   Router2(dhcp-config)#network 192.168.30.0 255.255.255.0
Tue Nov 14 10:50:24   Router2   Router2(dhcp-config)#default-router 192.168.30.1
Tue Nov 14 10:50:35   Router2   Router2(dhcp-config)#exit
Tue Nov 14 10:50:46   Router2   Router2(config)#ip dhcp excluded-address 192.168.30.1
Tue Nov 14 10:50:57   Router2   Router2#write 
Tue Nov 14 10:51:08   Router2   Router2#conf t
Tue Nov 14 10:51:19   Router2   Router2(config)#ip dhcp excluded-address 192.168.30.1 192.168.30.10
Tue Nov 14 10:51:30   Router2   Router2(config)#noip dhcp excluded-address 192.168.30.1
Tue Nov 14 10:51:41   Router2   Router2#cponf t
Tue Nov 14 10:51:52   Router2   Router2#conf t
Tue Nov 14 10:52:02   Router2   Router2(config)#no ip dhcp excluded-address 192.168.30.1
Tue Nov 14 10:52:13   Router2   Router2#wr
Tue Nov 14 10:52:24   Switch1   Switch1>show running-confing
Tue Nov 14 10:52:35   Switch1   Switch1>show
Tue Nov 14 10:52:46   Switch1   Switch1>show config
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