1. Ipconfig What is the IP address of the computer? 
192.168.1.10 and 192.168.1.11
2. What is the subnet mask of the computer?
255.255.255.0
3. Ping 192.168.1.11, was the ping successful?
YES
4. Click PCB (PC1)  Desktop  Command Prompt  a. Ipconfig What is the IP address of the computer?
192.168.1.10
5. What is the subnet mask of the computer? 
255.255.255.0
6. Ping 192.168.1.10 (Other PC’s IP Address) Was the ping successful? 
YES
