Note on drawing a basic shaped charge device with three parts: casing, HE charge and conical Liner

I suggest that when you draw the sketches for these three components you save time by :
· Draw casing first and save sketch
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· Draw Conical liner next and save sketch
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· Use these sketches as a reference to  draw the HE charge. Use the eraser tool to  eliminate unwanted lines
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To  display the results for only the liner:
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To display the 2D axisymmetric results as a 3D view:
[image: Graphical user interface

Description automatically generated]
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