First problem
On inside the hub as it wasn’t configured while its responsible for the connection from branch one to the hub
IP NAT Inside added to s0/1/0 in hub.


Second problem
Factory interface gig0/0/1 is down
Enabling it allows connection to network

Third problem
PC3 still unable to ping other PCs upon further inspection of factory switch it is clear that the network has not been added to the OSPF router.
Fixing allow the pc to ping other hosts

Fourth problem
PC5 ping is timed out. Upon further inspection pc5 default gateway is incorrect and needs to be changed to the correct one.
Default gateway changed

Fifth problem
PC6 and PC7 are unreachable. Bridge 2 is also unreachable. After investigation it is found that there was an incorrect IP in bridge 2 correcting this solved the issue.
IP for S0/1/0 on bridge 2 changed.

