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Verify HSRP is working as expected
Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-2, ping 172.16.0.1. Ping should not be successful    no  
 From PC-2, ping default gateway. Is it successful?  No
  From PC-2, ping 209.165.200.225. Is it successful? 
/no



