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Fire safety is a critical issue in the hotel industry, and there are various legal requirements that hotels must comply with to ensure the safety of their guests and employees. Customers consider safety and security while choosing a hotel. While planning a hotel’s safety, hoteliers typically adhere to municipal requirements (Chan and Lam, 2016, p. 202).

The 1990 Hotel and Motel Fire Safety Act initially compelled the hotel sector to modernise its fire-safety apparatus. Government staff had to book accommodations with full fire safety systems. (Miller, 1997, p.3). Hotels must comply with local building codes that provide minimum standards for fire safety in the design and construction of buildings. These codes set requirements for the installation of fire alarms, sprinklers, and smoke detectors, as well as the use of fire-resistant materials in the building's construction. Both in established and developing nations, fire poses a serious risk to people’s lives, buildings, property, and the environment.(Venkatesh, Puneet, and Muhammad, 2020).
The building and upkeep of fire exit pathways are among the stringent safety requirements that must be met in hotels in order to comply with modern standards of hotel fire risk management. (Flaherty, Hession and cuggy, 2016, pp. 529-530).

Hotels must have a fire prevention plan in place that outlines the procedures for preventing and responding to fires. This plan must include evacuation procedures, fire drills, and training for employees on fire safety. There should be sufficient emergency exits that are clearly marked and unobstructed. They must also have emergency lighting and exit signs that are visible in the event of a power outage.  Hotel must have fire extinguishers that are easily accessible and properly maintained. The location of the fire extinguishers must be clearly marked, and employees must be trained on how to use them. Many jurisdictions require hotels to be smoke-free, which can help prevent fires caused by smoking materials. Hotels must undergo regular inspections by local fire authorities to ensure that they are in compliance with all fire safety regulations.

Fire is a serious issue for human lives. The safety of people is seriously endangered by flames, and over the past few years, numerous spectacular fires in under-construction buildings have been documented ( Numan et al., 2020, p. 1704). Failure to comply with these legal requirements can result in fines, penalties, and legal liability in the event of a fire. It is essential for hotels to take fire safety seriously and implement all necessary measures to protect their guests and employees from harm.
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