Rhydian Preece
[bookmark: _Hlk69473446][image: ]

[bookmark: _Hlk56775645]
A report focussing on a:

Client Letter and Draft BEP



Prepared for:

Gavin Traylor

Created by:

Rhydian Preece

Word Count (Excluding BEP and References) – 1338 words

Date Completed:
April 29th, 2021
Table of Contents – Client Letter
									Page Number
1.0 Introduction                                                                                                                       4

2.0 What is BIM?                                                                                                                     4                                  

3.0 BIM Level 2                                                                                                                        5
3.1 Understand and follow the BIM protocol                                                        5
3.2 Create a Level 2-ready project plan                                                                  6
3.3 Collaborate and Co-ordinate                                                                              6
3.4 Share data securely                                                                                              7
3.5 Speak the same language                                                                                   7
3.6 Use COBie in your project                                                                                   7
3.7 Pass on the baton                                                                                                 7
3.8 Plan for a smooth handover                                                                               7
3.9 Information Delivery Cycle Diagram                                                                  7
4.0 References                                                                                                                            9


Table of Contents – BIM Execution Plan (BEP)
Page Number
BIM Execution Plan (BEP)                                                                                   11
1.0 Project Information                                                                                                             11

2.0 Management                                                                                                                         11
2.1	Roles, Responsibilities, & Authorities                                                                         11
2.2	Major Project Milestones                                                                                              13
2.3	PIM Deliverable Strategy                                                                                               13
2.4	Survey Strategy                                                                                                                13
2.5	Existing Legacy Data                                                                                                        14
2.6	Approval of Information                                                                                                 14
2.7	PIM Authorization Process                                                                                             14
 
3.0 Planning and Documenting                                                                                                  15
3.1	Project Implementation Plan                                                                                          15
3.2	Agreed Processes for Collaboration & Information Modelling                                 15
3.3	Task Information Delivery Plan                                                                                       15
3.4	Master Information Delivery Plan                                                                                  16


4.0 Standards, Methods, and Procedures                                                                                16
4.1	Volume Strategy                                                                                                                16
4.2	PIM Origin and Orientation                                                                                              16
4.3	File Naming Convention                                                                                                    17
4.4 	Object Naming                                                                                                                    17
4.5	Agreed Construction Tolerances                                                                                     18
4.6	Drawing Sheet Template                                                                                                   18
4.7	Annotations, Dimensions, Abbreviations, and Symbols                                              18
4.8	Attribute Data                                                                                                                     18

5.0 IT Solutions	                                                                                         20
5.1	Software Versions                                                                                                                20
5.2	Exchange Formats                                                                                                                20
5.3 Process and Data Management Systems                                                                         20


















[bookmark: _Hlk70536922]1.0 Introduction
The following letter will be to highlight my understanding of the requirements of BIM level 2. Firstly, one shall outline what BIM is and then go into further detail, explaining what BIM level 2 is and how information will be shared, coordinated, and managed through the appropriate standards.
2.0 What is BIM?
The Little Book of BIM (2021) define BIM as “BIM is a collaborative way of working underpinned by digital technologies. It uses a shared digital representation of an asset to facilitate design, construction, and operation processes to form a reliable basis for decisions. Greater efficiencies can be realized due to significant pre-planning during the design and construction phases, providing comprehensive information at handover stage”. A lot of people mistake BIM for being a software when it is not, it is a process that can improve the design and construction process in many ways. Nancy Reyes (n.d.) states that “there are five significant benefits of BIM in the design and construction process”. Those being:
· Cost and resource savings.
· Greater efficiency and shorter project lifecycles.
· Improved communications and coordination.
· More opportunities for prefabrication and modular construction.
· Higher quality results.
[image: ]
Figure 1 – BIM Layout of disciplines 
In my opinion, the best part about BIM is how it brings all the disciplines together. Instead of so many different drawings for each division, BIM lets everyone view the model with their respected design and allows the different workers to comment on whether something is wrong with the design or if they want something changed. Everyone will be working together and more efficiently. Communication is key in BIM which is why all disciplines are connected on the project and can communicate ideas or problems back to each other.
3.0 BIM Level 2
The diagram shown below is the one used by most professionals when trying to describe the different levels of BIM that we work at. For this project, we are working at BIM level 2 and this letter will indicate everything included at this level. BIM level 2 “involves developing building information in a collaborative 3D environment with data attached but created in separate discipline models” Designing Buildings 2021. This is a simple explanation of what BIM level 2 entails but there is much more in-depth information that can be outlined to explain it.
[image: ]
Figure 2 – The different levels of BIM
[bookmark: _Hlk70527628]All information in this following section highlighting the key elements of BIM Level 2 will be provided by Autodesk BIM 360 (c.2016) unless referenced otherwise. The key elements of BIM Level 2 are: 
· [bookmark: _Hlk70526532]Understand and follow the BIM protocol
· Create a Level 2-ready project plan
· Collaborate and Co-ordinate
· Share data securely
· Speak the same language
· Use COBie in your project
· Pass on the baton
· Plan for a smooth handover
3.1 Understand and Follow the BIM Protocol
The BIM Protocol is a legal addendum that is outlined in every government project contract which outlines the BIM requirements for the project. If someone wants to work on a project, they need to understand and comply with all the requirements. According to McPartland (2017), the “protocol puts in place specific obligations, liabilities and associated limitations on the use of those models”.
3.2 Create a Level 2-Ready Project Plan
The start of the project plan for BIM level 2 is done by responding to the Employer’s Information Requirements (EIR) under BS EN ISO 19650-1:2018 sec 5.5. The EIR is the information that that will be required by the employer from their internal team and from suppliers to develop the project and for the operation of the completed built asset. To respond to the EIR, a BIM Execution (BEP), Master Information Delivery Plan (MIDP), and a Task Information Delivery Pan (TIDP) must be prepared. Information on the MIDP and TIDP can be found in the appended BEP.
3.3 Collaborate and Co-ordinate
During the project’s life, team members will need to store, manage and exchange complex information, to do this you’ll have to use a CDE or Common Data Environment. A CDE is a digitally shared workspace where everyone involved in the project will store and exchange project data. The CDE is like a single data point and is intended to help people manage the project development process. The CDE however will require a structured approval process.
[image: ]
Figure 3 – Diagram of the CDE
Under BS EN ISO 19650-1:2018 sec 12, there are four states of the CDE being work in progress, shared, published, and archive. The work in progress state is used for information while it is being developed by its task team. Then information goes through a check/review/approve transition where the information is compared against the information delivery plan and against agreed standards, methods, and procedures for producing information. Then the shared state is to enable constructive and collaborative development of the information model within a delivery team. Another review stage where the information is compared against the relevant information requirements for coordination, completeness, and accuracy. The published state then allows information that has been authorized for use. The final stage is an archive where information is stored that has been shared and published during the information management process. Types of information that can be stored in the CDE are geometrical models, databases, schedules, pdf documents, scans, photos, videos, etc.
3.4 Share Data Securely 
It’s important that another standard is followed during the project life that ensures data is being shared securely. That standard is ISO 19650-5 provides technical security considerations on how to safely share project data, related to the nature of the client and project. This means that controls will be in place that ensures information is being shared securely. The software being used will provide controlled access to information stored in the CDE and can track and manage activity. 
3.5 Speak the Same Language
Everyone working on this project will know where all types of data live, what it is, and where to find it, and so a unified classification system will be put in place that provides a ‘common language’.
A system such as Uniclass will be put in place that is compatible with BIM Level 2.
3.6 Use COBie in Your Project 
COBie is a Construction-Operations Building Information Exchange.
COBie can be represented as a central spreadsheet where primarily non-graphical data can be securely stored, shared, and updated throughout the construction project. This information will eventually be passed onto the client to help support the operations and maintenance of the building. COBie can also be used to verify that your data meets the requirements of the project.
3.7 Pass on the Baton
Once the project has finished, the project data will be delivered back to the client. The project data can include an as-constructed Asset Information Model which is developed through the stages of the information delivery cycle. This type of model will include necessary information to help those managing and maintaining the building more efficiently.
3.8 Plan for a Smooth Handover
The Soft Landings policy outlined by the Government will ensure that the facility operational team is involved from the beginning of the project and will continue supporting them for a predetermined length of time post-handover. These are the people that will be managing and maintaining the building once it's finished, so by including them from the start of the project, they will know the building inside and out which will make the handover process much easier. 
3.9 Information Delivery Cycle Diagram
[image: ]
Figure 4 – Information Delivery Cycle Diagram
The diagram shown above outlines the information delivery cycle. This is at the heart of the BS EN ISO 19650-2:2018 sec 13 standard which provides a logical framework to produce information at different stages of the whole building lifecycle. The culmination is the Asset Information Model from which the operational phase of a building’s life can be optimised.
I sincerely hope this letter has provided you with sufficient information on BIM and given you confidence that we have a good understanding of the requirements of BIM Level 2 for this project. 
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[bookmark: _Hlk70536939]BIM Execution Plan (BEP)
This BEP template has been taken from Rossiter (2016). I have filled in information where possible to suit my project, however, some information is from the BEP template as this is only a draft. An EIR has not been given so some of the information stated will be in response to a given EIR.
Notes
This draft BIM Execution Plan (BEP) document has been structured using the headings described within BE EN ISO 19650-2:2018. 
Where information has been provided for guidance it will appear in blue.
Note:  Further clarification on any of the terms and definition used within this document can be found using the BRE BIM Terminology Tool, located here:  https://www.bre.co.uk/bim-terminology.jsp
1.0	Project Information
The information provided below shall be used throughout this project and included where appropriate on any deliverables produced.   The information provided in this table is put in place to satisfy the EIR.
	Project Name:
	Ysgol Bae Abertawe

	Project Number:
	5010

	Project Description:
	Delivery of a ‘state of the art’ infant school in Swansea

	Site Name:
	Ysgol Bae Abertawe

	Site Description:
	Omitted to protect personal information

	Facility Name:
	Ysgol Bae Abertawe

	Facility Description:
	Omitted to protect personal information


Table 1 - Project Information
[bookmark: _Hlk70536949]2.0	Management
This section of the BEP covers the requirements of BS EN ISO 19650-2, SECTION
2.1	Roles, Responsibilities, & Authorities
The purpose of this section is to define specific information management responsibilities.
Outlined below are the individuals and their respective organisations undertaking Information Management Responsibilities, as outlined within BS EN ISO 19650-2, TABLE
	Name
	Company
	Role
	Resources
	Contact Information

	Rhydian Preece
	RJP Ltd
	Client
	Client1
	Rhydpreece@outlook.com

	Jim Burton
	RJP Ltd
	Architectural
	Arch1
	Jimburton@outlook.com

	Gabriel Williams
	RJP Ltd
	Mechanical
	Mech1
	Gabwilliams@outlook.com

	Eric Morgan
	RJP Ltd
	Electrical
	Elect1
	Ericmorgan@outlook.com


Table 2 - Project Contacts
The following Employer’s Representative responsibilities apply to each individual as follows:
	Responsibility
	Resource

	Capture Key Decision Points
	Client1

	Produce Plain Language Questions
	Client1

	Capture Required Standards, Methods, and Procedures
	Client1

	Ensure the Appointment of a Project Information Manager
	Archx`1*

	Review the Supplier Information Exchanges against the EIR
	Client1


Table 4 - Employer's Representative Responsibilities
The following Project Information Manager responsibilities apply to each individual as follows:
	Responsibility
	Resource

	Enable Information Exchanges through a CDE
	**

	Maintain and Receive Information Into the Information Model
	Arch1

	Enable Integration and Coordination of Information
	Arch1

	Configure Information for Project Outputs
	Arch1

	Populate the Information Exchange Format
	Arch1

	Accept/Reject Information Exchanges
	Arch1


Table 5 - Project Information Manager Responsibilities
The following Project Delivery Manager responsibilities apply to each individual as follows:
	Responsibility
	Resource

	Assure Delivery of Information Exchanges
	Arch1

	Confirm Suppliers Ability to Deliver Information Requirements
	***

	Accept/Reject Information Exchanges
	Arch1


Table 6 - Project Delivery Manager Responsibilities

The following Lead Designer/Contractor responsibilities apply to each individual as follows:
	Responsibility
	Resource

	Coordinate Delivery of all Design Information
	Arch1

	Manage Information Development and Information Approvals
	Arch1

	Confirm Design Deliverables
	Arch1

	Overall Lead for Configuration Management
	Arch1

	Confirm Status and Approve Information for Issue
	Arch1

	Approve Design Changes Proposed to Resolve Clashes
	Arch1


Table 7 - Lead Designer/Contractor Responsibilities
The following Task Team responsibilities apply to each individual as follows:
	Responsibility
	Resource
Architectural
	Resource
Mechanical
	Resource
Electrical

	Production of Design Outputs Related to Specific Tasks
	Arch1
	Mech1
	Elect1

	Issue Approved Information
	**
	**
	**

	Direct the Production of Information in compliance with SMP
	Arch1
	Mech1
	Elect1

	Direct the Production of Information Using Agreed Systems
	Arch1
	Mech1
	Elect1

	Confirmation that Information is Suitable for Issue
	Arch1
	Mech1
	Elect1

	Manage Spatial Coordination on behalf of the Task Team
	Arch1
	Mech1
	Elect1

	Propose Resolution to Coordination Clashes
	Arch1
	Mech1
	Elect1

	Develop Constituent Parts of the Information Model
	Arch1
	Mech1
	Elect1

	Production of Project Outputs
	Arch1
	Mech1
	Elect1


Table 8 - Task Team Responsibilities
[bookmark: _Hlk70536960]*	This document confirms the successful deferral of an Employer’s Representative responsibility to the supply chain. This will be in response to the EIR.
2.2	Major Project Milestones
The purpose of this section is to confirm the project milestones.
Project Milestones will be indicated on the MIDP when made available. In line with the exchange of information in response to the EIR.
2.3	PIM Deliverable Strategy
The purpose of this section is to define what deliverables will be exchanges at each major project milestone.
Following review of the exchange of information requirements in response to the EIR, scheduled below are the deliverables that will be exchanged at each major project milestone.  Any additional items that have been included (shown in red) are to satisfy the Client's Strategic Purposes in response to the EIR.
	
	Brief & Planning
	Model Generation

	Graphical Models
	
	Native Discipline Models
Federated IFC Model

	Non-graphical Data
	
	Federated COBie

	Documentation
	BIM Execution Plan
	Site Plans, Floor Plans, Elevations, Sections, Door Schedule, Window Schedule


Table 9 - PIM Deliverable Strategy
[bookmark: _Hlk70536966]2.4	Survey Strategy
The purpose of this section is to identify how survey information will be received/exchanged.
All surveys undertaken on this project will utilise the origin and coordinate convention outlined within section 4.2, to the units and tolerances identified within section 4.6, and will be accessible to the authoring software identified within section 5.2.
Scheduled below are the intended surveys to be undertaken.
	Survey Method
	Delivery Format
	Details, Notes:

	Manual ‘Disto’ Survey
	DWG
	Layers to Comply with BS EN ISO 19650-1:2018 & Uniclass 2015

	
	
	


Table 10 - Survey Strategy
[bookmark: _Hlk70536977]2.5	Existing Legacy Data
The purpose of this section is to identify available existing asset data.
Following the review of existing documentation available scheduled within in response to the EIR, information will be extracted and formatted to suit integration into the information model.  
2.6	Approval of Information
The purpose of this section is to confirm the approval process when issuing information.
Prior to the issue of any information, the individual(s) responsible for confirming suitability and approval of information identified within section 3.1 will undertake the following steps:
1. Check deliverable for compliance to SMPs; – Section 4
2. If applicable, check deliverable for dimensional accuracy;
3. If applicable, check deliverable for spatial coordination; – Section 3.2
4. If applicable, check deliverable for sufficient attribute data;
5. Sign Checker box;
6. Check deliverable for completeness to satisfy the purpose of issue;
7. Update suitability code;
8. Update Revision code; and
9. Sign Approver box.
If non-conformity is identified during the process, the deliverable will be rejected.  Rejected deliverables will be amended by the information author and the approval process will be reset & repeated.
2.7	PIM Authorization Process
The purpose of this section is to confirm the authorisation process when receiving information.
It is assumed that the person responsible for the review of supplier information will undertake the following steps prior to authorization:
1. Confirm ability to assess deliverable against IT Constraints; - in response to EIR
2. Check deliverable against the Exchange of Information table; – in response to EIR
3. Review deliverable appropriateness against the Client Strategic Purposes; – in response to EIR
4. Update suitability code; and
5. Update Revision code.

Following the issue of information, authorization must be completed within five (5) working days to prevent programme delays.
3.0	Planning and Documenting
This section of the BEP covers the requirements of BS EN ISO 19650-2:2018 (Add section)
3.1	Project Implementation Plan
The purpose of this section is to confirm that the capability of the supply has been considered.
Due to the nature of this project, no other organisations have been appointed. 
As such no Project Implementation Plan has been produced.  Should any organisations be appointed, they will be assessed for their capability in response to the EIR and recorded on the PIP.
3.2	Agreed Processes for Collaboration & Information Modelling
The purpose of this section is to confirm how information will be exchanged and managed.
To satisfy the Client Strategic Purposes in response to the EIR, graphical and non-graphical information will be developed in accordance with the required attribute data outlined within section 4.9.  To the LOD & LOI specified with the Responsibility Matrix.
All deliverables will be developed progressively in accordance with the Master Information Delivery Plan (MIDP), utilising the software and formats outlined within section 5.1 & section 5.2 respectively.  
Through sequential development of information in accordance with the MIDP, and approved in compliance with section 2.6, a Clash Avoidance strategy will have been implemented.  Therefore, negating the need to Clash Detect.
The file naming, suitability, and revision convention outlined within BS EN ISO 19650-1:2018 will comply in response to the EIR, and the process and the data management process as shown within section 5.3 will be used.
Models and Deliverables will be placed onto a designated GoogleDrive folder to the viewing, access, and authorisation of information.  
To satisfy the data security requirements in response to the EIR, FF&E Graphical model and associated COBie data will be excluded from this exchange. In response to the EIR, training requirements have been identified to view, access, or authorise information based on the above collaboration processes.
3.3	Task Information Delivery Plan
The purpose of this section is to confirm the production of the Task Information Delivery Plans.
For ease of readability, the Task Information Delivery Plans (TIDP) have not been included within this document.  TIDPs are available on request.

3.4	Master Information Delivery Plan
The purpose of this section is to confirm the production of the Master Information Delivery Plan.
In response to the EIR, a Master Information Delivery Plan (MIDP) will be produced. 
The Development of the MIDP will be done through collaboration with other team members to ensure that the minimum amount of information required by them to produce their deliverables has been identified as ‘dependants’.
4.0	Standards, Methods, and Procedures
This section of the BEP covers the requirements of BS EN ISO 19650-2:2018 (Add section)
In response to the EIR, all identified standards have been included within section 4.0 of this BIM Execution Plan.  Any additional standards have been identified below
4.1	Volume Strategy
The purpose of this section is to define any specified geometric subdivision within the project.
Volume strategy has been defined within the file naming convention within section 4.3.
4.2	PIM Origin and Orientation
The purpose of this section is to define the common origin point for spatial coordination.
Due to the requirements to protect personal information in response to the EIR, OS grid references will not be used.  The project base point will be the external side boundary of the front garden wall as shown below, set to 0,0.  The project FFL will also be set to 0 with all other figures (including the project base point) to be set relative to this value.
[image: ]
Figure 1 - Project Base Point
CHANGE TO MY BASE POINT
Additional information will be used to populate the table below when available.
	Reference
	Position

	Ground Floor FFL
	0 (mm)

	Project Base Point 
	00000 N, 00000E (mm)

	Building Point 1
	192364.7 N, 265976 E (mm) 

	Building Point 2
	192364.7 N, 265976 E (mm) 


Table 11 - Origin and Orientation Values
[bookmark: _Hlk70536988]4.3	File Naming Convention
The purpose of this section is to confirm the file naming convention.
In response to the EIR, all deliverables will be named in accordance with BS EN ISO 19650-1:2018
Specified below are the permitted values for each field.
	Project Number
	Originator
	Volume
	Level
	File Type
	Role
	Classification
(optional)
	Number

	5010
	RJP
	xx
	GF
	DR
	A
	
	1001

	5010
	RJP
	xx
	GF
	DR
	S
	
	1001

	
	
	
	02
	
	
	
	

	
	
	
	ZZ
	
	
	
	


Table 12 - File Naming Values
[bookmark: _Hlk70536995]In addition to complying with BS EN ISO 19650-1:2018, section the number field will be further distinguished through the use of a Uniclass 2015 top-level code for the first two digits and one of the following series numbers for the third digit:
	Series
	Drawing

	xx1xx
	Plans

	xx2xx
	Elevations

	xx3xx
	Sections

	xx4xx
	Large-Scale Views

	xx5xx
	Details

	xx6xx
	Schedules & Diagrams


Table 13 - File Numbering Convention
[bookmark: _Hlk70537029]4.4 	Object Naming
The purpose of this section is to confirm the object naming convention.
In response to the EIR, all objects produced will be named in accordance with BS 8541-1.
Specified below are the permitted values for each field.
	Source
	Type
	SubType

	Author,
Manufacturer
	See Ifc[Type]
	See ...TypeEnum
See product name


Table 14 - Object Naming Values
[bookmark: _Hlk70537035]All objects types shall also be named following the following convention: [...TypeEnum]Type[Number] e.g DoorType01.
4.5	Agreed Construction Tolerances
The purpose of this section is to confirm the construction tolerances to be adhered to.
All produced information shall consider the tolerances outlined within ISO 5601.
4.6	Drawing Sheet Template
The purpose of this section is to specify and standard drawing sheet templates.
All drawings produced for this project shall utilise the ISO 5457 compliant drawing sheet provided.
All deliverables shall include the following ISO 7200 compliant title block.
[image: ]
PLACE MY TITLEBLOCK

[bookmark: _Hlk70537042]4.7	Annotations, Dimensions, Abbreviations, and Symbols
The purpose of this section is to define references for Annotations and Symbology.
All Annotations, dimensions, and symbols for this project will comply with BS 8541-2.
All Abbreviations used will be sourced from the BRE BIM Terminology Tool http://www.bre.co.uk/bimterminology.jsp.  Any abbreviations not sourced within this tool will be scheduled below:

	Term
	Acronym
	Definition

	
	
	


Table 16 - Project Terms

[bookmark: _Hlk70537049]4.8	Attribute Data
The purpose of this section is to define the attribute data to be exchanged.
In response to the EIR, all Employer specified attribute data has been identified and shall be delivered where appropriate.  In addition, in response to the EIR, the expected attribute data within BS 1192-4 shall also be delivered where appropriate.
Only a single classification code shall be included on each object which describes its primary function.  Classification shall be included in the Attribute ClassificationRefForObjects.
When exchanging project information the Revision and Status code out convention outlined in the diagram below shall be applied as attribute data to all files.  D codes shall be exclusively for unapproved information exchanged to aid in at-risk preparatory work.  Information with a D code status shall not be referenced to generate any deliverables.
[image: ]
When inputting geometry information the following convention shall be complied with:
[image: ]



[bookmark: _Hlk70537057]5.0	IT Solutions
This section of the BEP covers the requirements of BS EN ISO 19650-2:2018 (Add section)
5.1	Software Versions
The purpose of this section is to confirm the software and version to be used throughout the project.
Only the software outlined in the table below will be used to generate project deliverables.
No software shall be upgraded beyond the versions specified below without consent of the individual undertaking the Project Information Management responsibilities outlined within Section 4.1.
	Company
	Purpose
	Software
	Version

	Autodesk
	2D Modelling
	AutoCAD
	2021

	Autodesk
	3D Modelling & Creating of Drawings
	Revit
	2021

	CodePlex
	Federation & IFC Export 
	xBIM
	2.4.1.29

	
	
	
	


Table 17 - Project Software
[bookmark: _Hlk70537063]5.2	Exchange Formats
[bookmark: _Hlk70537069]The purpose of this section is to define the exchange formats to be used throughout the project.
The following exchange formats will be used throughout the project.
	Export Software
	Format
	Version

	AutoCAD
	.dwg
	2021

	Revit
	.rvt
	2021

	Revit
	.ifc
	2021, 2x3

	xBIM
	.xls
	COBie-UK 2021

	Revit
	.pdf
	-

	
	
	



5.3	Process and Data Management Systems 
The purpose of this section is to confirm the Data Management Systems utilised.
No Data Management System will be utilised on this project
Data will be managed and transferred in line with the following diagram: 
[image: ]
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12.2 The work in progress state

The work in progress state is used for information while it is being developed by its task team. An
information container in this state should not be visible or accessible to any other task team. This is
particularly important if the CDE solution is implemented through a shared system, for example a
shared server or web-portal.
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information delivery cycle specifically recognizes the existence of decision points within delivery
teams based on their own production of information.

PAS 1192-2:2013 and BS EN ISO 19650-1 information delivery cycle diagrams
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provided by Autodesk BIM 360 (c.2016) unless referenced otherwise. The key elements of
BIM Level 2 are:

Understand and follow the BIM protocol
Create a Level 2-ready project plan
Collaborate and Co-ordinate

Share data securely DELIVERY EXECUTION
Speak the same language Master Information BIM Execution Plan
Use COBie in your project Delivery Man (8EP)

Pass on the baton
Plan for a smooth handover

Understand and Follow the BIM Protocol L Project information Model (PIM)

‘Asset Information Model (AIM) |
| t

The BIM protocol is a legal addendurm that is outlined in every government project contract
which outlines the BIM requirements for the project. If someone wants to work on a
project, they need to understand and comply with all the requirements. According to
McPartland (2017), the “protocol puts in place specific obligations, liabilties and associated
limitations on the use of those models”.

Information Model

Maintain, Refurbish. End of i o

Create a Level 2-Ready Project Plan

The start of the project plan for BIM level 2 is done by responding to the Employer's !
Information Requirements (EIR). The EIR is the information that that will be required by the |

<> Q> <@ Q> Q> Q>
)l() OO0 Ol() C)l() (SN rerr—

employer from their own internal team and from suppliers to develop the project and for information exchanges |
the operation of the completed built asset. To respond to the EIR, a BIM Execution (BEP), 0 40} (o) @ @ jand employers decsion.

Master Information Delivery Plan (MIDP), and a Task Information Delivery Pan (TIDP) must
be prepared. Information on the MIDP and TIDP can be found in the appended BEP.

Collaborate and Co-ordinate

During the project’s life, team members will need to store, manage and exchange complex
information, to do this you'll have to use a CDE or Common Data Environment. A CDE is @
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Status & Revision Convention

Revision \ evision | \
- == n

Unapproved Approved
Unapproved Status Codes Approved Status Codes
S0, Work In Progress S1, Suitable for Coordination
D1, Suitable for Costing S2, Suitable for Information
D2, Suitable for Tender S3, Suitable for Review & Comment
D3, Suitable for Contractor Design S4, Suitable for Approval
D4, Suitable for Manufacture/Procurement S5, not used

S6, Suitable for PIM Authorization
S7, Suitable for AIM Authorization

Authorization

Authorized

Authorized Status Codes
An, Approved at Stage n
Bn, Approved with comments at Stage n*

CR, As Constructed Record

* While Published Bn status codes are not approved by the task team, so are given an unapproved status code
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Nominal Directions

Width = X-Axis (across the front)
Depth = Y-Axis (across the side)
Height = Z-Axis (up to the top)

Relative Directions

Length = Perpendicular to Profile.

Thickness = Distance between two
parallel distances.
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