R1#show run
Building configuration...


Current configuration : 1246 bytes
!
version 12.4
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
logging message-counter syslog
enable secret 5 $1$ivVU$NaRfGCv3VZqv3ziFu7.dL0
enable password 7 072A2F4D4C051C56370118
!
no aaa new-model
!
dot11 syslog
ip source-route
!
!
ip cef
!
!
no ip domain lookup
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
voice-card 0
!
!
!
!
!
archive
 log config
  hidekeys
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 172.16.2.1 255.255.255.192
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 ip address 172.16.2.65 255.255.255.240
 duplex auto
 speed auto
!
interface Serial0/0/0
 no ip address
 shutdown
 no fair-queue
 clock rate 2000000
!
interface Serial0/0/1
 no ip address
 shutdown
 clock rate 2000000
!
ip forward-protocol nd
no ip http server
no ip http secure-server
!
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
!
!
!
banner motd ^C Unauthorized access is strictly prohibited^C
!
line con 0
 password 7 05080F1C2243
 login
line aux 0
line vty 0 4
 password 7 0822455D0A16
 login
line vty 5 15
 password 7 0822455D0A16
 login
!
scheduler allocate 20000 1000
end
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