SCENIC PAINTING PRODUCTS
Paint Products: 
      Trade emulsion paints:
      BRANDS: Leyland, Johnstones, Valspar, Dulux
· Water-based paint with vinyl binder

· Paint dries to a fairly tough and moderately elastic film that remains 
      water-resistant. Interior use only!
· Low VOC (Volatile Organic Compound)
· Available in ready mixed and tinted colours in a range of finishes
Traditional dry scenic colours:
BRANDS: Haussmann, Flints
· Dry powder form of pigment

· Powder is mixed with a binder and water or dispersant!
· Available in various scenic colours, fluorescent and pearl powders
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Rosco Supersaturated paints:

· A concentrated acrylic paint designed to be diluted with water!

· A matt, non reflective paint for interior and exterior use
· Can be used on most surfaces including canvas, wood, plaster, various plastics and metal
· Available in a range of earth and dye colours including velour black
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Rosco Off Broadway paints:

· A matt vinyl acrylic paint designed to be used directly from the pot!
· Can be used on most surfaces including canvas, wood, plaster, various plastics and metal
· Available in a range of earth and dye colours including black

      Bristol/Rosco metallic paints:

· Vinyl acrylic paint designed to be used directly from the pot!
· Can be used on most surfaces including canvas, wood, plaster, various plastics and metal 
· Available in various metallic pigments including bronze, silver and gold
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Bristol/Rosco fluorescent paints:

· Vivid vinyl acrylic paint that is fluorescent under ultraviolet or black light

· Can be used on most surfaces including canvas, wood, plaster, various plastics and metal
      Spray paints:

       BRANDS: Plasti-kote, Krylon, Valspar
· Oil-based paint in pressurized can
· Available in a variety of primers, colours and finishes including metallic, glitter, fluorescent & textural products
· Commonly used for priming or spray-painting metallic objects such as lampposts or metal railings etc….
· Spray paints work well through a stencil
· Very High VOC and Extremely Flammable!  
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Bases and Priming Products:
Rosco white base:

· A white acrylic emulsion with titanium dioxide filler

· For use when priming new canvas or to prime old paint surfaces

· Must be diluted according to paint surface. New canvas dilute in ratio 2:1 water to base!

Rosco neutral base:
· An acrylic binder with no pigment

· For use when paint has been diluted with water, to increase adhesion!
      Flints multi-purpose primer:

· A low odour and non-flammable water-based primer suitable for painting wood, steel and plastics
· Good adhesion and provides a completely opaque covering!
· Available in black and white
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Rosco tough prime:

· A water-based primer with special adhesion properties which allows it to bond onto PVC pipe, aluminium and plastics, as well as muslin, wood and foam

· Dries to a tough, durable coating that can be over painted

· Suitable for interior and exterior use!

· Available in black and white
Covent garden prime:

•
Designed for the Royal Opera House for priming vacuum-formed plastics

•
It is water-based, can be tinted and is ideal for difficult surfaces such as dance 
            floor, PVC, clear plastics and rubber flooring 

•
Covent garden primer is formulated to be a first coat prior to conventional 
      painting although adding 20% to your scenic paint will normally make it stick 
      to dance floor materials
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      PVA:
BRANDS: Evo-stik, Polyten, Unibond, No Nonsense
· Adhesive for wood, paper and card

· Used as a binder or size 

Copydex/Flints…dex:

· Latex solvent free adhesive
· Used for bonding canvas, polystyrene, cork, plastic and non-porous surfaces
Glazes, Varnish, Wood Stain/Dyes:

Acrylic glaze:
BRANDS: Flints, Rosco, Bristol

· Water-based surface treatment applied to paint finishes, hard scenery etc…
· Used directly or diluted 1:1 with water

· Matt, Gloss, Satin finish

· Can be mixed with scenic paints to increase the binder strength & appearance!
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Rosco premiere clear:

· Advanced water-bourne polyurethane coating suitable for sealing and protecting paint finishes, hard scenery and floors even in high traffic areas
· Matt, Gloss, Satin finish

· Virtually odourless and can be tinted with water-based products!
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Crackle glaze:
BRANDS: Mylands, Polyvine
· Used for the effective reproduction of old cracked layers of paint

· A base coat of emulsion paint is applied and allowed to dry. Then the crackle glaze is applied. When the glaze is either tacky or completely dry, the topcoat of emulsion is then applied. The cracks will appear in the topcoat revealing the base colour!
Wood Stains/Dyes:
BRANDS: Hannants, Ronseal, Rustins

· A finish suitable for penetrating hard and soft wood surfaces that is coloured with pigment, dye or a mixture of both
· Available in various wood finishes including oak, pine, mahogany and walnut
· Water and Oiled based products available!

· Interior and Exterior grade
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Varnish:
BRANDS: Ronseal, Polyvine, PPG 
· A transparent, hard protective finish for wood surfaces and other materials
· Typically gives a gloss finish but satin or semi-gloss sheens are available
· Water and Oiled based products!
· Interior and Exterior grade
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White spirit:

· Thinning solution for oils. Used to clean oil-based paint products from painting tools.

Clean spirit:
· A water-based alternative to white spirit, turpentine substitute and paint brush cleaner. Used to clean both water and oil-based paint products from painting tools.         
Textures:

     Artex textured finish:

· Powder mixed with water

· Non-toxic and non hazardous
· Nonflexible finish that can crack easily!
· Interior use! 

· Can be overpainted. Available in white

Idenden Brushcote & Spraycote and Flintex:

· A durable, flexible & flame-retardant texture coating that will not crack or flake!

· Can be easily applied with a brush, roller or trowel directly to timber, canvas, hessian, vacuum form plastics and polystyrene 

· Idenden Spraycote a thinner product can be used in a texture gun to create textured effects
· Interior and Exterior use

· Both can be tinted or overpainted. Idenden is available in white, grey & black. Flintex available in white only!
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Traditional Effects:
PVC glitter & Rosco glitter:

· Brilliant effects under stage lighting! 

· Available in a range of colours, metallic, fluorescent and holographic glitters
· Can be fixed by sprinkling directly onto Rosco acrylic glaze
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      Mica flakes:

· Interesting sparkling decorative finish

· Available in a range of colours including black, silver and gold

· Can be fixed by sprinkling onto wet PVA adhesive or Rosco acrylic glaze
      Fuller’s earth:

· Beige coloured powder used by set dressers for ageing and dusting down scenery
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      Iron powder:

· Fine iron powder will rust quickly with water and is an excellent realistic rust effect 
· For best results apply a coat of acrylic glaze, while the glaze is still wet sprinkle liberal quantities of iron powder into the glaze and spray with vinegar
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NOTE: 

•
SAFETY DATA SHEETS must be made available for all paints, adhesives, glazes etc… products manufactured & sold. Here’s an example of one for Rosco’s Tough Prime so you can see what safety information & guidance these sheets provide.

https://us.rosco.com/sites/default/files/content/resource/2018-08/TP-BLACK-EN-6055.pdf
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