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	TOOLS TO BE USED AND MAXIMUM PERMITTED USAGE
These are the tools that will be used to accomplish the task. If additional tools are used, must also be assessed to give a total daily exposure time.

	Make/Model
	Vibration Magnitude
(M/S)
	Time to EAV
(h/min)
	Time to ELV (hrs/mins)
	Points per 15mins
	Points per 1 hour
	Rating
	Noise dBA

	
Makita DTD 152 – 18v Impact Driver
	
10.5
	
27 mins
	
1hr 49mins
	
55.25
	
221
	
HIGH
	
93

	
Makita DSS 610 – 18v 165mm Circular Saw
	
2.5
	
8 hrs
	
>24 hrs
	
3.25
	
13
	
LOW
	
91

	
Makita DGA 454 – 18v 115mm Angle Grinder
	
8.5
	
42 mins
	
2hrs 46mins
	
36.25
	
145
	
MED
	
73

	
Makita DHR 202 – 18v Rotary SDS Hammer Drill
	
Drilling 3

Hammer drilling 14.5
	
5hrs 33mins

14 mins 
	
22hrs 13mins

57mins

	
4.5

105.25
	
18

421

	
LOW

HIGH
	

87

	
Makita DCS 550 – 18v Metal Saw
	
3
	
5hrs 33 mins
	
22hrs 13mins
	
4.5
	
18
	
LOW
	
101

	
Makita DJR186Z – Recipro Saw

	
12.6
	
20 mins
	
1hr 15mins
	
75
	
300
	
HIGH
	
99

	
Makita DJV180Z
JIGSAW


	
Chipboard – 8

Metal – 3  
	
43 mins

5hrs 33 mins
	
3hrs 7 mins

22hrs 12 mins
	
32

4.5
	
128

18
	
MED

LOW
	

78

	
Stihl TS 410

	
6.8
	
1hr 5mins
	
4hrs 20mins
	
23
	
92
	
HIGH
	
114

	
Hilti WSR Reciprocating saw

	
18
	
12 mins
	
48 mins
	
162
	
648
	
HIGH
	
86

	
Hilti SID Impact Driver

	
11
	
25 mins
	
1hr 40 mins
	
60.5
	
242
	
HIGH
	
86

	
Hilti SIW impact wrench

	
11
	
25 mins
	
1hr 40mins
	
60.5
	
242
	
HIGH
	
86

	
Hilti TE4 Rotary Hammer Drill

	
11
	
25 mins
	
1hr 40 mins
	
60.5
	
242
	
HIGH
	
86

	
Hilti AG 125 Angle Grinder

	
5.2
	
1hr 41 mins
	
7hrs 24 mins
	
13.5
	
54
	
LOW
	
84

	
Hilti SCW Circular Saw

	
2.5
	
8 hrs
	
 > 24 hrs
	
3.25
	
13
	
LOW
	
91
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