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[bookmark: _Toc218433527]3.1 On-site evidence
On-site evidence was gathered to verify that the survey was carried out at the Dylan Thomas Centre. The 3D laser scanning evidence was gathered as shown in Appendix 1, for measurements done with tape measures and a handheld laser scanner. Evidence photos will be provided under Appendix 2. 
The visual confirmation that the survey was completed is evident, as the surveyor has annotated both figures: one by hand and the other digitally produced. These annotations support the validity of the survey by demonstrating that the measurements were taken on-site. 

3.2 Survey Execution Summary 
The survey execution followed the survey plan. With multiple groups following the building plan to ensure comprehensive coverage of the surveyed floor, it allowed for multiple scans to be taken and all measurements to be gathered, resulting in consistent data collection. However, the scanner's location is not always consistent, which creates a potential issue affecting data quality. 
[bookmark: _Toc218433529]
3.3 Problems Encountered
As previously stated, the location of the scanner is a variable because it is not possible for the scanner to be perfectly placed in a precise location each time. This introduced minor variability in the scan geometry; however, the impact on the data was limited, as the scans were compared and set together to create an average of each measurement and a completed layout for the survey. 






4. Appendices 

Appendix 1 – The full scan
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Appendix 2 – Manual Drawings 
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