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1)
a)	The Harvard architecture uses a 16 pic series microcontroller

b)	INCFSZ- incremented ‘f’ skips if 0
	NOP – No Operation
	GOTO – Go to address
	CLRW -	Clear ‘w’
	CLRWDT – Clear watchdog timer

c)	Interrupt are internal/external signals that suspend the main routine being done/executed. 
