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1A: A	
1B: B
1C: A

Load Supply Current = 26.5mA
2B: C
Connecting a short across the load, the supply voltage drops down to a low value, approx. 1v p-p
2C:  D
2D: B
2E: B
2F: A
Knowledge:
1: A
2: D
3: B
4: A
5: C
6: B
Fault Included: B
The connection between 4.3 and 7.1 is shorted. Circuit 7 (Power Factor Correction) is completely shorted.


