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Packet Tracer Log File.
Tue Nov 14 10:27:43 2023   Router2   Router>en
Tue Nov 14 10:27:53 2023   Router2   Router#conf t
Tue Nov 14 10:28:46 2023   Router3   Router>en
Tue Nov 14 10:28:48 2023   Router3   Router#config t
Tue Nov 14 10:28:52 2023   Router3   Router(config)#hostname
Tue Nov 14 10:29:03 2023   Router3   Router(config)#hostname RA
Tue Nov 14 10:34:15 2023   Router5   Router>en
Tue Nov 14 10:34:17 2023   Router5   Router#config t
Tue Nov 14 10:34:22 2023   Router5   Router(config)#hostname RC
Tue Nov 14 10:39:08 2023   Router8   Router>en
Tue Nov 14 10:39:11 2023   Router8   Router#conf t
Tue Nov 14 10:39:17 2023   Router8   Router(config)#hostname RB
Tue Nov 14 10:51:35 2023   Router13   Router>en
Tue Nov 14 10:51:37 2023   Router13   Router#conf t
Tue Nov 14 10:51:50 2023   Router13   Router(config)#hostname RA
Tue Nov 14 11:02:36 2023   Router14   Router>en
Tue Nov 14 11:02:38 2023   Router14   Router#conf t
Tue Nov 14 11:02:50 2023   Router14   Router(config)#hostname RB
Tue Nov 14 11:03:05 2023   Router14   RB(config)#interface Se0/1/0
Tue Nov 14 11:15:32 2023   RA   RA>IP ?
Tue Nov 14 11:15:35 2023   RA   RA>ip?
Tue Nov 14 11:15:45 2023   RA   RA>en
Tue Nov 14 11:15:50 2023   RA   RA#config t
Tue Nov 14 11:15:52 2023   RA   RA(config)#ip?
Tue Nov 14 11:15:54 2023   RA   RA(config)#ip ?
Tue Nov 14 11:16:43 2023   RA   RA(config)#interface Se3/0
Tue Nov 14 11:17:23 2023   RA   RA#config
Tue Nov 14 11:17:34 2023   RA   RA(config)#interface Se3/0
Tue Nov 14 11:18:33 2023   RA   RA(config-if)#ip address 10.0.23.0 255.255.255.252
Tue Nov 14 11:18:52 2023   RA   RA(config-if)#ip address 10.0.23.0 ?
Tue Nov 14 11:19:09 2023   RA   RA(config-if)#ip address 10.0.23.0 255.255.255.252 ?
Tue Nov 14 11:19:11 2023   RA   RA(config-if)#ip address 10.0.23.0 255.255.255.252 
Tue Nov 14 11:20:05 2023   RA   RA(config-if)#exit
Tue Nov 14 11:20:17 2023   RA   RA(config)#interface Se2/0
Tue Nov 14 11:20:39 2023   RA   RA(config-if)#ip address 10.0.12.0 255.255.255.252
Tue Nov 14 11:23:08 2023   RA   RA(config-if)#ip address 10.0.12.1 255.255.255.252
Tue Nov 14 11:23:17 2023   RA   RA(config-if)#do wr
Tue Nov 14 11:23:53 2023   RA   RA(config-if)#exit
Tue Nov 14 11:24:03 2023   RA   RA(config)#interface Fa/0/0
Tue Nov 14 11:24:08 2023   RA   RA(config)#interface Fa0/0
Tue Nov 14 11:25:04 2023   RA   RA(config-if)#ip address 10.0.12.1 255.255.255.252 ?
Tue Nov 14 11:25:05 2023   RA   RA(config-if)#ip address 10.0.12.1 255.255.255.252 
Tue Nov 14 11:25:09 2023   RA   RA(config-if)#do wr
Tue Nov 14 11:27:18 2023   RB   RB>en
Tue Nov 14 11:27:20 2023   RB   RB#conf t
Tue Nov 14 11:27:41 2023   RB   RB(config)#interface Fa0/0
Tue Nov 14 11:28:00 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.252 ?
Tue Nov 14 11:28:00 2023   RB   RB(config-if)#ip address 10.0.12.2 255.255.255.252 
Tue Nov 14 11:28:05 2023   RB   RB(config-if)#do wr
Tue Nov 14 11:28:28 2023   RC   Router>en
Tue Nov 14 11:28:34 2023   RC   Router#conf t
Tue Nov 14 11:28:40 2023   RC   Router(config)#hostname RC
Tue Nov 14 11:28:54 2023   RC   RC(config)#interface Fa0/0
Tue Nov 14 11:29:16 2023   RC   RC(config-if)#ip address 10.0.23.2 255.255.255.252
Tue Nov 14 11:29:18 2023   RC   RC(config-if)#do wr
Tue Nov 14 11:29:38 2023   SM1   Switch>en
Tue Nov 14 11:29:40 2023   SM1   Switch#conf 
Tue Nov 14 11:29:47 2023   SM1   Switch(config)#hostname SM1
Tue Nov 14 11:29:52 2023   SM1   SM1(config)#vlan 1
Tue Nov 14 11:29:57 2023   SM1   SM1(config-vlan)#ip?
Tue Nov 14 11:31:04 2023   SB   Switch>sn
Tue Nov 14 11:31:31 2023   SB   Switch>en
Tue Nov 14 11:31:33 2023   SB   Switch#conf t
Tue Nov 14 11:31:41 2023   SB   Switch(config)#hostname SB
Tue Nov 14 11:31:56 2023   SB   SB(config)#interface Fa0/11
Tue Nov 14 11:39:41 2023   SB   SB(config-if)#vlan 20
Tue Nov 14 11:39:50 2023   SB   SB(config-vlan)#name 
Tue Nov 14 11:39:53 2023   SB   SB(config-vlan)#name ?
Tue Nov 14 11:40:02 2023   SB   SB(config-vlan)#vlan name ?
Tue Nov 14 11:40:05 2023   SB   SB(config-vlan)#vlan name ?
Tue Nov 14 11:40:09 2023   SB   SB(config-vlan)#name ?
Tue Nov 14 11:40:25 2023   SB   SB(config-vlan)#name Lecurer
Tue Nov 14 11:40:32 2023   SB   SB(config-vlan)#name LECTURER
Tue Nov 14 11:40:45 2023   SB   SB(config-vlan)#ip?
Tue Nov 14 11:43:56 2023   SA   Switch>en
Tue Nov 14 11:44:03 2023   SA   Switch#hostname 
Tue Nov 14 11:44:20 2023   SA   Switch#hostname SA
Tue Nov 14 11:44:26 2023   SA   Switch#config t
Tue Nov 14 11:44:30 2023   SA   Switch(config)#hostname SA
Tue Nov 14 11:44:45 2023   SA   SA(config)#vlan 10
Tue Nov 14 11:44:47 2023   SA   SA(config-vlan)#exit
Tue Nov 14 11:44:56 2023   SA   SA(config)#interface  vlan 10
Tue Nov 14 11:45:09 2023   SA   SA(config-if)#ip ?
Tue Nov 14 11:45:32 2023   SA   SA(config-if)#ip address 192.168.1.2 255.255.255.0?
Tue Nov 14 11:45:34 2023   SA   SA(config-if)#ip address 192.168.1.2 255.255.255.0 ?
Tue Nov 14 11:45:35 2023   SA   SA(config-if)#ip address 192.168.1.2 255.255.255.0 
Tue Nov 14 11:45:37 2023   SA   SA(config-if)#do wr
Tue Nov 14 11:45:53 2023   SA   SA(config-if)#exit
Tue Nov 14 11:46:02 2023   SA   SA(config)#vlan 10 
Tue Nov 14 11:46:11 2023   SA   SA(config-vlan)#name STUDENT
Tue Nov 14 11:48:07 2023   SB   SB(config-vlan)#exit
Tue Nov 14 11:48:12 2023   SB   SB(config)#interface Vlan 20
Tue Nov 14 11:48:17 2023   SB   SB(config-if)#name ?
Tue Nov 14 11:48:34 2023   SB   SB(config-if)#ip address 192.168.2.2 255.255.255.0 ?
Tue Nov 14 11:48:34 2023   SB   SB(config-if)#ip address 192.168.2.2 255.255.255.0 
Tue Nov 14 11:48:36 2023   SB   SB(config-if)#do wr
Tue Nov 14 11:48:40 2023   SB   SB(config-if)#exit
Tue Nov 14 11:48:51 2023   SB   SB(config)#vlan 20
Tue Nov 14 11:48:53 2023   SB   SB(config-vlan)#name ?
Tue Nov 14 11:49:03 2023   SB   SB(config-vlan)#exit
Tue Nov 14 11:49:57 2023   RA   RA>en
Tue Nov 14 11:49:58 2023   RA   RA#conf ty
Tue Nov 14 11:50:00 2023   RA   RA#conf t
Tue Nov 14 11:50:03 2023   RA   RA(config)#no ip domain-lookup
Tue Nov 14 11:50:06 2023   RA   RA(config)#do wr
Tue Nov 14 11:50:15 2023   RB   RB>en
Tue Nov 14 11:50:17 2023   RB   RB#conf t
Tue Nov 14 11:50:21 2023   RB   RB(config)#no ip domain-lookup
Tue Nov 14 11:50:24 2023   RB   RB(config)#exit
Tue Nov 14 11:50:36 2023   RC   RC>en
Tue Nov 14 11:50:38 2023   RC   RC#conf t
Tue Nov 14 11:50:52 2023   RC   RC(config)#no ip domain-lookup
Tue Nov 14 11:51:02 2023   RC   RC(config)#no ip domain-lookup
Tue Nov 14 11:52:01 2023   SM1   SM1>en
Tue Nov 14 11:52:07 2023   SM1   SM1#conf t
Tue Nov 14 11:52:14 2023   SM1   SM1(config)#vlan 1
Tue Nov 14 11:52:21 2023   SM1   SM1(config-vlan)#exit
Tue Nov 14 11:52:27 2023   SM1   SM1(config)#interface  vlan1
Tue Nov 14 11:52:52 2023   SM1   SM1(config-if)#ip address 172.16.0.12 ?
Tue Nov 14 11:53:06 2023   SM1   SM1(config-if)#ip address 172.16.0.12  255.255.255.0 ?
Tue Nov 14 11:53:07 2023   SM1   SM1(config-if)#ip address 172.16.0.12  255.255.255.0 
Tue Nov 14 11:53:10 2023   SM1   SM1(config-if)#do wr
Tue Nov 14 11:53:34 2023   SM1   SM1(config-if)#exit
Tue Nov 14 11:53:50 2023   SM2   Switch>en
Tue Nov 14 11:53:51 2023   SM2   Switch#conf t
Tue Nov 14 11:53:57 2023   SM2   Switch(config)#hostname SM2
Tue Nov 14 11:54:09 2023   SM2   SM2(config)#interface vlan1
Tue Nov 14 11:54:46 2023   SM2   SM2(config-if)#ip address 172.16.0.12 255.255.255.0
Tue Nov 14 11:54:48 2023   SM2   SM2(config-if)#do wr
Tue Nov 14 11:56:17 2023   SB   SB(config)#switchport mode access
Tue Nov 14 11:56:42 2023   SB   SB(config)#interface vlan20
Tue Nov 14 11:56:46 2023   SB   SB(config-if)#switchport mode access
Tue Nov 14 11:56:54 2023   SB   SB(config-if)#switchport ?
Tue Nov 14 11:57:22 2023   SB   SB(config-if)#switchport access vlan20
Tue Nov 14 11:57:24 2023   SB   SB(config-if)#exit
Tue Nov 14 11:57:29 2023   SB   SB(config)#switchport access vlan20
Tue Nov 14 11:57:35 2023   SB   SB(config)#switchport access ?
Tue Nov 14 11:57:59 2023   SA   SA>en
Tue Nov 14 11:58:00 2023   SA   SA#conf t
Tue Nov 14 11:58:04 2023   SA   SA(config)#spanning-tree mode rapid-pvst
Tue Nov 14 11:58:07 2023   SA   SA(config)#spanning-tree mode rapid-pvst ?
Tue Nov 14 11:58:08 2023   SA   SA(config)#spanning-tree mode rapid-pvst 
Tue Nov 14 11:58:10 2023   SA   SA(config)#do wr
Tue Nov 14 11:58:20 2023   SB   SB(config)#spanning-tree mode rapid-pvst
Tue Nov 14 11:58:23 2023   SB   SB(config)#do wer
Tue Nov 14 11:58:28 2023   SB   SB(config)#do wr
Tue Nov 14 11:59:03 2023   RB   RB#conf t
Tue Nov 14 11:59:06 2023   RB   RB(config)#standby 1 ip 172.16.0.3
Tue Nov 14 11:59:11 2023   RB   RB(config)#standby 1 ip ?
Tue Nov 14 11:59:14 2023   RB   RB(config)#standby?
Tue Nov 14 11:59:48 2023   RB   RB(config)#standby ?
Tue Nov 14 12:02:40 2023   RA   RA>en
Tue Nov 14 12:02:42 2023   RA   RA#conf t
Tue Nov 14 12:02:47 2023   RA   RA(config)#router eigrp 12
Tue Nov 14 12:03:03 2023   RA   RA(config-router)#network
Tue Nov 14 12:03:11 2023   RA   RA(config-router)#network?
Tue Nov 14 12:03:13 2023   RA   RA(config-router)#network
Tue Nov 14 12:03:19 2023   RA   RA(config-router)#network
Tue Nov 14 12:03:35 2023   RA   RA(config-router)#no auto-summary
Tue Nov 14 12:03:44 2023   RA   RA(config-router)#eigrp router-id 1.1.1.1
Tue Nov 14 12:03:54 2023   RA   RA(config-router)#passive-interface default
Tue Nov 14 12:04:26 2023   RB   RB(config)#router eigrp 12
Tue Nov 14 12:04:31 2023   RB   RB(config-router)#network
Tue Nov 14 12:04:39 2023   RB   RB(config-router)#no auto-summary
Tue Nov 14 12:05:22 2023   RB   RB(config-router)#eigrp router-id 2.2.2.2
Tue Nov 14 12:05:41 2023   RB   RB(config-router)#passive-interface default
Tue Nov 14 12:05:56 2023   RB   RB(config-router)#exit
Tue Nov 14 12:06:06 2023   RC   RC>en
Tue Nov 14 12:06:09 2023   RC   RC#conf t
Tue Nov 14 12:06:53 2023   RC   RC(config)#router eigrp 12
Tue Nov 14 12:08:02 2023   RC   RC(config-router)#network 10.0.23.2
Tue Nov 14 12:08:21 2023   RC   RC(config-router)#no auto-summary
Tue Nov 14 12:08:31 2023   RC   RC(config-router)#eigrp router-id 3.3.3.3
Tue Nov 14 12:08:44 2023   RC   RC(config-router)#passive-interface default
Tue Nov 14 12:09:03 2023   RB   RB#en
Tue Nov 14 12:09:04 2023   RB   RB#conf t
Tue Nov 14 12:09:06 2023   RB   RB(config)#router eigrp 12
Tue Nov 14 12:09:23 2023   RB   RB(config-router)#network 10.0.12.2
Tue Nov 14 12:09:40 2023   RB   RB(config-router)#no auto-summary
Tue Nov 14 12:09:46 2023   RB   RB(config-router)#passive-interface default 
Tue Nov 14 12:09:48 2023   RB   RB(config-router)#do wr
Tue Nov 14 12:09:50 2023   RB   RB(config-router)#exit
Tue Nov 14 12:10:36 2023   RA   RA(config-router)#network 192.168.1.1 
Tue Nov 14 12:10:43 2023   RA   RA(config-router)#no auto-summary
Tue Nov 14 12:10:46 2023   RA   RA(config-router)#passive-interface default
Tue Nov 14 12:10:47 2023   RA   RA(config-router)#do wr
Tue Nov 14 12:10:51 2023   RA   RA(config-router)#exit
Tue Nov 14 12:12:41 2023   RB   RB(config)#exit
Tue Nov 14 12:12:46 2023   RB   RB#conf t
Tue Nov 14 12:15:55 2023   RB   RB(config)#interface Fa0/0
Tue Nov 14 12:16:06 2023   RB   RB(config-if)#standby 1 ip 172.16.0.3 ?
Tue Nov 14 12:16:07 2023   RB   RB(config-if)#standby 1 ip 172.16.0.3 
Tue Nov 14 12:16:37 2023   RB   RB(config-if)#standby 1 priority 110
Tue Nov 14 12:16:45 2023   RB   RB(config-if)#standby 1 preempt
Tue Nov 14 12:18:19 2023   RC   RC(config-router)#exit
Tue Nov 14 12:21:18 2023   RC   RC(config)#int Fa0/0
Tue Nov 14 12:21:42 2023   RC   RC(config-if)#standby 1 ip 172.16.0.3
Tue Nov 14 12:23:35 2023   RC   RC(config-if)#interface Fa0/0
Tue Nov 14 12:24:01 2023   RC   RC(config-if)#ip address 172.16.0.2 255.255.255.0
Tue Nov 14 12:24:16 2023   RC   RC(config-if)#standby 1 ip 172.16.0.3
Tue Nov 14 12:25:26 2023   RB   RB(config-if)#ip address 172.16.0.2 255.255.255.0
Tue Nov 14 12:25:30 2023   RB   RB(config-if)#standby 1 ip 172.16.0.3 
Tue Nov 14 12:25:33 2023   RB   RB(config-if)#standby 1 preempt
Tue Nov 14 12:25:36 2023   RB   RB(config-if)#standby 1 priority 110
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