5. Estimates 
Bridge Works 
Footbridge = £4100 x 816(m2) = £3,345,600 
per m² of deck maximum span between piers or abutments; include for the works described to the bridge decks and abutments, but exclude any approach works 
Rate acquired from Spon’s chose to go with higher band of estimate due to the expensive material chosen in the design. 
Tilt & Vertical lift designs to be priced by specialist contractor at later date. 
Approach works 
Roadworks = £3700 x 15(m) = £55,500 
Tarmacadam or reinforced concrete roads, including all earthworks, drainage, lighting, signs, fencing and safety barriers 7.30m wide two-lane carriageway 
Tarmac Footpath = £100 x 50(m2) = £5000 
Tarmacadam paving two layers; limestone or igneous chipping finish paving on subbase; including excavation and type 1 subbase 
Granite Footpath = £180 x 20(m2) = £3600 
granite setts on 100mm thick concrete subbase; including excavation; pointing mortar joints 
Zebra crossing = £25,000(number) x 2 
Costs include road markings, beacons, lights, signs, advance danger Signs. 
 
TOTALS 
BRIDGE WORKS                                                     = £3,345,600 
APPROACH WORKS                                              = £114,100 
TOTAL (x WALES REGION FACTOR 0.86)          = £2,975,342 

