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Question - Please advise what software has been used to construct the flood model referred to in SC5, which we understand is to be used by the consultant for both flood risk and geomorphological modelling (SC6). Please advise the geographical extent and resolution of the model and the calibration that has been conducted.

Answer -  

[bookmark: _GoBack]The software used for the flood model - Tuflow (Build: 2013-12-AC-iSP-w64)

Geographical context /boundary set
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Resolution of the model - 2m grid

Calibration conducted - Not calibrated
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