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You need to complete the following tasks:  
1. Build a virtual network configuration
2. Install and Configure
a. Critical network services
b. Routing

Critical Details
Login: -: Username: Administrator, Password: Pa55w0rD!
System Configuration: -: Language: English US, Time Format: London UK
1. In SW Network, 
1.1. Install Routing and Remote access Service and modify firewall rules to allow ICMP Traffic.
1.2. Configure Site-to-Site VPN to LD Network. Set the connection type to “persistent connection”.
1.3. Create a forest named WSSIT.NSA
1.4. Create all appropriate A records for all servers on 10.1.0.0/24 and 10.2.0.1/24.
1.5. Create a reverse lookup zone creating PTR records for all servers.
2. In LD Network, 
2.1. Install Routing and Remote access Service and modify firewall rules to allow ICMP Traffic.
2.2. Configure Site-to-Site VPN to Swansea Network. Set the connection type to “persistent connection”.
2.3. Create a child domain named LD.WSSIT.NSA in WSSIT.NSA tree
2.4. Create user accounts for LD.WSSIT.NSA domain with all the parameters defined in the users_list.xlsx document. 
2.5. Mount second disk drive to C:\LondonFiles. 
2.6. Configure DHCP Services. The range is 10.2.0.10 – 10.2.0.20. Determine other DHCP options as per the infrastructure.
3. Sharing Disk Drive: 
3.1. To the earlier created C:\LondonFiles, set access permissions to allow users in the users_list.xlsx has full control permissions and other network users have only read access. 
3.2. Share the drive to both LD and SW network.
4. Configure IIS Server
4.1. Create https://web.ld.wssit.nsa website and enable windows internal authentication. All the LD users can be authenticated.
4.2. All authenticated users should be presented a text “Welcome to LD Website”.
5. Remote Desktop Services: 
5.1. Configure remote access for LD-DC from any other machines in the network. 
5.2. Make sure that the Remote Desktop Services login page should be accessed via https://rds.ld.wssit.nsa and necessary certificates are signed. 
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