In the VISUALIZER Module:
· Select VIEW ODB display options:
· [image: ]

In the SWEEP Tab:
Choose the rotation angle to sweep through and choose the number of segments for refinement. In thi exmaple I sweep through 360 degrees with a segment angle of 10 degrees:
[image: ]









This gives:
[image: ]

You can vary the parameters to give the display you desire
[bookmark: _GoBack]In the next example I choose to sweep through only 180 degrees and it is more informative:
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